*PADS-LOGIC-V9.0-CP936* 来自 PADS LOGIC VVX.2.7 的设计导出文件
*SCH*        GENERAL PARAMETERS OF THE SCHEMATIC DESIGN"

CUR SHEET    1              Current Active Sheet
USERGRID     2      50      Design and Label/Text grid settings
LINEWIDTH    10             Width items will be created with
CONNWIDTH    10             Width used to plot connections
BUSWIDTH     25             Width used to plot buses
BUSANGLE     25             Angle used when plotting buses
NNVISPWRGND  4              Pwr/Gnd netname visibility default flag
PCBFLAGS     1039           PCB Netlist and ECO options
PINNAMESIZE  97     10      Height and LineWidth used by pin names
TEXTSIZE     111    10      Height and LineWidth text will be created width
JOBTIME      0              Amount of time spent on this LOGIC design
DOTGRID      10             Space in thous/inch between graphic dots
BACKUPTIME   5              Number of minutes between database backups
TIEDOTSIZE   75             Diameter of tiedot point
REFNAMESIZE  100    10      Height and LineWidth used by part ref. names
PARTNAMESIZE 100    10      Height and LineWidth used by part type names
PINNOSIZE    97     10      Height and LineWidth used by pin numbers
NETNAMESIZE  100    10      Height and LineWidth used by net names
REAL WIDTH   36             Widths greater then this are displayed real size
SHEET SIZE   A4            
UNITS        0              Rules units type
JOBNAME      N32G030K6L7_STB_V1.0.sch
NTXCOL 11 9
HIRCOL 2
LINCOL 0
TXTCOL 0 31
CONCOL 9
BUSCOL 4
PTXCOL 0 31
COMCOL 4
NMCOL  1 31
PNMCOL 1 31
PINCOL 0 31
NETCOL 4 31
FBGCOL 1 31
OFFREFVIEW   0              Offsheet references visibility default flag
OFFREFNUM    0              Offsheet references per line
SHEETNUMSEP  []             Sheet Number separators
FONT MODE   System
DEFAULT FONT "Regular Tahoma"
BORDER NAME DRW_NATIONS_A4
FIELDCOL 1 0

*CAM* PLOTTER SETTINGS 
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

PLOT_SECTION	5.0
{
PLOT_DEFAULTS_PHOTO_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_MPOS_V1
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Current
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PEN_PLOTTER	NULL
{
DEFAULT_FILE_PREFIX	 Z32HUA_FNT_V0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 Y
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	Selected
DEFAULT_SHEET_LIST	NULL
{
SHEET_1	2
SHEET_2	4
SHEET_3	5
SHEET_4	6
SHEET_5	8
SHEET_6	1
SHEET_7	7
}
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_DEFAULTS_PRINTER	NULL
{
DEFAULT_FILE_PREFIX	 NZ3101_FNT_BCM_0
DEFAULT_SCALE	 1 1
DEFAULT_ORIENTATION	 0
DEFAULT_JUSTIFICATION	 SF
DEFAULT_OFFSETS	 0 0
DEFAULT_WINDOW_PLOT	 N
DEFAULT_PLOT_JOBNAME	 N
DEFAULT_PLOT_OLE	 N
DEFAULT_SHEET	All
DEFAULT_CONNECTIONS	1
DEFAULT_BUSSES	1
DEFAULT_LINES	1
DEFAULT_TEXT	1
DEFAULT_PARTS	1
DEFAULT_REFDES	1
DEFAULT_PARTTYPES	1
DEFAULT_PARTEXT	1
DEFAULT_PINNUMBERS	1
DEFAULT_PINNAMES	1
DEFAULT_NETNAMES	1
DEFAULT_HIERSYMS	1
}
PLOT_AUGMENT_ON_THE_FLY	Y
}

*MISC*      MISCELLANEOUS PARAMETERS
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	MILS
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	Top
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ASSOCIATED_SILK_SCREEN	Silkscreen Top
ASSOCIATED_PASTE_MASK	Paste Mask Top
ASSOCIATED_SOLDER_MASK	Solder Mask Top
ASSOCIATED_ASSEMBLY	Assembly Drawing Top
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	Bottom
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Layer_3
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	4
{
LAYER_NAME	Layer_4
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	10
COPPER_THICKNESS	1.35
DIELECTRIC	4.300000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	1.35
DIELECTRIC	3.300000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	Layer_21
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Layer_22
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Layer_23
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	Layer_24
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Layer_26
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	Layer_27
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	Layer_28
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Layer_29
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	Layer_30
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	31
{
LAYER_NAME	Layer_31
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	32
{
LAYER_NAME	Layer_32
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	33
{
LAYER_NAME	Layer_33
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	34
{
LAYER_NAME	Layer_34
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	35
{
LAYER_NAME	Layer_35
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	36
{
LAYER_NAME	Layer_36
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	37
{
LAYER_NAME	Layer_37
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	38
{
LAYER_NAME	Layer_38
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	39
{
LAYER_NAME	Layer_39
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	40
{
LAYER_NAME	Layer_40
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	41
{
LAYER_NAME	Layer_41
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	42
{
LAYER_NAME	Layer_42
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	43
{
LAYER_NAME	Layer_43
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	44
{
LAYER_NAME	Layer_44
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	45
{
LAYER_NAME	Layer_45
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	46
{
LAYER_NAME	Layer_46
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	47
{
LAYER_NAME	Layer_47
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	48
{
LAYER_NAME	Layer_48
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	49
{
LAYER_NAME	Layer_49
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	50
{
LAYER_NAME	Layer_50
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	51
{
LAYER_NAME	Layer_51
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	52
{
LAYER_NAME	Layer_52
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	53
{
LAYER_NAME	Layer_53
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	54
{
LAYER_NAME	Layer_54
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	55
{
LAYER_NAME	Layer_55
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	56
{
LAYER_NAME	Layer_56
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	57
{
LAYER_NAME	Layer_57
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	58
{
LAYER_NAME	Layer_58
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	59
{
LAYER_NAME	Layer_59
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	60
{
LAYER_NAME	Layer_60
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	61
{
LAYER_NAME	Layer_61
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	62
{
LAYER_NAME	Layer_62
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	63
{
LAYER_NAME	Layer_63
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	64
{
LAYER_NAME	Layer_64
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	65
{
LAYER_NAME	Layer_65
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	66
{
LAYER_NAME	Layer_66
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	67
{
LAYER_NAME	Layer_67
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	68
{
LAYER_NAME	Layer_68
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	69
{
LAYER_NAME	Layer_69
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	70
{
LAYER_NAME	Layer_70
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	71
{
LAYER_NAME	Layer_71
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	72
{
LAYER_NAME	Layer_72
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	73
{
LAYER_NAME	Layer_73
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	74
{
LAYER_NAME	Layer_74
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	75
{
LAYER_NAME	Layer_75
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	76
{
LAYER_NAME	Layer_76
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	77
{
LAYER_NAME	Layer_77
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	78
{
LAYER_NAME	Layer_78
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	79
{
LAYER_NAME	Layer_79
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	80
{
LAYER_NAME	Layer_80
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	81
{
LAYER_NAME	Layer_81
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	82
{
LAYER_NAME	Layer_82
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	83
{
LAYER_NAME	Layer_83
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	84
{
LAYER_NAME	Layer_84
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	85
{
LAYER_NAME	Layer_85
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	86
{
LAYER_NAME	Layer_86
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	87
{
LAYER_NAME	Layer_87
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	88
{
LAYER_NAME	Layer_88
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	89
{
LAYER_NAME	Layer_89
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	90
{
LAYER_NAME	Layer_90
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	91
{
LAYER_NAME	Layer_91
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	92
{
LAYER_NAME	Layer_92
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	93
{
LAYER_NAME	Layer_93
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	94
{
LAYER_NAME	Layer_94
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	95
{
LAYER_NAME	Layer_95
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	96
{
LAYER_NAME	Layer_96
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	97
{
LAYER_NAME	Layer_97
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	98
{
LAYER_NAME	Layer_98
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	99
{
LAYER_NAME	Layer_99
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	100
{
LAYER_NAME	Layer_100
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	101
{
LAYER_NAME	Layer_101
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	102
{
LAYER_NAME	Layer_102
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	103
{
LAYER_NAME	Layer_103
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	104
{
LAYER_NAME	Layer_104
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	105
{
LAYER_NAME	Layer_105
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	106
{
LAYER_NAME	Layer_106
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
ASSOCIATED_SILK_SCREEN	Layer_29
ASSOCIATED_PASTE_MASK	Layer_22
ASSOCIATED_SOLDER_MASK	Layer_28
ASSOCIATED_ASSEMBLY	Layer_30
COMPONENT	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	107
{
LAYER_NAME	Layer_107
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	108
{
LAYER_NAME	Layer_108
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	109
{
LAYER_NAME	Layer_109
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	110
{
LAYER_NAME	Layer_110
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	111
{
LAYER_NAME	Layer_111
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	112
{
LAYER_NAME	Layer_112
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	113
{
LAYER_NAME	Layer_113
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	114
{
LAYER_NAME	Layer_114
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	115
{
LAYER_NAME	Layer_115
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	116
{
LAYER_NAME	Layer_116
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	117
{
LAYER_NAME	Layer_117
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	118
{
LAYER_NAME	Layer_118
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	119
{
LAYER_NAME	Layer_119
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	120
{
LAYER_NAME	Layer_120
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	121
{
LAYER_NAME	Solder Mask Top
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	122
{
LAYER_NAME	Paste Mask Bottom
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	123
{
LAYER_NAME	Paste Mask Top
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	124
{
LAYER_NAME	Drill Drawing
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	125
{
LAYER_NAME	Layer_125
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	126
{
LAYER_NAME	Silkscreen Top
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	127
{
LAYER_NAME	Assembly Drawing Top
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	128
{
LAYER_NAME	Solder Mask Bottom
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	129
{
LAYER_NAME	Silkscreen Bottom
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	130
{
LAYER_NAME	Assembly Drawing Bottom
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	131
{
LAYER_NAME	Layer_131
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	132
{
LAYER_NAME	Layer_132
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	133
{
LAYER_NAME	Layer_133
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	134
{
LAYER_NAME	Layer_134
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	135
{
LAYER_NAME	Layer_135
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	136
{
LAYER_NAME	Layer_136
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	137
{
LAYER_NAME	Layer_137
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	138
{
LAYER_NAME	Layer_138
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	139
{
LAYER_NAME	Layer_139
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	140
{
LAYER_NAME	Layer_140
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	141
{
LAYER_NAME	Layer_141
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	142
{
LAYER_NAME	Layer_142
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	143
{
LAYER_NAME	Layer_143
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	144
{
LAYER_NAME	Layer_144
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	145
{
LAYER_NAME	Layer_145
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	146
{
LAYER_NAME	Layer_146
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	147
{
LAYER_NAME	Layer_147
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	148
{
LAYER_NAME	Layer_148
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	149
{
LAYER_NAME	Layer_149
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	150
{
LAYER_NAME	Layer_150
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	151
{
LAYER_NAME	Layer_151
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	152
{
LAYER_NAME	Layer_152
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	153
{
LAYER_NAME	Layer_153
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	154
{
LAYER_NAME	Layer_154
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	155
{
LAYER_NAME	Layer_155
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	156
{
LAYER_NAME	Layer_156
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	157
{
LAYER_NAME	Layer_157
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	158
{
LAYER_NAME	Layer_158
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	159
{
LAYER_NAME	Layer_159
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	160
{
LAYER_NAME	Layer_160
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	161
{
LAYER_NAME	Layer_161
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	162
{
LAYER_NAME	Layer_162
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	163
{
LAYER_NAME	Layer_163
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	164
{
LAYER_NAME	Layer_164
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	165
{
LAYER_NAME	Layer_165
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	166
{
LAYER_NAME	Layer_166
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	167
{
LAYER_NAME	Layer_167
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	168
{
LAYER_NAME	Layer_168
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	169
{
LAYER_NAME	Layer_169
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	170
{
LAYER_NAME	Layer_170
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	171
{
LAYER_NAME	Layer_171
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	172
{
LAYER_NAME	Layer_172
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	173
{
LAYER_NAME	Layer_173
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	174
{
LAYER_NAME	Layer_174
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	175
{
LAYER_NAME	Layer_175
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	176
{
LAYER_NAME	Layer_176
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	177
{
LAYER_NAME	Layer_177
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	178
{
LAYER_NAME	Layer_178
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	179
{
LAYER_NAME	Layer_179
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	180
{
LAYER_NAME	Layer_180
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	181
{
LAYER_NAME	Layer_181
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	182
{
LAYER_NAME	Layer_182
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	183
{
LAYER_NAME	Layer_183
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	184
{
LAYER_NAME	Layer_184
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	185
{
LAYER_NAME	Layer_185
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	186
{
LAYER_NAME	Layer_186
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	187
{
LAYER_NAME	Layer_187
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	188
{
LAYER_NAME	Layer_188
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	189
{
LAYER_NAME	Layer_189
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	190
{
LAYER_NAME	Layer_190
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	191
{
LAYER_NAME	Layer_191
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	192
{
LAYER_NAME	Layer_192
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	193
{
LAYER_NAME	Layer_193
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	194
{
LAYER_NAME	Layer_194
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	195
{
LAYER_NAME	Layer_195
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	196
{
LAYER_NAME	Layer_196
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	197
{
LAYER_NAME	Layer_197
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	198
{
LAYER_NAME	Layer_198
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	199
{
LAYER_NAME	Layer_199
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	200
{
LAYER_NAME	Layer_200
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	201
{
LAYER_NAME	Layer_201
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	202
{
LAYER_NAME	Layer_202
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	203
{
LAYER_NAME	Layer_203
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	204
{
LAYER_NAME	Layer_204
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	205
{
LAYER_NAME	Layer_205
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	206
{
LAYER_NAME	Layer_206
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	207
{
LAYER_NAME	Layer_207
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	208
{
LAYER_NAME	Layer_208
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	209
{
LAYER_NAME	Layer_209
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	210
{
LAYER_NAME	Layer_210
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	211
{
LAYER_NAME	Layer_211
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	212
{
LAYER_NAME	Layer_212
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	213
{
LAYER_NAME	Layer_213
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	214
{
LAYER_NAME	Layer_214
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	215
{
LAYER_NAME	Layer_215
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	216
{
LAYER_NAME	Layer_216
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	217
{
LAYER_NAME	Layer_217
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	218
{
LAYER_NAME	Layer_218
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	219
{
LAYER_NAME	Layer_219
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	220
{
LAYER_NAME	Layer_220
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	221
{
LAYER_NAME	Layer_221
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	222
{
LAYER_NAME	Layer_222
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	223
{
LAYER_NAME	Layer_223
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	224
{
LAYER_NAME	Layer_224
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	225
{
LAYER_NAME	Layer_225
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	226
{
LAYER_NAME	Layer_226
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	227
{
LAYER_NAME	Layer_227
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	228
{
LAYER_NAME	Layer_228
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	229
{
LAYER_NAME	Layer_229
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	230
{
LAYER_NAME	Layer_230
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	231
{
LAYER_NAME	Layer_231
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	232
{
LAYER_NAME	Layer_232
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	233
{
LAYER_NAME	Layer_233
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	234
{
LAYER_NAME	Layer_234
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	235
{
LAYER_NAME	Layer_235
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	236
{
LAYER_NAME	Layer_236
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	237
{
LAYER_NAME	Layer_237
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	238
{
LAYER_NAME	Layer_238
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	239
{
LAYER_NAME	Layer_239
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	240
{
LAYER_NAME	Layer_240
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	241
{
LAYER_NAME	Layer_241
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	242
{
LAYER_NAME	Layer_242
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	243
{
LAYER_NAME	Layer_243
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	244
{
LAYER_NAME	Layer_244
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	245
{
LAYER_NAME	Layer_245
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	246
{
LAYER_NAME	Layer_246
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	247
{
LAYER_NAME	Layer_247
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	248
{
LAYER_NAME	Layer_248
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	249
{
LAYER_NAME	Layer_249
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	250
{
LAYER_NAME	Layer_250
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	MILS
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	10
COPPER_TO_VIA	10
COPPER_TO_PAD	10
COPPER_TO_SMD	10
COPPER_TO_COPPER	10
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	13
OUTLINE_TO_VIA	13
OUTLINE_TO_PAD	13
OUTLINE_TO_SMD	13
OUTLINE_TO_COPPER	13
DRILL_TO_TRACK	7
DRILL_TO_VIA	7
DRILL_TO_PAD	7
DRILL_TO_SMD	7
DRILL_TO_COPPER	7
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	30
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	50000
STUB_LENGTH	0
PARALLEL_LENGTH	1000
PARALLEL_GAP	200
TANDEM_LENGTH	1000
TANDEM_GAP	200
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	200
MATCH_LENGTH_TOLERANCE	200
}
}
RULE_SET	(4)
{
FOR	:
{
NET	PB0/RST
NET	$$$29264
NET	$$$18547
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	6
VIA_TO_TRACK	6
VIA_TO_VIA	6
PAD_TO_TRACK	6
PAD_TO_VIA	6
PAD_TO_PAD	6
SMD_TO_TRACK	6
SMD_TO_VIA	6
SMD_TO_PAD	6
SMD_TO_SMD	6
COPPER_TO_TRACK	20
COPPER_TO_VIA	20
COPPER_TO_PAD	20
COPPER_TO_SMD	20
COPPER_TO_COPPER	20
TEXT_TO_TRACK	6
TEXT_TO_VIA	6
TEXT_TO_PAD	6
TEXT_TO_SMD	6
OUTLINE_TO_TRACK	20
OUTLINE_TO_VIA	20
OUTLINE_TO_PAD	20
OUTLINE_TO_SMD	20
OUTLINE_TO_COPPER	20
DRILL_TO_TRACK	7
DRILL_TO_VIA	7
DRILL_TO_PAD	7
DRILL_TO_SMD	7
DRILL_TO_COPPER	7
SAME_NET_SMD_TO_VIA	6
SAME_NET_SMD_TO_CRN	6
SAME_NET_VIA_TO_VIA	6
SAME_NET_PAD_TO_CRN	6
MIN_TRACK_WIDTH	6
REC_TRACK_WIDTH	6
MAX_TRACK_WIDTH	30
DRILL_TO_DRILL	6
BODY_TO_BODY	6
SAME_NET_TRACK_TO_CRN	6
}
}
}
}

*FIELDS*    USER FIELDS

"Drawn By" 
"Checked By" 
"QC By" 
"Released By" 
"Drawn Date" 2020-07-01
"Checked Date" 
"QC Date" 
"Release Date" 
"Company Name" Nations
"TITLE" N32G030K6L7_STB
"CODE" 
"Drawing Number" 
"Revision" V1.0
"SCALE" 
"DRAWN" 
"CHECKED" 
"QUALITY CONTROL" 
"RELEASED" 
"COMPANY" 
"COMPANY ADDRESS" 
"DRAWING NO" 
"REV" 

*SHT*   1 NS-LINK -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        2.464          Scale of window expansion
WINDOWCENTER 6213   0       Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

2550   7150   0   1 222  10 0 "Regular Tahoma"
DEBUG USB
5350   1850   0   1 222  10 0 "Regular Tahoma"
HEADER
2250   4050   0   1 222  10 0 "Regular Tahoma"
LED
4850   7150   0   1 222  10 0 "Regular Tahoma"
MCU
6100   7550   0   1 222  10 0 "Regular Tahoma"
NS-LINK

*LINES*      LINES ITEMS

DRW20918         LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1200  232    0   0 111  10 1 "Regular Tahoma"
TITLE
-1202  -110   0   0 83   10 1 "Regular Tahoma"
Drawn Date
-300   42     0   0 83   10 1 "Regular Tahoma"
Revision
50     774    0   0 250  25 0 "Regular Tahoma"
A
50     2650   0   0 250  25 0 "Regular Tahoma"
B
50     4524   0   0 250  25 0 "Regular Tahoma"
C
50     6400   0   0 250  25 0 "Regular Tahoma"
D
-896   7400   0   0 250  25 0 "Regular Tahoma"
1
-2680  7400   0   0 250  25 0 "Regular Tahoma"
2
-4526  7400   0   0 250  25 0 "Regular Tahoma"
3
-6246  7400   0   0 250  25 0 "Regular Tahoma"
4
-8026  7400   0   0 250  25 0 "Regular Tahoma"
5
-9810  7400   0   0 250  25 0 "Regular Tahoma"
6
-1560  42     0   0 97   10 0 "Regular Tahoma"
SIZE:
-1560  -110   0   0 97   10 0 "Regular Tahoma"
DATED:
-10900 2650   0   0 250  25 0 "Regular Tahoma"
B
-10900 774    0   0 250  25 0 "Regular Tahoma"
A
-10900 4524   0   0 250  25 0 "Regular Tahoma"
C
-10900 6400   0   0 250  25 0 "Regular Tahoma"
D
-1102  42     0   0 83   10 1 "Regular Tahoma"
Sheet Size
-118   -110   0   0 83   10 1 "Regular Tahoma"
Number of Sheets
-320   -110   0   0 83   10 1 "Regular Tahoma"
Sheet Number
-630   -110   0   0 97   10 0 "Regular Tahoma"
SHEET:     OF
-630   42     0   0 97   10 0 "Regular Tahoma"
REV:
-1560  232    0   0 97   10 0 "Regular Tahoma"
TITLE:
D25057           LINES    3300   7400   1   0
CLOSED 5   10  0  
0      0     
0      -5100 
7400   -5100 
7400   0     
0      0     
D25058           LINES    700    7400   1   0
CLOSED 5   10  0  
0      0     
0      -2900 
2500   -2900 
2500   0     
0      0     
D25059           LINES    700    2200   1   0
CLOSED 5   10  0  
0      0     
0      -1600 
7400   -1600 
7400   0     
0      0     
D25060           LINES    700    4400   1   0
CLOSED 5   10  0  
0      0     
0      -2100 
2500   -2100 
2500   0     
0      0     
DRW26078         LINES    600    7800   1   0
OPEN   8   10  0  
0      0     
0      -7300 
7600   -7300 
7600   -5600 
10200  -5600 
10200  0     
0      0     
0      -100  

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CON_MINIUSB      32000 32000 100 10 100 10 4 1 0 11 0 0
TIMESTAMP 2019.12.11.09.21.40
"Default Font"
"Default Font"
80 1260 0 4 100 10 "Default Font"
REF-DES
290 -40 0 6 100 10 "Default Font"
PART-TYPE
340 -150 0 6 100 10 "Default Font"
*
350 -270 0 6 100 10 "Default Font"
*
OPEN   5   10  255
0     0    
0     1200 
500   1200 
500   0    
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CON-SIP-4P       32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.11.27.05.40.08
"Default Font"
"Default Font"
50 50 0 4 97 10 "Default Font"
REF-DES
100 -500 0 6 97 10 "Default Font"
PART-TYPE
100 -600 0 6 97 10 "Default Font"
*
100 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -500 
200   -500 
200   0    
0     0    
T-100  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -200  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -300  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -400  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

DIODE            32000 32000 90 10 80 10 4 4 0 2 18 0
TIMESTAMP 2019.12.01.15.48.44
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0

HEADER\8X2       32000 32000 100 10 100 10 4 18 0 16 0 0
TIMESTAMP 2019.03.12.09.21.06
"Default Font"
"Default Font"
300 950 0 4 100 10 "Default Font"
REF-DES
300 900 0 6 100 10 "Default Font"
PART-TYPE
350 -200 0 6 100 10 "Default Font"
SPIL PART #
350 -300 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
200   600  
250   600  
CIRCLE 2   10  255
200   500  
250   500  
CIRCLE 2   10  255
200   400  
250   400  
CIRCLE 2   10  255
200   300  
250   300  
CIRCLE 2   10  255
200   200  
250   200  
CIRCLE 2   10  255
200   100  
250   100  
CIRCLE 2   10  255
200   0    
250   0    
CIRCLE 2   10  255
300   600  
350   600  
CIRCLE 2   10  255
300   500  
350   500  
CIRCLE 2   10  255
300   400  
350   400  
CIRCLE 2   10  255
300   300  
350   300  
CIRCLE 2   10  255
300   200  
350   200  
CIRCLE 2   10  255
300   100  
350   100  
CIRCLE 2   10  255
300   0    
350   0    
CLOSED 5   10  255
150   650  
400   650  
400   -150 
150   -150 
150   650  
CIRCLE 2   10  255
200   -100 
250   -100 
CIRCLE 2   10  255
300   -100 
350   -100 
CIRCLE 2   10  255
300   -100 
350   -100 
T0     600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

N32G4XC          32000 32000 97 10 97 10 4 1 0 48 0 0
TIMESTAMP 2019.11.28.08.56.49
"Default Font"
"Default Font"
2300 2340 0 0 97 10 "Default Font"
REF-DES
2300 -40 0 2 97 10 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 "Default Font"
*
2300 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2300  0    
2300  2300 
0     2300 
0     0    
T-200  1700  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1700  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.28
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CAP              32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2019.11.28.11.16.25
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CON1X3           32000 32000 100 10 100 10 4 7 0 3 0 0
TIMESTAMP 2019.12.01.16.15.06
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 -250 0 6 100 10 "Default Font"
PART-TYPE
0 -240 0 6 100 10 "Default Font"
*
0 -340 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
0     50   
0     150  
CIRCLE 2   10  255
0     -50  
0     50   
CLOSED 5   10  255
-100  200  
-100  -200 
100   -200 
100   200  
-100  200  
CIRCLE 2   10  255
0     -50  
0     -150 
OPEN   2   10  255
-100  100  
-50   100  
OPEN   2   10  255
-100  -100 
-50   -100 
OPEN   2   10  255
-50   0    
-100  0    
T-200  100   0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

MINIUSB CON  1   0   0     0
TIMESTAMP 2019.12.11.09.21.39
GATE 1 11 0
CON_MINIUSB
1 0 U VBUS
2 0 U D-
3 0 U D+
4 0 U ID
5 0 U GND
6 0 U SHIELD1
7 0 U SHIELD2
8 0 U SHIELD3
9 0 U SHIELD4
10 0 U H1
11 0 U H2

CON-SIP-4P CON  1   0   0     0
TIMESTAMP 2019.11.27.05.40.07
GATE 1 4 0
CON-SIP-4P
1 0 U
2 0 U
3 0 U
4 0 U

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

DIODE_2 UND  1   0   0     0
TIMESTAMP 2019.12.01.15.48.43
GATE 1 2 0
DIODE
1 0 U
2 0 U

HEADER-8X2 CON  1   0   0     0
TIMESTAMP 2019.03.12.09.21.05
GATE 1 16 0
HEADER\8X2
1 0 U
3 0 U
5 0 U
7 0 U
9 0 U
11 0 U
13 0 U
15 0 U
2 0 U
4 0 U
6 0 U
8 0 U
10 0 U
12 0 U
14 0 U
16 0 U

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

N32G4XC UND  1   0   0     0
TIMESTAMP 2019.11.28.08.56.48
GATE 1 48 0
N32G4XC
1 0 U VBAT
2 0 U PC13-TAMPER-RTC
3 0 U PC14-OSC32_IN
4 0 U PC15-OSC32_OUT
5 0 U PD0-OSC_IN
6 0 U PD1-OSC_OUT
7 0 U NRST
8 0 U VSSA
9 0 U VDDA
10 0 U PA0-WKUP
11 0 U PA1
12 0 U PA2
13 0 U PA3
14 0 U PA4
15 0 U PA5
16 0 U PA6
17 0 U PA7
18 0 U PB0
19 0 U PB1
20 0 U PB2-BOOT
21 0 U PB10
22 0 U PB11
23 0 U VSS_1
24 0 U VDD_1
25 0 U PB12
26 0 U PB13
27 0 U PB14
28 0 U PB15
29 0 U PA8
30 0 U PA9
31 0 U PA10
32 0 U PA11
33 0 U PA12
34 0 U PA13-SWDIO
35 0 U VSS_2
36 0 U VDD_2
37 0 U PA14-SWCLK
38 0 U PA15
39 0 U PB3
40 0 U PB4
41 0 U PB5
42 0 U PB6
43 0 U PB7
44 0 U BOOT0
45 0 U PB8
46 0 U PB9
47 0 U VSS_3
48 0 U VDD_3

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

C0603 CAP  1   0   0     0
TIMESTAMP 2019.11.28.11.16.24
GATE 1 2 0
CAP
1 1 U
2 1 U

CON1X3 CON  1   0   0     3
TIMESTAMP 2019.12.01.16.15.04
GATE 1 3 0
CON1X3
1 0 U
2 0 U
3 0 U
1 2 3 

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U



*PART*       ITEMS



J4           MINIUSB          1350  5150    0 1 97 10 97 10 4 3 11 0 0 0
"Regular Tahoma"
"Regular Tahoma"
250 1300 0 4 97 10 0 "Regular Tahoma"
REF-DES
290 -40 0 6 97 10 0 "Regular Tahoma"
PART-TYPE
340 -150 0 6 97 10 0 "Regular Tahoma"
*
350 -270 0 6 97 10 0 "Regular Tahoma"
*
"DECAL" 
"Description" 6 pin header
"PCB DECAL" CON_MINIUSB
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1

J10          CON-SIP-4P       7000  1600    0 0 97 10 97 10 4 1 4 0 0 2
"Default Font"
"Default Font"
100 50 0 4 97 10 0 "Default Font"
REF-DES
100 -500 0 6 97 10 0 "Default Font"
PART-TYPE
100 -600 0 6 97 10 0 "Default Font"
*
100 -700 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SIP-4P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1
3 60 10 0 1

R20          R0402            2750  3650    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R15          R0402            2750  3050    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D6           LED0805          1850  3700    0 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
300 -200 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D7           LED0805          1850  3100    0 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
300 -200 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D5           DIODE_2          2050  6400    0 0 83 10 83 10 4 2 2 0 0 18
"Regular Tahoma"
"Regular Tahoma"
250 150 0 4 97 10 0 "Regular Tahoma"
REF-DES
250 -150 0 6 97 10 0 "Regular Tahoma"
PART-TYPE
300 -150 0 6 97 10 1 "Regular Tahoma"
VALUE
250 -350 0 6 97 10 0 "Regular Tahoma"
*
"PCB DECAL" SOD123
"VALUE" SS14L
0 130 14 0 1
1 130 14 0 1

J5           HEADER-8X2       2750  1000    0 0 97 10 97 10 4 10 16 0 0 2
"Regular Tahoma"
"Regular Tahoma"
300 -250 0 4 97 10 0 "Regular Tahoma"
REF-DES
300 900 0 6 97 10 0 "Regular Tahoma"
PART-TYPE
350 -200 0 6 97 10 2 "Regular Tahoma"
Spil Part #
350 -300 0 6 97 10 0 "Regular Tahoma"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"Description" 7 X 2 PIN POLARIZED HEADER, 0.1" CENTERS
"Cost" 
"Part Number" 
"Manufacturer #1" 
"Spil Part #" 34-117
"Mating Spil Part #" ???
"PCB DECAL" HEADER16
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1

R11          R0402            1850  6100    0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 100 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R12          R0402            1850  6000    0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -50 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 100 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C22          CAP1206          1800  6850    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
40 -170 0 0 83 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
40 -310 0 2 83 10 3 "Default Font"
Value
180 -360 0 2 83 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

U4           N32G4XC          6400  3400    0 0 97 10 97 10 4 2 48 0 0 2
"Default Font"
"Default Font"
1050 1300 0 0 97 10 0 "Default Font"
REF-DES
950 1050 0 2 97 10 0 "Default Font"
PART-TYPE
850 1050 0 2 97 10 1 "Default Font"
Value
2300 -240 0 2 97 10 0 "Default Font"
*
"PCB DECAL" QFP48-3
"Value" N32G455CCL7
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

C30          0402C            4250  5400    0 0 97 10 97 10 3 22 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
0 90 0 4 69 7 0 "Regular Tahoma"
REF-DES
10 -80 0 6 69 7 0 "Regular Tahoma"
PART-TYPE
10 -160 0 6 69 7 3 "Regular Tahoma"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C32          0402C            4250  4600    0 0 97 10 97 10 3 22 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
0 90 0 4 69 7 0 "Regular Tahoma"
REF-DES
10 -80 0 6 69 7 0 "Regular Tahoma"
PART-TYPE
10 -160 0 6 69 7 3 "Regular Tahoma"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

R19          R0402            9000  4050    0 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -40 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 140 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 100R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R17          R0402            7650  2750   90 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
200 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 160 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R4           R0402            4750  4050    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 -10 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R18          R0402            7350  6400   90 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
150 -50 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -50 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C5           C0603            5350  5350    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C9           C0603            5500  4200    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C14          C0603            8300  3100    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C18          C0603            9200  5600    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C19          C0603            6000  5800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
-150 -400 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
-250 -100 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C20          C0603            6300  5800    0 3 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
-150 -400 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
-250 -100 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

R24          R0402            6050  4150    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J12          CON1X3           5900  6900    0 1 97 10 97 10 4 2 3 0 0 2
"Regular Tahoma"
"Regular Tahoma"
0 250 0 4 97 10 0 "Regular Tahoma"
REF-DES
0 -250 0 6 97 10 0 "Regular Tahoma"
PART-TYPE
0 -240 0 6 97 10 0 "Regular Tahoma"
*
0 -340 0 6 97 10 0 "Regular Tahoma"
*
"Marking" 
"PCB DECAL" 2.54MM_CON3P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1

C1           C0603            5000  3900    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

Y1           CRYSTAL_2PIN     4700  5250   90 3 97 10 97 10 4 2 2 0 0 2
"Default Font"
"Default Font"
250 -200 90 4 97 10 0 "Default Font"
REF-DES
260 -120 0 6 97 10 0 "Default Font"
PART-TYPE
350 -200 90 5 97 10 1 "Default Font"
Value
240 -396 0 6 97 10 0 "Default Font"
*
"Value" 8MHz
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 1800   6850   0 3 0
@@@O1    DP_NSLINK $OSR_SYMS 2350   6050   0 1 0
@@@O2    DM_NSLINK $OSR_SYMS 2350   6150   0 1 0
@@@O3    GND $GND_SYMS 1750   5450   0 0 0
@@@O4    GND $GND_SYMS 3000   3050   0 0 0
@@@O5    LED_CON/PB6 $OSR_SYMS 1750   3700   0 0 0
@@@O6    LED_RUN/PA8 $OSR_SYMS 1750   3100   0 0 0
@@@O7    5V $PWR_SYMS 2750   6450   0 0 0
@@@O8    VDD_LINK $PWR_SYMS 6750   1600   0 0 0
@@@O9    PA13/TMS/SWDIO $OSR_SYMS 6700   1400   0 0 0
@@@O10   PA14/TCK/SWCLK $OSR_SYMS 6700   1300   0 0 0
@@@O11   GND $GND_SYMS 6750   1150   0 0 0
@@@O12   PB0/RST $OSR_SYMS 2250   1100   0 0 0
@@@O13   VDD_LINK $PWR_SYMS 2550   1700   0 0 0
@@@O14   MCU_PA14/SWDCK $OSR_SYMS 3750   1400   0 1 0
@@@O15   MCU_PA13/SWDIO $OSR_SYMS 3750   1500   0 1 0
@@@O16   NSLINK_TMS_SWDIO $OSR_SYMS 2250   1500   0 0 0
@@@O17   NSLINK_TCK_SWCLK $OSR_SYMS 2250   1400   0 0 0
@@@O18   NRST $OSR_SYMS 3750   1100   0 1 0
@@@O19   VDD_LINK $PWR_SYMS 3450   1700   0 0 0
@@@O20   5V $PWR_SYMS 2500   1000   90 0 0
@@@O21   5V $PWR_SYMS 3750   1000   90 1 0
@@@O22   GND $GND_SYMS 2700   900    90 1 0
@@@O23   GND $GND_SYMS 3500   900    90 0 0
@@@O24   MCU_PA9/TX1 $OSR_SYMS 3750   1300   0 3 0
@@@O25   MCU_PA10/RX1 $OSR_SYMS 3750   1200   0 3 0
@@@O26   NSLINK_USART1_TX $OSR_SYMS 2250   1200   0 0 0
@@@O27   NSLINK_USART1_RX $OSR_SYMS 2250   1300   0 0 0
@@@O28   VDD_LINK $PWR_SYMS 4300   4100   90 0 0
@@@O29   GND $GND_SYMS 5000   3350   0 0 0
@@@O30   DM_NSLINK $OSR_SYMS 9450   4700   0 1 0
@@@O31   DP_NSLINK $OSR_SYMS 9450   4800   0 1 0
@@@O32   PB0/RST $OSR_SYMS 7500   3050   90 0 0
@@@O33   PA14/TCK/SWCLK $OSR_SYMS 8100   6000   90 2 0
@@@O34   PA13/TMS/SWDIO $OSR_SYMS 9450   4900   0 1 0
@@@O35   LED_RUN/PA8 $OSR_SYMS 9450   4400   0 1 0
@@@O36   LED_CON/PB6 $OSR_SYMS 7600   6000   90 2 0
@@@O37   GND $GND_SYMS 7700   2600   0 0 0
@@@O38   VDD_LINK $PWR_SYMS 5600   5800   0 0 0
@@@O39   VDD_LINK $PWR_SYMS 7000   6450   0 0 0
@@@O40   VDD_LINK $PWR_SYMS 9000   5800   0 0 0
@@@O41   GND $GND_SYMS 9250   5000   90 0 0
@@@O42   GND $GND_SYMS 7100   6100   0 2 0
@@@O43   GND $GND_SYMS 8000   3000   0 0 0
@@@O44   VDD_LINK $PWR_SYMS 8550   3100   90 1 0
@@@O45   NSLINK_TCK_SWCLK $OSR_SYMS 9450   4100   0 1 0
@@@O46   NSLINK_TMS_SWDIO $OSR_SYMS 9450   4200   0 1 0
@@@O47   GND $GND_SYMS 4050   4600   90 1 0
@@@O48   GND $GND_SYMS 4050   5400   90 1 0
@@@O49   GND $GND_SYMS 6200   4400   90 1 0
@@@O50   VDD_LINK $PWR_SYMS 6150   7000   90 1 0
@@@O51   GND $GND_SYMS 6200   6800   90 0 0
@@@O52   NSLINK_USART1_RX $OSR_SYMS 9450   4600   0 1 0
@@@O53   NSLINK_USART1_TX $OSR_SYMS 9450   4500   0 1 0
@@@O54   GND $GND_SYMS 6200   5700   0 0 0
@@@O55   GND $GND_SYMS 5350   4900   0 0 0
@@@O56   GND $GND_SYMS 5500   3450   0 0 0
@@@O57   GND $GND_SYMS 8300   2600   0 0 0

*TIEDOTS*



@@@D0    1750   5750  
@@@D1    1750   5650  
@@@D2    1750   5550  
@@@D3    1750   5450  
@@@D4    1800   6400  
@@@D5    3000   3100  
@@@D6    5000   4100  
@@@D7    9350   4200  
@@@D8    4700   5400  
@@@D9    4700   4600  
@@@D10   5600   4300  
@@@D11   5600   5100  
@@@D12   6200   5700  
@@@D13   7000   6400  
@@@D14   6300   6400  
@@@D15   5600   5550  
@@@D16   5600   4300  
@@@D17   8300   3100  
@@@D18   9000   5700  
@@@D19   9200   5000  

*CONNECTION*


*SIGNAL* MCU_PA10/RX1 0 0
J5.10        @@@O25       2 0
3300   1200  
3750   1200  

*SIGNAL* MCU_PA13/SWDIO 0 0
@@@O15       J5.4         2 0
3750   1500  
3300   1500  

*SIGNAL* MCU_PA9/TX1 0 0
J5.8         @@@O24       2 0
3300   1300  
3750   1300  

*SIGNAL* MCU_PA14/SWDCK 0 0
@@@O14       J5.6         2 0
3750   1400  
3300   1400  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        C22.1        2 0
1800   6850  
1800   6850  
J4.5         @@@D0        3 0
1550   5850  
1750   5850  
1750   5750  
J4.6         @@@D0        2 0
1550   5750  
1750   5750  
@@@D0        @@@D1        2 0
1750   5750  
1750   5650  
J4.7         @@@D1        2 0
1550   5650  
1750   5650  
@@@D1        @@@D2        2 0
1750   5650  
1750   5550  
J4.8         @@@D2        2 0
1550   5550  
1750   5550  
@@@D2        @@@D3        2 0
1750   5550  
1750   5450  
J4.9         @@@D3        2 0
1550   5450  
1750   5450  
@@@D3        @@@O3        2 0
1750   5450  
1750   5450  
@@@D5        R20.1        3 0
3000   3100  
3000   3700  
2850   3700  
@@@D5        R15.1        2 0
3000   3100  
2850   3100  
@@@D5        @@@O4        2 0
3000   3100  
3000   3050  
J10.4        @@@O11       3 0
6900   1200  
6750   1200  
6750   1150  
J5.15        @@@O22       2 0
2750   900   
2700   900   
J5.16        @@@O23       2 0
3300   900   
3500   900   
C1.2         @@@O29       2 0
5000   3400  
5000   3350  
@@@O37       R17.1        2 0
7700   2600  
7700   2650  
U4.35        @@@D19       2 0
8900   5000  
9200   5000  
U4.47        @@@O42       2 0
7100   5900  
7100   6100  
@@@O47       C32.1        2 0
4050   4600  
4150   4600  
C30.1        @@@O48       2 0
4150   5400  
4050   5400  
U4.8         @@@O49       2 0
6200   4400  
6200   4400  
U4.23        @@@O43       2 0
8000   3200  
8000   3000  
J12.3        @@@O51       2 0
6100   6800  
6200   6800  
C20.1        @@@D12       3 0
6300   5800  
6300   5700  
6200   5700  
@@@D12       C19.1        3 0
6200   5700  
6000   5700  
6000   5800  
@@@D12       @@@O54       2 0
6200   5700  
6200   5700  
C5.2         @@@O55       2 0
5350   4850  
5350   4900  
C9.2         @@@O56       2 0
5500   3700  
5500   3450  
C14.2        @@@O57       2 0
8300   2600  
8300   2600  
C18.2        @@@D19       2 0
9200   5100  
9200   5000  
@@@D19       @@@O41       2 0
9200   5000  
9250   5000  

*SIGNAL* NRST 0 0
@@@O18       J5.12        2 0
3750   1100  
3300   1100  

*SIGNAL* 5V 0 0
D5.1         @@@O7        3 0
2550   6400  
2750   6400  
2750   6450  
J5.13        @@@O20       2 0
2750   1000  
2500   1000  
J5.14        @@@O21       2 0
3300   1000  
3750   1000  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J10.1        @@@O8        3 0
6900   1500  
6750   1500  
6750   1600  
J5.1         @@@O13       3 0
2750   1600  
2550   1600  
2550   1700  
J5.2         @@@O19       3 0
3300   1600  
3450   1600  
3450   1700  
@@@O28       R4.2         2 0
4300   4100  
4450   4100  
U4.9         @@@D10       2 0
6200   4300  
5600   4300  
@@@O38       @@@D15       2 0
5600   5800  
5600   5550  
@@@O39       @@@D13       2 0
7000   6450  
7000   6400  
@@@D18       @@@O40       2 0
9000   5700  
9000   5800  
C14.1        @@@D17       2 0
8300   3100  
8300   3100  
@@@D10       R24.2        3 0
5600   4300  
5600   4200  
5750   4200  
@@@D11       @@@D16       2 0
5600   5100  
5600   4300  
@@@D11       U4.1         2 0
5600   5100  
6200   5100  
J12.1        @@@O50       2 0
6100   7000  
6150   7000  
@@@D13       @@@D14       2 0
7000   6400  
6300   6400  
C20.2        @@@D14       2 0
6300   6300  
6300   6400  
@@@D13       U4.48        2 0
7000   6400  
7000   5900  
@@@D14       C19.2        3 0
6300   6400  
6000   6400  
6000   6300  
C5.1         @@@D15       3 0
5350   5350  
5350   5550  
5600   5550  
@@@D15       @@@D11       2 0
5600   5550  
5600   5100  
C9.1         @@@D16       3 0
5500   4200  
5500   4300  
5600   4300  
@@@D16       @@@D10       2 0
5600   4300  
5600   4300  
U4.24        @@@D17       3 0
8100   3200  
8100   3100  
8300   3100  
@@@D17       @@@O44       2 0
8300   3100  
8550   3100  
@@@D18       U4.36        3 0
9000   5700  
9000   5100  
8900   5100  
@@@D18       C18.1        3 0
9000   5700  
9200   5700  
9200   5600  

*SIGNAL* $$$4465 64 0
C22.2        @@@D4        2 0
1800   6350  
1800   6400  
@@@D4        J4.1         3 0
1800   6400  
1800   6250  
1550   6250  
@@@D4        D5.2         2 0
1800   6400  
2050   6400  

*SIGNAL* DM_NSLINK 0 0
R11.2        @@@O2        2 0
2150   6150  
2350   6150  
U4.32        @@@O30       2 0
8900   4700  
9450   4700  

*SIGNAL* DP_NSLINK 0 0
R12.2        @@@O1        2 0
2150   6050  
2350   6050  
U4.33        @@@O31       2 0
8900   4800  
9450   4800  

*SIGNAL* $$$24935 64 0
J4.2         R11.1        2 0
1550   6150  
1750   6150  

*SIGNAL* $$$24997 64 0
J4.3         R12.1        2 0
1550   6050  
1750   6050  

*SIGNAL* $$$32273 64 0
D6.1         R20.2        2 0
2350   3700  
2450   3700  

*SIGNAL* $$$32275 64 0
D7.1         R15.2        2 0
2350   3100  
2450   3100  

*SIGNAL* LED_CON/PB6 0 0
D6.2         @@@O5        2 0
1850   3700  
1750   3700  
U4.42        @@@O36       2 0
7600   5900  
7600   6000  

*SIGNAL* LED_RUN/PA8 0 0
D7.2         @@@O6        2 0
1850   3100  
1750   3100  
@@@O35       U4.29        2 0
9450   4400  
8900   4400  

*SIGNAL* PA13/TMS/SWDIO 0 0
J10.2        @@@O9        2 0
6900   1400  
6700   1400  
U4.34        @@@O34       2 0
8900   4900  
9450   4900  

*SIGNAL* PA14/TCK/SWCLK 0 0
J10.3        @@@O10       2 0
6900   1300  
6700   1300  
U4.37        @@@O33       2 0
8100   5900  
8100   6000  

*SIGNAL* PB0/RST 0 0
@@@O12       J5.11        2 0
2250   1100  
2750   1100  
@@@O32       U4.18        2 0
7500   3050  
7500   3200  

*SIGNAL* NSLINK_TMS_SWDIO 0 0
J5.3         @@@O16       2 0
2750   1500  
2250   1500  
@@@D7        U4.27        2 0
9350   4200  
8900   4200  
R19.2        @@@D7        3 0
9300   4000  
9350   4000  
9350   4200  
@@@D7        @@@O46       2 0
9350   4200  
9450   4200  

*SIGNAL* NSLINK_TCK_SWCLK 0 0
J5.5         @@@O17       2 0
2750   1400  
2250   1400  
@@@O45       U4.26        2 0
9450   4100  
8900   4100  

*SIGNAL* NSLINK_USART1_TX 0 0
J5.9         @@@O26       2 0
2750   1200  
2250   1200  
U4.30        @@@O53       2 0
8900   4500  
9450   4500  

*SIGNAL* NSLINK_USART1_RX 0 0
J5.7         @@@O27       2 0
2750   1300  
2250   1300  
U4.31        @@@O52       2 0
8900   4600  
9450   4600  

*SIGNAL* $$$14362 64 0
R4.1         @@@D6        2 0
4850   4100  
5000   4100  
@@@D6        U4.7         4 0
5000   4100  
5300   4100  
5300   4500  
6200   4500  
@@@D6        C1.1         2 0
5000   4100  
5000   3900  

*SIGNAL* $$$32474 64 0
R17.2        U4.20        2 0
7700   3050  
7700   3200  

*SIGNAL* $$$32494 64 0
U4.44        R18.1        2 0
7400   5900  
7400   6300  

*SIGNAL* $$$29264 64 0
R18.2        J12.2        3 0
7400   6700  
7400   6900  
6100   6900  

*SIGNAL* $$$18547 64 0
U4.25        R19.1        2 0
8900   4000  
8900   4000  

*SIGNAL* $$$26932 64 0
Y1.2         @@@D9        2 0
4700   4698  
4700   4600  
U4.6         @@@D9        2 0
6200   4600  
4700   4600  
@@@D9        C32.2        2 0
4700   4600  
4350   4600  

*SIGNAL* $$$26931 64 0
Y1.1         @@@D8        2 0
4700   5298  
4700   5400  
U4.5         @@@D8        4 0
6200   4700  
5100   4700  
5100   5400  
4700   5400  
@@@D8        C30.2        2 0
4700   5400  
4350   5400  

*SIGNAL* $$$3902 64 0
U4.10        R24.1        2 0
6200   4200  
6150   4200  

*NETNAMES*



DP_NSLINK    @@@O1        320    -40    0 0 0      0      0 3 -1 12 97 "Default Font"
DM_NSLINK    @@@O2        322    -32    0 0 0      0      0 3 -1 12 97 "Default Font"
LED_CON/PB6  @@@O5        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
LED_RUN/PA8  @@@O6        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
5V           @@@O7        0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O8        0      250    0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
PA13/TMS/SWDIO @@@O9        -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
PA14/TCK/SWCLK @@@O10       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
PB0/RST      @@@O12       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O13       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O14       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O15       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
NSLINK_TMS_SWDIO @@@O16       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NSLINK_TCK_SWCLK @@@O17       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NRST         @@@O18       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O19       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
5V           @@@O20       -290   -40    0 4 0      0      0 0 -1 10 97 "Default Font"
5V           @@@O21       310    -50    0 4 0      0      0 0 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O24       360    0      0 0 0      0      90 3 -1 10 97 "Regular Tahoma"
MCU_PA10/RX1 @@@O25       360    0      0 0 0      0      90 3 -1 10 97 "Regular Tahoma"
NSLINK_USART1_TX @@@O26       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
NSLINK_USART1_RX @@@O27       -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O28       -400   0      0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
DM_NSLINK    @@@O30       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
DP_NSLINK    @@@O31       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
PB0/RST      @@@O32       -50    -350   90 3 0      0      90 3 -1 10 97 "Regular Tahoma"
PA14/TCK/SWCLK @@@O33       -50    950    90 3 0      0      90 3 -1 10 97 "Regular Tahoma"
PA13/TMS/SWDIO @@@O34       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
LED_RUN/PA8  @@@O35       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
LED_CON/PB6  @@@O36       -50    850    90 3 0      0      90 3 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O38       0      250    0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O39       -300   100    0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O40       0      250    0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O44       400    50     0 7 0      0      0 0 -1 10 97 "Regular Tahoma"
NSLINK_TCK_SWCLK @@@O45       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
NSLINK_TMS_SWDIO @@@O46       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O50       400    0      0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
NSLINK_USART1_RX @@@O52       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"
NSLINK_USART1_TX @@@O53       360    0      0 0 0      0      0 3 -1 10 97 "Regular Tahoma"

*SHT*   2 MCU -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        5.440          Scale of window expansion
WINDOWCENTER 3758   1486    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

9700   4350   0   0 222  10 0 "Regular Tahoma"
RESET
7150   4350   0   0 222  10 0 "Regular Tahoma"
MCU WAKEUP
7700   7508   0   1 222  10 0 "Regular Tahoma"
KEY
10080  7508   0   1 222  10 0 "Regular Tahoma"
LED
3600   7508   0   1 222  10 0 "Regular Tahoma"
LDO
2700   5400   0   1 222  10 0 "Regular Tahoma"
MCU
7000   1700   0   0 222  10 0 "Regular Tahoma"
I2C RES

*LINES*      LINES ITEMS

DRW_NATIONS_A4   LINES    11200  550    35  25
OPEN   2   10  255
0      0     
-1600  0     
OPEN   2   10  255
-1600  650   
-1600  -150  
CLOSED 5   10  255
0      -150  
0      850   
-1600  850   
-1600  -150  
0      -150  
OPEN   2   10  255
0      150   
-1600  150   
OPEN   2   10  255
0      400   
-1600  400   
OPEN   2   10  255
-1600  850   
-1600  -150  
OPEN   2   10  255
-700   0     
-700   -150  
OPEN   2   10  255
0      250   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
0      450   
0      -26   
OPEN   2   10  255
-2506  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-2500  -150  
-3750  -150  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
OPEN   2   10  255
-1736  7350  
0      7350  
CLOSED 3   10  255
0      7350  
-1736  7350  
0      7350  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
0      7250  
0      6750  
OPEN   2   10  255
250    1724  
0      1724  
OPEN   2   10  255
250    3574  
0      3574  
OPEN   2   10  255
250    5474  
0      5474  
OPEN   2   10  255
-1786  7600  
-1786  7350  
OPEN   2   10  255
-3570  7600  
-3570  7350  
OPEN   2   10  255
-5350  7600  
-5350  7350  
OPEN   2   10  255
-7136  7600  
-7136  7350  
OPEN   2   10  255
-8920  7600  
-8920  7350  
OPEN   2   10  255
-10700 5474  
-10950 5474  
OPEN   2   10  255
-10700 3600  
-10950 3600  
OPEN   2   10  255
-10700 1724  
-10950 1724  
CLOSED 5   10  255
0      -150  
0      7350  
-10700 7350  
-10700 -150  
0      -150  
OPEN   2   10  255
-700   0     
-700   150   
-1200  232    0   0 111  10 1 "Regular Tahoma"
TITLE
-1560  232    0   0 97   10 0 "Regular Tahoma"
TITLE:
-630   42     0   0 97   10 0 "Regular Tahoma"
REV:
-630   -110   0   0 97   10 0 "Regular Tahoma"
SHEET:     OF
-320   -110   0   0 83   10 1 "Regular Tahoma"
Sheet Number
-118   -110   0   0 83   10 1 "Regular Tahoma"
Number of Sheets
-1102  42     0   0 83   10 1 "Regular Tahoma"
Sheet Size
-300   42     0   0 83   10 1 "Regular Tahoma"
Revision
-10900 6400   0   0 250  25 0 "Regular Tahoma"
D
-10900 4524   0   0 250  25 0 "Regular Tahoma"
C
-10900 774    0   0 250  25 0 "Regular Tahoma"
A
-10900 2650   0   0 250  25 0 "Regular Tahoma"
B
-1202  -110   0   0 83   10 1 "Regular Tahoma"
Drawn Date
-1560  -110   0   0 97   10 0 "Regular Tahoma"
DATED:
-1560  42     0   0 97   10 0 "Regular Tahoma"
SIZE:
-9810  7400   0   0 250  25 0 "Regular Tahoma"
6
-8026  7400   0   0 250  25 0 "Regular Tahoma"
5
-6246  7400   0   0 250  25 0 "Regular Tahoma"
4
-4526  7400   0   0 250  25 0 "Regular Tahoma"
3
-2680  7400   0   0 250  25 0 "Regular Tahoma"
2
-896   7400   0   0 250  25 0 "Regular Tahoma"
1
50     6400   0   0 250  25 0 "Regular Tahoma"
D
50     4524   0   0 250  25 0 "Regular Tahoma"
C
50     2650   0   0 250  25 0 "Regular Tahoma"
B
50     774    0   0 250  25 0 "Regular Tahoma"
A
D22894           LINES    8700   4700   1   0
CLOSED 5   10  0  
0      0     
0      -2600 
2400   -2600 
2400   0     
0      0     
D22895           LINES    6500   4700   1   0
CLOSED 5   10  0  
0      0     
0      -2600 
2100   -2600 
2100   0     
0      0     
D23128           LINES    6500   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2100   -3000 
2100   0     
0      0     
D23129           LINES    8700   7800   1   0
CLOSED 5   10  0  
0      0     
0      -3000 
2400   -3000 
2400   0     
0      0     
D24779           LINES    600    5800   1   0
CLOSED 5   10  0  
0      0     
0      -5300 
5800   -5300 
5800   0     
0      0     
D24819           LINES    600    7800   1   0
CLOSED 5   10  0  
0      0     
0      -1900 
5800   -1900 
5800   0     
0      0     
D31185           LINES    6500   2000   1   0
CLOSED 5   10  0  
0      0     
0      -1500 
2100   -1500 
2100   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CAP              32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2019.11.28.11.16.25
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2020.05.30.04.20.05
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

SPX1117-3V3      32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.12.11.09.57.22
"Default Font"
"Default Font"
200 100 0 4 97 10 "Default Font"
REF-DES
200 -500 0 6 97 10 "Default Font"
PART-TYPE
200 -600 0 6 97 10 "Default Font"
*
200 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -400 
400   -400 
400   0    
0     0    
T-200  -300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

SW_2P            32000 32000 97 10 97 10 4 6 0 2 16 0
TIMESTAMP 2019.01.05.10.52.59
"Default Font"
"Default Font"
0 100 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
0 -200 0 6 97 10 "Default Font"
*
0 -300 0 6 97 10 "Default Font"
*
OPEN   2   20  255
-150  40   
150   40   
OPEN   2   30  255
-80   60   
80    60   
CIRCLE 2   10  255
-60   0    
-100  0    
CIRCLE 2   10  255
100   0    
60    0    
OPEN   2   10  255
80    0    
200   0    
OPEN   2   10  255
-80   0    
-200  0    
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T200   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

HEAD2X10         32000 32000 97 10 97 10 4 1 0 20 0 0
TIMESTAMP 2019.12.01.07.43.15
"Default Font"
"Default Font"
200 1140 0 4 97 10 "Default Font"
REF-DES
150 -40 0 6 97 10 "Default Font"
PART-TYPE
150 -140 0 6 97 10 "Default Font"
*
150 -240 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
200   0    
200   1100 
0     1100 
0     0    
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.42
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0201R            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2018.02.11.07.24.24
"Default Font"
"Default Font"
370 -200 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     30   
0     -30  
200   -30  
200   30   
0     30   
T-100  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

N32G032K6L7      32000 32000 97 10 97 10 4 1 0 32 0 0
TIMESTAMP 2020.12.17.03.28.54
"Default Font"
"Default Font"
1900 1940 0 0 97 10 "Default Font"
REF-DES
1900 -40 0 2 97 10 "Default Font"
PART-TYPE
1900 -140 0 2 97 10 "Default Font"
*
1900 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
1500  0    
1500  1500 
0     1500 
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1700  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

C0603 CAP  1   0   0     0
TIMESTAMP 2019.11.28.11.16.24
GATE 1 2 0
CAP
1 1 U
2 1 U

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2020.05.30.04.20.03
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

AMS1117-3.3 UND  1   0   0     0
TIMESTAMP 2019.12.11.09.57.22
GATE 1 4 0
SPX1117-3V3
1 0 U GND
2 0 U OUT
3 0 U IN
4 0 U OUT

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

SW_2P UND  1   0   0     2
TIMESTAMP 2019.01.05.10.52.56
GATE 1 2 0
SW_2P
1 0 U
2 0 U
1 2 

HEAD2X10 UND  1   0   0     0
TIMESTAMP 2019.12.01.07.43.14
GATE 1 20 0
HEAD2X10
1 0 L
2 0 L
3 0 L
4 0 L
5 0 L
6 0 L
7 0 L
8 0 L
9 0 L
10 0 L
11 0 L
12 0 L
13 0 L
14 0 L
15 0 L
16 0 L
17 0 L
18 0 L
19 0 L
20 0 L

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U

0201R RES  1   0   0     0
TIMESTAMP 2018.02.11.07.24.23
GATE 1 2 0
0201R
1 0 U
2 0 U

N32G030K6L7 UND  1   0   0     0
TIMESTAMP 2020.12.17.03.28.54
GATE 1 32 0
N32G032K6L7
1 0 U VDD
2 0 U PF0-OSC_IN
3 0 U PF1-OSC_OUT
4 0 U NRST
5 0 U VDDA
6 0 U PA0
7 0 U PA1
8 0 U PA2
9 0 U PA3
10 0 U PA4
11 0 U PA5
12 0 U PA6
13 0 U PA7
14 0 U PB0
15 0 U PB1
16 0 U VSS
17 0 U VDD
18 0 U PA8
19 0 U PA9
20 0 U PA10
21 0 U PA11
22 0 U PA12
23 0 U PA13
24 0 U PA14
25 0 U PA15
26 0 U PB3
27 0 U PB4
28 0 U PB5
29 0 U PB6
30 0 U PB7
31 0 U BOOT0
32 0 U VSS



*PART*       ITEMS



C31          CAP1206          3100  7000    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 83 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
46 -352 0 2 83 10 3 "Default Font"
Value
180 -360 0 2 83 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

C7           CAP1206          1450  7050    0 0 97 10 97 10 4 15 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
48 -172 0 0 83 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
48 -338 0 2 83 10 3 "Default Font"
Value
180 -360 0 2 83 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

J15          CONDIP2_A        4600  7200   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

D4           LED0805          3950  7100   90 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
100 -100 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

U2           AMS1117-3.3      2400  7300    0 0 97 10 97 10 4 1 4 0 0 0
"Default Font"
"Default Font"
200 100 0 4 97 10 0 "Default Font"
REF-DES
200 -500 0 6 97 10 0 "Default Font"
PART-TYPE
200 -600 0 6 97 10 0 "Default Font"
*
200 -700 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SOT223
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1

J6           CONDIP2_A        1150  7200   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R5           R0402            4000  6500   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J8           CONDIP2_A        4600  6850   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

C2           C0603            1850  7050    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
44 -160 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
24 -334 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C11          C0603            3450  7000    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
46 -162 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
38 -328 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

S7           SW_2P            10450 3100    0 0 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

S6           SW_2P            8000  3450   90 0 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
50 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R8           R0402            10050 3550   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R9           R0402            8050  2950   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C37          C0603            10000 3000    0 0 97 10 97 10 4 4 2 0 0 26
"Regular Tahoma"
"Regular Tahoma"
50 -150 0 0 97 10 0 "Regular Tahoma"
REF-DES
210 -40 0 2 97 10 0 "Regular Tahoma"
PART-TYPE
50 -350 0 2 97 10 3 "Regular Tahoma"
Value
150 -340 0 2 97 10 0 "Regular Tahoma"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

J11          CONDIP2_A        7600  3100   90 2 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

D1           LED0805          9200  6200   90 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D2           LED0805          9900  6200   90 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D3           LED0805          10600 6200   90 2 83 10 83 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

S1           SW_2P            7600  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
50 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R6           R0402            7650  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S2           SW_2P            8000  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
50 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R7           R0402            8050  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S3           SW_2P            8400  6050   90 0 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
50 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R10          R0402            8450  5650   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R1           R0402            9250  5500   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R2           R0402            9950  5500   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R3           R0402            10650 5500   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J3           CONDIP2_A        7400  7100   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J7           CONDIP2_A        7400  6800   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J9           CONDIP2_A        7400  6500   90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J13          CONDIP2_A        9200  6550    0 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-140 -10 0 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J14          CONDIP2_A        9900  6550    0 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-140 -10 0 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

J16          CONDIP2_A        10600 6550    0 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-120 -10 0 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

C52          C0603            2550  3100    0 0 100 10 100 10 4 4 2 0 0 26
"Default Font"
"Default Font"
0 -150 0 0 100 10 0 "Default Font"
REF-DES
210 -40 0 2 100 10 0 "Default Font"
PART-TYPE
0 -350 0 2 100 10 3 "Default Font"
Value
150 -340 0 2 100 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C53          C0603            5350  3100    0 0 100 10 100 10 4 4 2 0 0 26
"Default Font"
"Default Font"
0 -150 0 0 100 10 0 "Default Font"
REF-DES
210 -40 0 2 100 10 0 "Default Font"
PART-TYPE
0 -350 0 2 100 10 3 "Default Font"
Value
150 -340 0 2 100 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C50          C0603            2600  4300    0 3 100 10 100 10 4 4 2 0 0 26
"Default Font"
"Default Font"
-150 -400 0 0 100 10 0 "Default Font"
REF-DES
210 -40 0 2 100 10 0 "Default Font"
PART-TYPE
-200 -100 0 2 100 10 3 "Default Font"
Value
150 -340 0 2 100 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C51          C0603            2900  4300    0 3 100 10 100 10 4 4 2 0 0 26
"Default Font"
"Default Font"
-150 -400 0 0 100 10 0 "Default Font"
REF-DES
210 -40 0 2 100 10 0 "Default Font"
PART-TYPE
-200 -100 0 2 100 10 3 "Default Font"
Value
150 -340 0 2 100 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

J1           HEAD2X10         1900  700     0 0 97 10 97 10 4 1 20 0 0 0
"Default Font"
"Default Font"
100 1150 0 4 97 10 0 "Default Font"
REF-DES
150 -40 0 6 97 10 0 "Default Font"
PART-TYPE
150 -140 0 6 97 10 0 "Default Font"
*
150 -240 0 6 97 10 0 "Default Font"
*
"PCB DECAL" HEAD2X10
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1

C6           0402C            1550  4150    0 0 100 10 100 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 70 7 0 "Default Font"
REF-DES
10 -80 0 6 70 7 0 "Default Font"
PART-TYPE
10 -160 0 6 69 7 3 "Regular Tahoma"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C8           0402C            1550  3350    0 0 100 10 100 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 70 7 0 "Default Font"
REF-DES
10 -80 0 6 70 7 0 "Default Font"
PART-TYPE
10 -160 0 6 69 7 3 "Regular Tahoma"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

Y2           CRYSTAL_2PIN     1700  4000   90 2 97 10 97 10 4 2 2 0 0 2
"Default Font"
"Default Font"
250 150 90 4 97 10 0 "Default Font"
REF-DES
260 -120 0 6 97 10 0 "Default Font"
PART-TYPE
200 -250 90 5 97 10 1 "Default Font"
Value
240 -396 0 6 97 10 0 "Default Font"
*
"Value" 8MHz
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1

R22          0201R            1600  2950    0 3 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 100 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

R23          0201R            1400  4550    0 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 100 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

U3           N32G030K6L7      3500  2800    0 0 97 10 97 10 4 2 32 0 0 0
"Default Font"
"Default Font"
750 750 0 0 97 10 0 "Default Font"
REF-DES
550 700 0 2 97 10 0 "Default Font"
PART-TYPE
1900 -140 0 2 97 10 0 "Default Font"
*
1900 -240 0 2 97 10 0 "Default Font"
*
"VALUE" N32G4XXK
"PCB DECAL" QFP32
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1

R13          R0402            7400  1350    0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" NC/4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R14          R0402            7400  1150    0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" NC/4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R16          R0402            7400  950     0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" NC/4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R21          R0402            7400  750     0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 69 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 69 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" NC/4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J2           HEAD2X10         4800  700     0 0 97 10 97 10 4 1 20 0 0 0
"Default Font"
"Default Font"
100 1150 0 4 97 10 0 "Default Font"
REF-DES
150 -40 0 6 97 10 0 "Default Font"
PART-TYPE
150 -140 0 6 97 10 0 "Default Font"
*
150 -240 0 6 97 10 0 "Default Font"
*
"PCB DECAL" HEAD2X10
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 1650   6250   0 0 0
@@@O1    GND $GND_SYMS 3950   6200   0 0 0
@@@O2    GND $GND_SYMS 3200   6200   0 0 0
@@@O3    GND $GND_SYMS 2200   6800   0 0 0
@@@O4    VDD_MCU $PWR_SYMS 4900   7200   90 1 0
@@@O5    5V $PWR_SYMS 900    7250   0 0 0
@@@O6    VDD_LINK $PWR_SYMS 4900   6850   90 1 0
@@@O7    GND $GND_SYMS 10900  2800   0 0 0
@@@O8    GND $GND_SYMS 10000  2500   0 0 0
@@@O9    VDD_MCU $PWR_SYMS 10000  3750   0 0 0
@@@O10   NRST $OSR_SYMS 9400   3100   0 1 1
@@@O11   VDD_MCU $PWR_SYMS 8000   3800   0 0 0
@@@O12   GND $GND_SYMS 8000   2600   0 0 0
@@@O13   PA0_WKUP $OSR_SYMS 7300   3100   0 0 0
@@@O14   PB1 $OSR_SYMS 9200   6850   90 2 0
@@@O15   PB6 $OSR_SYMS 9900   6850   90 2 0
@@@O16   PB7 $OSR_SYMS 10600  6850   90 2 0
@@@O17   GND $GND_SYMS 9200   5150   0 0 0
@@@O18   GND $GND_SYMS 9900   5150   0 0 0
@@@O19   GND $GND_SYMS 10600  5150   0 0 0
@@@O20   GND $GND_SYMS 7600   5200   0 0 0
@@@O21   GND $GND_SYMS 8000   5200   0 0 0
@@@O22   GND $GND_SYMS 8400   5200   0 0 0
@@@O23   PA4 $OSR_SYMS 7150   6500   0 0 0
@@@O24   PA5 $OSR_SYMS 7150   6800   0 0 0
@@@O25   PA6 $OSR_SYMS 7150   7100   0 0 0
@@@O26   PA0_WKUP $OSR_SYMS 1400   1400   0 0 0
@@@O27   PA1 $OSR_SYMS 2500   1400   0 1 0
@@@O28   PA2 $OSR_SYMS 1400   1300   0 0 0
@@@O29   PA3 $OSR_SYMS 2500   1300   0 1 0
@@@O30   PA4 $OSR_SYMS 1400   1200   0 0 0
@@@O31   PA5 $OSR_SYMS 2500   1200   0 1 0
@@@O32   PA6 $OSR_SYMS 1400   1100   0 0 0
@@@O33   PA7 $OSR_SYMS 2500   1100   0 1 0
@@@O34   PB0 $OSR_SYMS 1400   1000   0 0 0
@@@O35   PA8 $OSR_SYMS 4500   1600   0 0 0
@@@O36   MCU_PA10/RX1 $OSR_SYMS 4500   1500   0 2 0
@@@O37   MCU_PA13/SWDIO $OSR_SYMS 5300   1300   0 3 0
@@@O38   MCU_PA9/TX1 $OSR_SYMS 5300   1500   0 3 0
@@@O39   PA15 $OSR_SYMS 5300   1200   0 1 0
@@@O40   PB4 $OSR_SYMS 5300   1100   0 3 0
@@@O41   MCU_PA14/SWDCK $OSR_SYMS 4500   1300   0 2 0
@@@O42   PB3 $OSR_SYMS 4500   1200   0 2 0
@@@O43   PB5 $OSR_SYMS 4500   1100   0 2 0
@@@O44   PB6 $OSR_SYMS 5300   1000   0 3 0
@@@O45   VDD_MCU $PWR_SYMS 5400   900    90 1 0
@@@O46   VDD_MCU $PWR_SYMS 4500   900    90 0 0
@@@O47   PB1 $OSR_SYMS 2500   1000   0 1 0
@@@O48   VDD_MCU $PWR_SYMS 2400   1700   90 1 0
@@@O49   VDD_MCU $PWR_SYMS 1500   1700   90 0 0
@@@O50   GND $GND_SYMS 1500   800    90 1 0
@@@O51   GND $GND_SYMS 2400   900    90 0 0
@@@O52   GND $GND_SYMS 2400   800    90 0 0
@@@O53   NRST $OSR_SYMS 3300   3600   0 0 0
@@@O54   PA0_WKUP $OSR_SYMS 3300   3400   0 0 0
@@@O55   PA4 $OSR_SYMS 4000   2500   90 0 0
@@@O56   PA5 $OSR_SYMS 4100   2500   90 0 0
@@@O57   PA6 $OSR_SYMS 4200   2500   90 0 0
@@@O58   PA7 $OSR_SYMS 4300   2500   90 0 0
@@@O59   PB0 $OSR_SYMS 4400   2500   90 0 0
@@@O60   PB1 $OSR_SYMS 4500   2500   90 0 0
@@@O61   PA12 $OSR_SYMS 5300   3700   0 1 0
@@@O62   MCU_PA10/RX1 $OSR_SYMS 5300   3500   0 1 0
@@@O63   MCU_PA9/TX1 $OSR_SYMS 5300   3400   0 1 0
@@@O64   PA8 $OSR_SYMS 5300   3300   0 1 0
@@@O65   PA11 $OSR_SYMS 5300   3600   0 1 0
@@@O66   MCU_PA13/SWDIO $OSR_SYMS 5300   3800   0 1 0
@@@O67   PA15 $OSR_SYMS 4600   4500   90 2 0
@@@O68   MCU_PA14/SWDCK $OSR_SYMS 5300   3900   0 3 0
@@@O69   PB3 $OSR_SYMS 4500   4500   90 2 0
@@@O70   BOOT0 $OSR_SYMS 4000   4500   90 2 0
@@@O71   PB5 $OSR_SYMS 4300   4500   90 2 0
@@@O72   PB4 $OSR_SYMS 4400   4500   90 2 0
@@@O73   PF0 $OSR_SYMS 2500   1500   0 1 0
@@@O74   PA12 $OSR_SYMS 5300   1400   0 3 0
@@@O75   PA11 $OSR_SYMS 4500   1400   0 2 0
@@@O76   GND $GND_SYMS 5350   1600   90 0 0
@@@O77   GND $GND_SYMS 5350   1700   90 0 0
@@@O78   GND $GND_SYMS 4550   1700   90 1 0
@@@O79   VDD_MCU $PWR_SYMS 5400   800    90 1 0
@@@O80   VDD_MCU $PWR_SYMS 4500   800    90 0 0
@@@O81   PF1 $OSR_SYMS 1400   1500   0 0 0
@@@O82   GND $GND_SYMS 1500   900    90 1 0
@@@O83   GND $GND_SYMS 1500   1600   90 1 0
@@@O84   BOOT0 $OSR_SYMS 2500   1600   0 1 0
@@@O85   VDD_MCU $PWR_SYMS 3200   5100   0 0 0
@@@O86   VDD_MCU $PWR_SYMS 2450   3200   90 0 0
@@@O87   VDD_MCU $PWR_SYMS 5550   3200   90 1 0
@@@O88   GND $GND_SYMS 2600   4100   0 0 0
@@@O89   GND $GND_SYMS 2550   2550   0 0 0
@@@O90   GND $GND_SYMS 5350   2550   0 0 0
@@@O91   PB6 $OSR_SYMS 4200   4500   90 2 0
@@@O92   PB7 $OSR_SYMS 4100   4500   90 2 0
@@@O93   PA3 $OSR_SYMS 3900   2500   90 0 0
@@@O94   PA1 $OSR_SYMS 3300   3300   0 0 0
@@@O95   PA2 $OSR_SYMS 3300   3200   0 0 0
@@@O96   PB7 $OSR_SYMS 4500   1000   0 2 0
@@@O97   GND $GND_SYMS 1350   3750   90 1 0
@@@O98   PF1 $OSR_SYMS 1250   2950   0 0 0
@@@O99   PF0 $OSR_SYMS 1250   4550   0 0 0
@@@O100  GND $GND_SYMS 3750   4650   0 0 0
@@@O101  GND $GND_SYMS 4600   2550   0 0 0
@@@O102  PA6 $OSR_SYMS 7200   1400   0 0 0
@@@O103  PA7 $OSR_SYMS 7200   1200   0 0 0
@@@O104  PB6 $OSR_SYMS 7200   1000   0 0 0
@@@O105  PB7 $OSR_SYMS 7200   800    0 0 0
@@@O106  VDD_MCU $PWR_SYMS 8300   1500   0 0 0

*TIEDOTS*



@@@D0    1450   7200  
@@@D1    3100   7200  
@@@D2    3950   7200  
@@@D3    4300   7200  
@@@D4    1650   6400  
@@@D5    1850   7200  
@@@D6    3200   6400  
@@@D7    3450   7200  
@@@D8    10000  3100  
@@@D9    10000  3100  
@@@D10   8000   3100  
@@@D11   3000   7200  
@@@D12   3200   4900  
@@@D13   2600   4200  
@@@D14   5350   3200  
@@@D15   2900   4900  
@@@D16   1400   3750  
@@@D17   1700   4150  
@@@D18   1700   3350  
@@@D19   2550   3200  
@@@D20   1700   4150  
@@@D21   1700   3350  
@@@D22   7900   1000  
@@@D23   7900   1200  
@@@D24   7900   1400  

*CONNECTION*


*SIGNAL* PA0_WKUP 0 0
J11.1        @@@O13       2 0
7400   3100  
7300   3100  
J1.7         @@@O26       2 0
1700   1400  
1400   1400  
U3.6         @@@O54       2 0
3300   3400  
3300   3400  

*SIGNAL* PA1 0 0
J1.8         @@@O27       2 0
2300   1400  
2500   1400  
U3.7         @@@O94       2 0
3300   3300  
3300   3300  

*SIGNAL* PA4 0 0
J9.2         @@@O23       2 0
7200   6500  
7150   6500  
J1.11        @@@O30       2 0
1700   1200  
1400   1200  
U3.10        @@@O55       2 0
4000   2600  
4000   2500  

*SIGNAL* PA5 0 0
J7.2         @@@O24       2 0
7200   6800  
7150   6800  
J1.12        @@@O31       2 0
2300   1200  
2500   1200  
U3.11        @@@O56       2 0
4100   2600  
4100   2500  

*SIGNAL* PA6 0 0
J3.2         @@@O25       2 0
7200   7100  
7150   7100  
J1.13        @@@O32       2 0
1700   1100  
1400   1100  
U3.12        @@@O57       2 0
4200   2600  
4200   2500  
R13.1        @@@O102      2 0
7300   1400  
7200   1400  

*SIGNAL* PA7 0 0
J1.14        @@@O33       2 0
2300   1100  
2500   1100  
U3.13        @@@O58       2 0
4300   2600  
4300   2500  
R14.1        @@@O103      2 0
7300   1200  
7200   1200  

*SIGNAL* MCU_PA10/RX1 0 0
J2.5         @@@O36       2 0
4600   1500  
4500   1500  
U3.20        @@@O62       2 0
5200   3500  
5300   3500  

*SIGNAL* MCU_PA13/SWDIO 0 0
J2.10        @@@O37       2 0
5200   1300  
5300   1300  
U3.23        @@@O66       2 0
5200   3800  
5300   3800  

*SIGNAL* MCU_PA9/TX1 0 0
J2.6         @@@O38       2 0
5200   1500  
5300   1500  
U3.19        @@@O63       2 0
5200   3400  
5300   3400  

*SIGNAL* MCU_PA14/SWDCK 0 0
J2.9         @@@O41       2 0
4600   1300  
4500   1300  
U3.24        @@@O68       2 0
5200   3900  
5300   3900  

*SIGNAL* PB6 0 0
J14.1        @@@O15       2 0
9900   6750  
9900   6850  
J2.16        @@@O44       2 0
5200   1000  
5300   1000  
U3.29        @@@O91       2 0
4200   4500  
4200   4500  
R16.1        @@@O104      2 0
7300   1000  
7200   1000  

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
@@@O4        J15.1        2 0
4900   7200  
4800   7200  
R8.1         @@@O9        2 0
10000  3650  
10000  3750  
@@@O11       S6.2         2 0
8000   3800  
8000   3650  
J2.18        @@@O45       2 0
5200   900   
5400   900   
J2.17        @@@O46       2 0
4600   900   
4500   900   
J1.2         @@@O48       2 0
2300   1700  
2400   1700  
J1.1         @@@O49       2 0
1700   1700  
1500   1700  
J2.20        @@@O79       2 0
5200   800   
5400   800   
J2.19        @@@O80       2 0
4600   800   
4500   800   
@@@D12       U3.1         3 0
3200   4900  
3200   3900  
3300   3900  
U3.5         @@@D19       3 0
3300   3500  
2550   3500  
2550   3200  
U3.17        @@@D14       2 0
5200   3200  
5350   3200  
C51.2        @@@D15       2 0
2900   4800  
2900   4900  
@@@D12       @@@O85       2 0
3200   4900  
3200   5100  
@@@D12       @@@D15       2 0
3200   4900  
2900   4900  
@@@O86       @@@D19       2 0
2450   3200  
2550   3200  
C53.1        @@@D14       2 0
5350   3100  
5350   3200  
@@@D14       @@@O87       2 0
5350   3200  
5550   3200  
@@@D15       C50.2        3 0
2900   4900  
2600   4900  
2600   4800  
@@@D19       C52.1        2 0
2550   3200  
2550   3100  
R21.2        @@@D22       3 0
7700   800   
7900   800   
7900   1000  
R14.2        @@@D23       2 0
7700   1200  
7900   1200  
@@@D22       R16.2        2 0
7900   1000  
7700   1000  
@@@D23       @@@D22       2 0
7900   1200  
7900   1000  
R13.2        @@@D24       2 0
7700   1400  
7900   1400  
@@@O106      @@@D24       3 0
8300   1500  
8300   1400  
7900   1400  
@@@D24       @@@D23       2 0
7900   1400  
7900   1200  

*SIGNAL* PB1 0 0
J13.1        @@@O14       2 0
9200   6750  
9200   6850  
J1.16        @@@O47       2 0
2300   1000  
2500   1000  
U3.15        @@@O60       2 0
4500   2600  
4500   2500  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        @@@D4        2 0
1650   6250  
1650   6400  
@@@O1        R5.2         2 0
3950   6200  
3950   6200  
C31.2        @@@D6        3 0
3100   6500  
3100   6400  
3200   6400  
U2.1         @@@O3        2 0
2200   7000  
2200   6800  
@@@D4        C7.2         3 0
1650   6400  
1450   6400  
1450   6550  
@@@D4        C2.2         3 0
1650   6400  
1850   6400  
1850   6550  
@@@D6        @@@O2        2 0
3200   6400  
3200   6200  
@@@D6        C11.2        3 0
3200   6400  
3450   6400  
3450   6500  
@@@O7        S7.2         3 0
10900  2800  
10900  3100  
10650  3100  
C37.2        @@@O8        2 0
10000  2500  
10000  2500  
R9.2         @@@O12       2 0
8000   2650  
8000   2600  
R1.2         @@@O17       2 0
9200   5200  
9200   5150  
R2.2         @@@O18       2 0
9900   5200  
9900   5150  
R3.2         @@@O19       2 0
10600  5200  
10600  5150  
R6.2         @@@O20       2 0
7600   5350  
7600   5200  
R7.2         @@@O21       2 0
8000   5350  
8000   5200  
R10.2        @@@O22       2 0
8400   5350  
8400   5200  
J1.19        @@@O50       2 0
1700   800   
1500   800   
J1.18        @@@O51       2 0
2300   900   
2400   900   
J1.20        @@@O52       2 0
2300   800   
2400   800   
J2.4         @@@O76       2 0
5200   1600  
5350   1600  
J2.2         @@@O77       2 0
5200   1700  
5350   1700  
J2.1         @@@O78       2 0
4600   1700  
4550   1700  
J1.17        @@@O82       2 0
1700   900   
1500   900   
J1.3         @@@O83       2 0
1700   1600  
1500   1600  
C51.1        @@@D13       3 0
2900   4300  
2900   4200  
2600   4200  
@@@D13       C50.1        2 0
2600   4200  
2600   4300  
@@@D13       @@@O88       2 0
2600   4200  
2600   4100  
C52.2        @@@O89       2 0
2550   2600  
2550   2550  
C53.2        @@@O90       2 0
5350   2600  
5350   2550  
@@@O97       @@@D16       2 0
1350   3750  
1400   3750  
C6.1         @@@D16       3 0
1450   4150  
1400   4150  
1400   3750  
@@@D16       C8.1         3 0
1400   3750  
1400   3350  
1450   3350  
U3.32        @@@O100      3 0
3900   4500  
3900   4650  
3750   4650  
U3.16        @@@O101      2 0
4600   2600  
4600   2550  

*SIGNAL* $$$7556 64 0
Y2.1         @@@D17       2 0
1700   4048  
1700   4150  
C6.2         @@@D17       2 0
1650   4150  
1700   4150  
@@@D17       @@@D20       2 0
1700   4150  
1700   4150  
U3.2         @@@D20       4 0
3300   3800  
2100   3800  
2100   4150  
1700   4150  
@@@D20       R23.2        2 0
1700   4150  
1700   4550  

*SIGNAL* NRST 0 0
S7.1         @@@D8        2 0
10250  3100  
10000  3100  
@@@D9        C37.1        2 0
10000  3100  
10000  3000  
@@@D8        @@@D9        2 0
10000  3100  
10000  3100  
@@@O10       @@@D9        2 0
9400   3100  
10000  3100  
R8.2         @@@D8        2 0
10000  3250  
10000  3100  
U3.4         @@@O53       2 0
3300   3600  
3300   3600  

*SIGNAL* $$$7560 64 0
Y2.2         @@@D18       2 0
1700   3448  
1700   3350  
C8.2         @@@D21       2 0
1650   3350  
1700   3350  
R22.1        @@@D18       2 0
1700   2950  
1700   3350  
U3.3         @@@D21       4 0
3300   3700  
2100   3700  
2100   3350  
1700   3350  
@@@D21       @@@D18       2 0
1700   3350  
1700   3350  

*SIGNAL* BOOT0 0 0
U3.31        @@@O70       2 0
4000   4500  
4000   4500  
J1.4         @@@O84       2 0
2300   1600  
2500   1600  

*SIGNAL* PB7 0 0
J16.1        @@@O16       2 0
10600  6750  
10600  6850  
U3.30        @@@O92       2 0
4100   4500  
4100   4500  
J2.15        @@@O96       2 0
4600   1000  
4500   1000  
R21.1        @@@O105      2 0
7300   800   
7200   800   

*SIGNAL* $$$16580 64 0
U2.3         @@@D5        2 0
2200   7200  
1850   7200  
@@@D0        C7.1         2 0
1450   7200  
1450   7050  
@@@D0        J6.1         2 0
1450   7200  
1350   7200  
C2.1         @@@D5        2 0
1850   7050  
1850   7200  
@@@D5        @@@D0        2 0
1850   7200  
1450   7200  

*SIGNAL* $$$18572 64 0
@@@D1        @@@D7        2 0
3100   7200  
3450   7200  
@@@D1        @@@D11       2 0
3100   7200  
3000   7200  
C31.1        @@@D1        2 0
3100   7000  
3100   7200  
D4.2         @@@D2        2 0
3950   7100  
3950   7200  
@@@D2        @@@D3        2 0
3950   7200  
4300   7200  
J8.2         @@@D3        3 0
4400   6850  
4300   6850  
4300   7200  
@@@D3        J15.2        2 0
4300   7200  
4400   7200  
C11.1        @@@D7        2 0
3450   7000  
3450   7200  
@@@D7        @@@D2        2 0
3450   7200  
3950   7200  
U2.2         @@@D11       2 0
3000   7000  
3000   7200  
@@@D11       U2.4         2 0
3000   7200  
3000   7200  

*SIGNAL* 5V 0 0
J6.2         @@@O5        3 0
950    7200  
900    7200  
900    7250  

*SIGNAL* $$$23084 64 0
R5.1         D4.1         2 0
3950   6600  
3950   6600  

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J8.1         @@@O6        2 0
4800   6850  
4900   6850  

*SIGNAL* $$$13829 64 0
S6.1         @@@D10       2 0
8000   3250  
8000   3100  
R9.1         @@@D10       2 0
8000   3050  
8000   3100  
@@@D10       J11.2        2 0
8000   3100  
7800   3100  

*SIGNAL* $$$2339 64 0
R1.1         D1.1         2 0
9200   5600  
9200   5700  

*SIGNAL* $$$2340 64 0
R2.1         D2.1         2 0
9900   5600  
9900   5700  

*SIGNAL* $$$10873 64 0
R3.1         D3.1         2 0
10600  5600  
10600  5700  

*SIGNAL* $$$7234 64 0
D1.2         J13.2        2 0
9200   6200  
9200   6350  

*SIGNAL* $$$7238 64 0
J16.2        D3.2         2 0
10600  6350  
10600  6200  

*SIGNAL* $$$13605 64 0
R6.1         S1.1         2 0
7600   5750  
7600   5850  

*SIGNAL* $$$13607 64 0
S2.1         R7.1         2 0
8000   5850  
8000   5750  

*SIGNAL* $$$13609 64 0
S3.1         R10.1        2 0
8400   5850  
8400   5750  

*SIGNAL* $$$6888 64 0
S1.2         J9.1         2 0
7600   6250  
7600   6500  

*SIGNAL* $$$6886 64 0
S2.2         J7.1         3 0
8000   6250  
8000   6800  
7600   6800  

*SIGNAL* $$$6884 64 0
S3.2         J3.1         3 0
8400   6250  
8400   7100  
7600   7100  

*SIGNAL* $$$7236 64 0
D2.2         J14.2        2 0
9900   6200  
9900   6350  

*SIGNAL* PA2 0 0
J1.9         @@@O28       2 0
1700   1300  
1400   1300  
U3.8         @@@O95       2 0
3300   3200  
3300   3200  

*SIGNAL* PA3 0 0
J1.10        @@@O29       2 0
2300   1300  
2500   1300  
U3.9         @@@O93       2 0
3900   2600  
3900   2500  

*SIGNAL* PB0 0 0
J1.15        @@@O34       2 0
1700   1000  
1400   1000  
U3.14        @@@O59       2 0
4400   2600  
4400   2500  

*SIGNAL* PA8 0 0
J2.3         @@@O35       2 0
4600   1600  
4500   1600  
U3.18        @@@O64       2 0
5200   3300  
5300   3300  

*SIGNAL* PA15 0 0
J2.12        @@@O39       2 0
5200   1200  
5300   1200  
U3.25        @@@O67       2 0
4600   4500  
4600   4500  

*SIGNAL* PB4 0 0
J2.14        @@@O40       2 0
5200   1100  
5300   1100  
U3.27        @@@O72       2 0
4400   4500  
4400   4500  

*SIGNAL* PB3 0 0
J2.11        @@@O42       2 0
4600   1200  
4500   1200  
U3.26        @@@O69       2 0
4500   4500  
4500   4500  

*SIGNAL* PB5 0 0
J2.13        @@@O43       2 0
4600   1100  
4500   1100  
U3.28        @@@O71       2 0
4300   4500  
4300   4500  

*SIGNAL* PF0 0 0
J1.6         @@@O73       2 0
2300   1500  
2500   1500  
R23.1        @@@O99       2 0
1300   4550  
1250   4550  

*SIGNAL* PA12 0 0
U3.22        @@@O61       2 0
5200   3700  
5300   3700  
J2.8         @@@O74       2 0
5200   1400  
5300   1400  

*SIGNAL* PA11 0 0
U3.21        @@@O65       2 0
5200   3600  
5300   3600  
J2.7         @@@O75       2 0
4600   1400  
4500   1400  

*SIGNAL* PF1 0 0
J1.5         @@@O81       2 0
1700   1500  
1400   1500  
R22.2        @@@O98       2 0
1300   2950  
1250   2950  

*NETNAMES*



VDD_MCU      @@@O4        400    50     0 6 0      0      0 0 -1 10 97 "Regular Tahoma"
5V           @@@O5        0      250    0 4 0      0      0 0 -1 10 97 "Regular Tahoma"
VDD_LINK     @@@O6        400    50     0 6 0      0      0 0 -1 10 97 "Regular Tahoma"
VDD_MCU      @@@O9        0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
NRST         @@@O10       -550   -50    0 0 0      0      0 2 -1 10 97 "Default Font"
VDD_MCU      @@@O11       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
PA0_WKUP     @@@O13       -350   -50    0 1 0      0      0 3 -1 10 97 "Default Font"
PB1          @@@O14       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB6          @@@O15       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB7          @@@O16       50     500    90 2 0      0      90 3 -1 10 97 "Default Font"
PA4          @@@O23       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O24       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O25       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA0_WKUP     @@@O26       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA1          @@@O27       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA2          @@@O28       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA3          @@@O29       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA4          @@@O30       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O31       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O32       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA7          @@@O33       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB0          @@@O34       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA8          @@@O35       -350   0      0 1 0      0      0 3 -1 10 97 "Default Font"
MCU_PA10/RX1 @@@O36       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O37       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O38       350    50     0 2 0      0      0 3 -1 10 97 "Default Font"
PA15         @@@O39       350    -50    0 0 0      0      0 3 -1 10 97 "Default Font"
PB4          @@@O40       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O41       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB3          @@@O42       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB5          @@@O43       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB6          @@@O44       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O46       -450   0      0 6 0      0      0 0 -1 10 100 "Default Font"
VDD_MCU      @@@O45       450    -50    0 5 0      0      0 0 -1 10 100 "Default Font"
PB1          @@@O47       350    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O48       400    50     0 7 0      0      0 0 -1 10 100 "Default Font"
VDD_MCU      @@@O49       -400   50     0 6 0      0      0 0 -1 10 100 "Default Font"
NRST         @@@O53       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA0_WKUP     @@@O54       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA4          @@@O55       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O56       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O57       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA7          @@@O58       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB0          @@@O59       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB1          @@@O60       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA12         @@@O61       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA10/RX1 @@@O62       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O63       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA8          @@@O64       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA11         @@@O65       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O66       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA15         @@@O67       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O68       350    50     0 2 0      0      0 3 -1 10 97 "Default Font"
PB3          @@@O69       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
BOOT0        @@@O70       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB5          @@@O71       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB4          @@@O72       0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PF0          @@@O73       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA12         @@@O74       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PA11         @@@O75       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O80       -450   0      0 6 0      0      0 0 -1 10 100 "Default Font"
VDD_MCU      @@@O79       450    -50    0 5 0      0      0 0 -1 10 100 "Default Font"
PF1          @@@O81       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
BOOT0        @@@O84       360    0      0 0 0      0      0 3 -1 10 100 "Default Font"
VDD_MCU      @@@O85       0      250    0 4 0      0      0 0 -1 10 100 "Default Font"
VDD_MCU      @@@O86       -400   0      0 4 0      0      0 0 -1 10 100 "Default Font"
VDD_MCU      @@@O87       400    -50    0 4 0      0      0 0 -1 10 100 "Default Font"
PB6          @@@O91       0      360    90 0 0      0      90 3 -1 10 100 "Default Font"
PB7          @@@O92       0      360    90 0 0      0      90 3 -1 10 100 "Default Font"
PA3          @@@O93       -50    -350   90 3 0      0      90 3 -1 10 100 "Default Font"
PA1          @@@O94       -360   0      0 1 0      0      0 3 -1 10 100 "Default Font"
PA2          @@@O95       -360   0      0 1 0      0      0 3 -1 10 100 "Default Font"
PB7          @@@O96       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PF1          @@@O98       -360   0      0 1 0      0      0 3 -1 10 100 "Default Font"
PF0          @@@O99       -360   0      0 1 0      0      0 3 -1 10 100 "Default Font"
PA6          @@@O102      -360   0      0 1 0      0      0 3 -1 10 100 "Default Font"
PA7          @@@O103      -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
PB6          @@@O104      -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
PB7          @@@O105      -360   0      0 1 0      0      0 3 -1 10 97 "Regular Tahoma"
VDD_MCU      @@@O106      0      250    0 4 0      0      0 0 -1 10 100 "Default Font"

*END*     OF ASCII OUTPUT FILE