1、功能说明
    1、TIM5周期触发DAC 输出三角波数据，在PA4输出三角波形
2、使用环境
    软件开发环境：  KEIL MDK-ARM V5.26.2.0
    硬件环境：      基于N32G43XRL-STB V1.0开发
3、使用说明
    系统配置；
        1、时钟源：
            HSE=8M,PLL=108M,AHB=108M,APB1=27M,APB2=54M,DAC CLK=27M,TIM5 CLK=54M
        2、端口配置：
            PA4选择为模拟功能DAC CH1 OUT
        3、TIM：
            TIM5 更新事件作为触发输出给DAC
        4、DAC：
            DAC选择TIM5 TRGO信号触发，使能三角波幅度2048，基值0X100
    使用方法：
        1、编译后打开调试模式，利用示波器观察PA4输出波形
        2、全速运行时，TIM5的每个周期触发PA4的一个数据，形成三角波
4、注意事项
    无



1. Function description
     1. TIM5 periodically triggers DAC to output triangular wave data, and outputs triangular waveform in PA4
2. Use environment
     Software development environment: KEIL MDK-ARM V5.26.2.0
     Hardware environment: Developed based on the development board N32G43XRL-STB V1.0
3. Instructions for use
     System Configuration;
         1. Clock source:
            HSE=8M,PLL=108M,AHB=108M,APB1=27M,APB2=54M,DAC CLK=27M,TIM5 CLK=54M
         2. Port configuration:
             PA4 is selected as analog function, DAC CH1 OUT
         3. TIM:
             TIM5 update event as trigger output to DAC
         4. DAC:
             DAC selects TIM5 TRGO signal trigger, enables triangle wave amplitude 2048, base value 0X100
     Instructions:
         1. Open the debug mode after compiling, and use the oscilloscope to observe the output waveform of the PA4
         2. When running at full speed, each cycle of TIM5 triggers a data of PA4 to form a triangular wave
4. Attention
   None