1、功能说明

	1、SPI DMA 单线发送和单线接收数据

2、使用环境

	/* 硬件环境：工程对应的开发硬件平台 */
	开发板：N32L43XM-STB N32L40XM-STB V1.1

3、使用说明
	
	/* 描述相关模块配置方法；例如:时钟，I/O等 */
	1、SystemClock：108MHz
	2、GPIO：SPI1: NSS--PA4  <--> SPI2--PB12
		SPI1: SCK--PA5  <--> SPI2: SCK--PB13
		SPI1: MOSI--PA7 <--> SPI2: MISO--PB14
	3、DMA：DMA_CH4 通道发送数据，DMA_CH1 通道接收数据

	/* 描述Demo的测试步骤和现象 */
	1、.编译后下载程序复位运行；
	2、SPI1 通过 DMA 发送数据，SPI2 通过 DMA 接收数据，数据传输完成后，查看 TransferStatus 状态为 PASSED；

4、注意事项
	“单线”数据线在主设备端为MOSI引脚，在从设备端为MISO引脚



1. Function description

	1. SPI DMA single-wire sending and single-wire receiving data

2. Use environment

	/* Hardware environment: the development hardware platform corresponding to the project */
	Development board: N32L43XM-STB N32L40XM-STB V1.1

3. Instructions for use

	/* Describe related module configuration methods; for example: clock, I/O, etc. */
	1. SystemClock: 108MHz
	2. GPIO: SPI1: NSS--PA4 <--> SPI2--PB12
	              SPI1: SCK--PA5 <--> SPI2: SCK--PB13
	              SPI1: MOSI--PA7 <--> SPI2: MISO--PB14
	3. DMA: DMA_CH4 channel sends data, DMA_CH1 channel receives data

	/* Describe the test steps and phenomena of the Demo */
	1. After compiling, download the program to reset and run;
	2. SPI1 sends data through DMA, and SPI2 receives data through DMA. After the data transfer is completed, check that the TransferStatus status is PASSED;

4. Attention
	The "single wire" data lines are MOSI pins on the master side and MISO pins on the slave side