1、功能说明

	该测例演示了USARTy（同步模式）与SPIy间通过查询检测标识实现的基础通信。
USARTy和SPIy可以是USART1和SPI1、USART3和SPI1或USART2和SPI2。
    首先，通过TXC检测标志，USARTy发送TxBuffer1数据至SPIy，而SPIy接收数据，
则查询RNE检测标志，接收的数据存至RxBuffer1。
    随后，SPIy通过查询TE检测标志，发送TxBuffer2数据至USARTy。USARTy则利用
RXDNE检测标志接收数据，将其存入RxBuffer2。
    最后，分别比较两组收、发数据，比较结果存入TransferStatus1变量
和TransferStatus2变量。


2、使用环境

	软件开发环境：KEIL MDK-ARM Professional Version 5.26.2.0

        硬件环境：最小系统板N32G43XRL-STB V1.0


3、使用说明
	
	系统时钟配置如下：
    - 时钟源 = HSE + PLL
    - 系统时钟 = 108MHz
    
    USART配置如下：
    - 波特率 = 115200 baud
    - 字长 = 8数据位
    - 1停止位
    - 校验控制禁用
    - 硬件流控制禁用（RTS和CTS信号）
    - 接收器和发送器使能
    - 时钟使能
    - 时钟极性：不对外发送时保持高电平
    - 时钟相位：在第二个时钟边沿采样第一个数据
    - 最后一位时钟脉冲：最后一位数据的时钟脉冲从CK输出
    
    SPI配置如下：
    - 方向 = “双线双向”模式
    - 模式 = 从模式
    - 数据大小 = 8位数据帧
    - CPOL = 空闲状态时，时钟保持高电平
    - CPHA = 数据采样从第二个时钟边沿开始
    - NSS = 启用软件从设备管理
    - 第1位 = 第1位为LSB
    
    
    USART引脚连接如下：    
    - USART1_Tx.PA9    <------->   SPI1_MOSI.PA7
    - USART1_Rx.PA10   <------->   SPI1_MISO.PA6
    - USART1_Clk.PA8   <------->   SPI1_SCK.PA5     
    或
    - USART3_Tx.PC10   <------->   SPI1_MOSI.PD6
    - USART3_Rx.PC11   <------->   SPI1_MISO.PD5
    - USART3_Clk.PC12  <------->   SPI1_SCK.PD4
    或
    - USART2_Tx.PA2    <------->   SPI2_MOSI.PB15
    - USART2_Rx.PA3    <------->   SPI2_MISO.PB14
    - USART2_Clk.PA4   <------->   SPI2_SCK.PB13

    
    测试步骤与现象：
    - Demo在KEIL环境下编译后，下载至MCU
    - 复位运行，依次查看变量TransferStatus1和TransferStatus2，其中，
      PASSED为测试通过，FAILED为测试异常


4、注意事项

1. Function description

This test example demonstrates the basic communication between USARTy (synchronous mode) and SPIy by querying the detection identifier.
USARTy and SPIy can be USART1 and SPI1, USART3 and SPI1 or USART2 and SPI2.
    First, through the TXC detection flag, USARTy sends TxBuffer1 data to SPIy, and SPIy receives the data, it queries the RNE detection flag, 
	and the received data is stored in RxBuffer1.
    Subsequently, SPIy sends TxBuffer2 data to USARTy by querying the TE detection flag. USARTy uses the RXDNE detection flag to receive 
	data and stores it in RxBuffer2.
    Finally, compare the two groups of receiving and sending data respectively, and store the comparison results in the TransferStatus1 
	variable and the TransferStatus2 variable.


2. Use environment

    Software development environment: KEIL MDK-ARM Professional Version 5.26.2.0

    Hardware environment: minimum system board N32G43XRL-STB V1.0


3. Instructions for use

The system clock configuration is as follows:
    -Clock source = HSE + PLL
    -System clock = 108MHz
    
    The USART configuration is as follows:
    -Baud rate = 115200 baud
    -Word length = 8 data bits
    -1 stop bit
    -Verification control disabled
    -Hardware flow control disabled (RTS and CTS signals)
    -Receiver and transmitter enable
    -Clock enable
    -Clock polarity: keep high level when not sending out
    -Clock phase: sample the first data on the second clock edge
    -The last clock pulse: the clock pulse of the last data is output from CK
    
    The SPI configuration is as follows:
    -Direction = "Two-wire two-way" mode
    -Mode = slave mode
    -Data size = 8-bit data frame
    -CPOL = In idle state, the clock stays high
    -CPHA = data sampling starts from the second clock edge
    -NSS = Enable software management from the device
    -1st bit = 1st bit is LSB
    
    
    The USART pin connections are as follows:
    -USART1_Tx.PA9 <-------> SPI1_MOSI.PA7
    -USART1_Rx.PA10 <-------> SPI1_MISO.PA6
    -USART1_Clk.PA8 <-------> SPI1_SCK.PA5
    or
    -USART3_Tx.PC10 <-------> SPI1_MOSI.PD6
    -USART3_Rx.PC11 <-------> SPI1_MISO.PD5
    -USART3_Clk.PC12 <-------> SPI1_SCK.PD4
    or
    -USART2_Tx.PA2 <-------> SPI2_MOSI.PB15
    -USART2_Rx.PA3 <-------> SPI2_MISO.PB14
    -USART2_Clk.PA4 <-------> SPI2_SCK.PB13

    
    Test steps and phenomena:
    -After the Demo is compiled in the KEIL environment, download it to the MCU
    -Reset operation, check the variables TransferStatus1 and TransferStatus2 in turn, among them,
      PASSED means the test passed, FAILED means the test is abnormal


4. Attention