*PADS-LOGIC-V9.0* 来自 PADS LOGIC VVX.2.7 的设计导出文件
*SCH*        GENERAL PARAMETERS OF THE SCHEMATIC DESIGN"

CUR SHEET    1              Current Active Sheet
USERGRID     50     50      Design and Label/Text grid settings
LINEWIDTH    10             Width items will be created with
CONNWIDTH    10             Width used to plot connections
BUSWIDTH     25             Width used to plot buses
BUSANGLE     25             Angle used when plotting buses
NNVISPWRGND  4              Pwr/Gnd netname visibility default flag
PCBFLAGS     1039           PCB Netlist and ECO options
PINNAMESIZE  97     10      Height and LineWidth used by pin names
TEXTSIZE     250    10      Height and LineWidth text will be created width
JOBTIME      0              Amount of time spent on this LOGIC design
DOTGRID      10             Space in thous/inch between graphic dots
BACKUPTIME   5              Number of minutes between database backups
TIEDOTSIZE   50             Diameter of tiedot point
REFNAMESIZE  100    10      Height and LineWidth used by part ref. names
PARTNAMESIZE 100    10      Height and LineWidth used by part type names
PINNOSIZE    97     10      Height and LineWidth used by pin numbers
NETNAMESIZE  100    10      Height and LineWidth used by net names
REAL WIDTH   20             Widths greater then this are displayed real size
SHEET SIZE   C             
UNITS        1              Rules units type
JOBNAME      N32G45XCL-STB_V1.1.sch
NTXCOL 11 9
HIRCOL 2
LINCOL 9
TXTCOL 0 31
CONCOL 9
BUSCOL 4
PTXCOL 0 31
COMCOL 4
NMCOL  1 31
PNMCOL 1 31
PINCOL 0 31
NETCOL 1 31
FBGCOL 13 31
OFFREFVIEW   0              Offsheet references visibility default flag
OFFREFNUM    0              Offsheet references per line
SHEETNUMSEP  []             Sheet Number separators
FONT MODE   System
DEFAULT FONT "Regular Arial Unicode MS"
BORDER NAME SIZEB
FIELDCOL 1 0

*CAM* PLOTTER SETTINGS 

*MISC*      MISCELLANEOUS PARAMETERS
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

LAYER	METRIC
{
LAYER	0
{
LAYER_THICKNESS	0
DIELECTRIC	3.300000
}
LAYER	1
{
LAYER_NAME	Top
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
ASSOCIATED_SILK_SCREEN	Silkscreen Top
ASSOCIATED_PASTE_MASK	Paste Mask Top
ASSOCIATED_SOLDER_MASK	Solder Mask Top
ASSOCIATED_ASSEMBLY	Assembly Drawing Top
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	2
{
LAYER_NAME	Bottom
LAYER_TYPE	ROUTING
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
ROUTABLE	Y
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	3.300000
COST	0
}
LAYER	3
{
LAYER_NAME	Layer_3
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	4
{
LAYER_NAME	Layer_4
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	3.300000
COST	0
}
LAYER	5
{
LAYER_NAME	Layer_5
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	HORIZONTAL
LAYER_THICKNESS	0.254
COPPER_THICKNESS	0.03429
DIELECTRIC	4.300000
COST	0
}
LAYER	6
{
LAYER_NAME	Layer_6
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	VERTICAL
ASSOCIATED_SILK_SCREEN	Silkscreen Bottom
ASSOCIATED_PASTE_MASK	Paste Mask Bottom
ASSOCIATED_SOLDER_MASK	Solder Mask Bottom
ASSOCIATED_ASSEMBLY	Assembly Drawing Bottom
COMPONENT	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0.03429
DIELECTRIC	3.300000
COST	0
}
LAYER	7
{
LAYER_NAME	Layer_7
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	8
{
LAYER_NAME	Layer_8
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	9
{
LAYER_NAME	Layer_9
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	10
{
LAYER_NAME	Layer_10
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	11
{
LAYER_NAME	Layer_11
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	12
{
LAYER_NAME	Layer_12
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	13
{
LAYER_NAME	Layer_13
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	14
{
LAYER_NAME	Layer_14
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	15
{
LAYER_NAME	Layer_15
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	16
{
LAYER_NAME	Layer_16
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	17
{
LAYER_NAME	Layer_17
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	18
{
LAYER_NAME	Layer_18
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	19
{
LAYER_NAME	Layer_19
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	20
{
LAYER_NAME	Layer_20
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	21
{
LAYER_NAME	Layer_21
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	22
{
LAYER_NAME	Layer_22
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	23
{
LAYER_NAME	Layer_23
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	24
{
LAYER_NAME	Layer_24
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	25
{
LAYER_NAME	Layer_25
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	26
{
LAYER_NAME	Layer_26
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	27
{
LAYER_NAME	Layer_27
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	28
{
LAYER_NAME	Layer_28
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	29
{
LAYER_NAME	Layer_29
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	30
{
LAYER_NAME	Layer_30
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	31
{
LAYER_NAME	Layer_31
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	32
{
LAYER_NAME	Layer_32
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	33
{
LAYER_NAME	Layer_33
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	34
{
LAYER_NAME	Layer_34
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	35
{
LAYER_NAME	Layer_35
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	36
{
LAYER_NAME	Layer_36
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	37
{
LAYER_NAME	Layer_37
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	38
{
LAYER_NAME	Layer_38
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	39
{
LAYER_NAME	Layer_39
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	40
{
LAYER_NAME	Layer_40
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	41
{
LAYER_NAME	Layer_41
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	42
{
LAYER_NAME	Layer_42
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	43
{
LAYER_NAME	Layer_43
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	44
{
LAYER_NAME	Layer_44
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	45
{
LAYER_NAME	Layer_45
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	46
{
LAYER_NAME	Layer_46
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	47
{
LAYER_NAME	Layer_47
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	48
{
LAYER_NAME	Layer_48
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	49
{
LAYER_NAME	Layer_49
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	50
{
LAYER_NAME	Layer_50
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	51
{
LAYER_NAME	Layer_51
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	52
{
LAYER_NAME	Layer_52
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	53
{
LAYER_NAME	Layer_53
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	54
{
LAYER_NAME	Layer_54
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	55
{
LAYER_NAME	Layer_55
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	56
{
LAYER_NAME	Layer_56
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	57
{
LAYER_NAME	Layer_57
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	58
{
LAYER_NAME	Layer_58
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	59
{
LAYER_NAME	Layer_59
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	60
{
LAYER_NAME	Layer_60
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	61
{
LAYER_NAME	Layer_61
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	62
{
LAYER_NAME	Layer_62
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	63
{
LAYER_NAME	Layer_63
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	64
{
LAYER_NAME	Layer_64
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	65
{
LAYER_NAME	Layer_65
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	66
{
LAYER_NAME	Layer_66
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	67
{
LAYER_NAME	Layer_67
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	68
{
LAYER_NAME	Layer_68
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	69
{
LAYER_NAME	Layer_69
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	70
{
LAYER_NAME	Layer_70
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	71
{
LAYER_NAME	Layer_71
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	72
{
LAYER_NAME	Layer_72
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	73
{
LAYER_NAME	Layer_73
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	74
{
LAYER_NAME	Layer_74
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	75
{
LAYER_NAME	Layer_75
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	76
{
LAYER_NAME	Layer_76
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	77
{
LAYER_NAME	Layer_77
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	78
{
LAYER_NAME	Layer_78
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	79
{
LAYER_NAME	Layer_79
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	80
{
LAYER_NAME	Layer_80
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	81
{
LAYER_NAME	Layer_81
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	82
{
LAYER_NAME	Layer_82
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	83
{
LAYER_NAME	Layer_83
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	84
{
LAYER_NAME	Layer_84
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	85
{
LAYER_NAME	Layer_85
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	86
{
LAYER_NAME	Layer_86
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	87
{
LAYER_NAME	Layer_87
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	88
{
LAYER_NAME	Layer_88
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	89
{
LAYER_NAME	Layer_89
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	90
{
LAYER_NAME	Layer_90
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	91
{
LAYER_NAME	Layer_91
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	92
{
LAYER_NAME	Layer_92
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	93
{
LAYER_NAME	Layer_93
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	94
{
LAYER_NAME	Layer_94
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	95
{
LAYER_NAME	Layer_95
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	96
{
LAYER_NAME	Layer_96
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	97
{
LAYER_NAME	Layer_97
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	98
{
LAYER_NAME	Layer_98
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	99
{
LAYER_NAME	Layer_99
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	100
{
LAYER_NAME	Layer_100
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	101
{
LAYER_NAME	Layer_101
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	102
{
LAYER_NAME	Layer_102
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	103
{
LAYER_NAME	Layer_103
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	104
{
LAYER_NAME	Layer_104
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	105
{
LAYER_NAME	Layer_105
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	106
{
LAYER_NAME	Layer_106
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	107
{
LAYER_NAME	Layer_107
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	108
{
LAYER_NAME	Layer_108
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	109
{
LAYER_NAME	Layer_109
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	110
{
LAYER_NAME	Layer_110
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	111
{
LAYER_NAME	Layer_111
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	112
{
LAYER_NAME	Layer_112
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	113
{
LAYER_NAME	Layer_113
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	114
{
LAYER_NAME	Layer_114
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	115
{
LAYER_NAME	Layer_115
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	116
{
LAYER_NAME	Layer_116
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	117
{
LAYER_NAME	Layer_117
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	118
{
LAYER_NAME	Layer_118
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	119
{
LAYER_NAME	Layer_119
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	120
{
LAYER_NAME	Layer_120
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	121
{
LAYER_NAME	Solder Mask Top
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	122
{
LAYER_NAME	Paste Mask Bottom
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	123
{
LAYER_NAME	Paste Mask Top
LAYER_TYPE	PASTE_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	124
{
LAYER_NAME	Drill Drawing
LAYER_TYPE	DRILL
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	125
{
LAYER_NAME	Layer_125
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	126
{
LAYER_NAME	Silkscreen Top
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	127
{
LAYER_NAME	Assembly Drawing Top
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	128
{
LAYER_NAME	Solder Mask Bottom
LAYER_TYPE	SOLDER_MASK
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	129
{
LAYER_NAME	Silkscreen Bottom
LAYER_TYPE	SILK_SCREEN
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	130
{
LAYER_NAME	Assembly Drawing Bottom
LAYER_TYPE	ASSEMBLY
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
VISIBLE	Y
SELECTABLE	Y
ENABLED	Y
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	131
{
LAYER_NAME	Layer_131
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	132
{
LAYER_NAME	Layer_132
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	133
{
LAYER_NAME	Layer_133
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	134
{
LAYER_NAME	Layer_134
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	135
{
LAYER_NAME	Layer_135
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	136
{
LAYER_NAME	Layer_136
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	137
{
LAYER_NAME	Layer_137
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	138
{
LAYER_NAME	Layer_138
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	139
{
LAYER_NAME	Layer_139
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	140
{
LAYER_NAME	Layer_140
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	141
{
LAYER_NAME	Layer_141
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	142
{
LAYER_NAME	Layer_142
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	143
{
LAYER_NAME	Layer_143
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	144
{
LAYER_NAME	Layer_144
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	145
{
LAYER_NAME	Layer_145
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	146
{
LAYER_NAME	Layer_146
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	147
{
LAYER_NAME	Layer_147
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	148
{
LAYER_NAME	Layer_148
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	149
{
LAYER_NAME	Layer_149
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	150
{
LAYER_NAME	Layer_150
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	151
{
LAYER_NAME	Layer_151
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	152
{
LAYER_NAME	Layer_152
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	153
{
LAYER_NAME	Layer_153
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	154
{
LAYER_NAME	Layer_154
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	155
{
LAYER_NAME	Layer_155
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	156
{
LAYER_NAME	Layer_156
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	157
{
LAYER_NAME	Layer_157
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	158
{
LAYER_NAME	Layer_158
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	159
{
LAYER_NAME	Layer_159
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	160
{
LAYER_NAME	Layer_160
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	161
{
LAYER_NAME	Layer_161
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	162
{
LAYER_NAME	Layer_162
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	163
{
LAYER_NAME	Layer_163
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	164
{
LAYER_NAME	Layer_164
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	165
{
LAYER_NAME	Layer_165
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	166
{
LAYER_NAME	Layer_166
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	167
{
LAYER_NAME	Layer_167
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	168
{
LAYER_NAME	Layer_168
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	169
{
LAYER_NAME	Layer_169
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	170
{
LAYER_NAME	Layer_170
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	171
{
LAYER_NAME	Layer_171
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	172
{
LAYER_NAME	Layer_172
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	173
{
LAYER_NAME	Layer_173
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	174
{
LAYER_NAME	Layer_174
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	175
{
LAYER_NAME	Layer_175
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	176
{
LAYER_NAME	Layer_176
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	177
{
LAYER_NAME	Layer_177
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	178
{
LAYER_NAME	Layer_178
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	179
{
LAYER_NAME	Layer_179
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	180
{
LAYER_NAME	Layer_180
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	181
{
LAYER_NAME	Layer_181
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	182
{
LAYER_NAME	Layer_182
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	183
{
LAYER_NAME	Layer_183
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	184
{
LAYER_NAME	Layer_184
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	185
{
LAYER_NAME	Layer_185
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	186
{
LAYER_NAME	Layer_186
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	187
{
LAYER_NAME	Layer_187
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	188
{
LAYER_NAME	Layer_188
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	189
{
LAYER_NAME	Layer_189
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	190
{
LAYER_NAME	Layer_190
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	191
{
LAYER_NAME	Layer_191
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	192
{
LAYER_NAME	Layer_192
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	193
{
LAYER_NAME	Layer_193
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	194
{
LAYER_NAME	Layer_194
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	195
{
LAYER_NAME	Layer_195
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	196
{
LAYER_NAME	Layer_196
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	197
{
LAYER_NAME	Layer_197
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	198
{
LAYER_NAME	Layer_198
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	199
{
LAYER_NAME	Layer_199
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	200
{
LAYER_NAME	Layer_200
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	201
{
LAYER_NAME	Layer_201
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	202
{
LAYER_NAME	Layer_202
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	203
{
LAYER_NAME	Layer_203
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	204
{
LAYER_NAME	Layer_204
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	205
{
LAYER_NAME	Layer_205
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	206
{
LAYER_NAME	Layer_206
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	207
{
LAYER_NAME	Layer_207
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	208
{
LAYER_NAME	Layer_208
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	209
{
LAYER_NAME	Layer_209
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	210
{
LAYER_NAME	Layer_210
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	211
{
LAYER_NAME	Layer_211
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	212
{
LAYER_NAME	Layer_212
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	213
{
LAYER_NAME	Layer_213
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	214
{
LAYER_NAME	Layer_214
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	215
{
LAYER_NAME	Layer_215
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	216
{
LAYER_NAME	Layer_216
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	217
{
LAYER_NAME	Layer_217
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	218
{
LAYER_NAME	Layer_218
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	219
{
LAYER_NAME	Layer_219
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	220
{
LAYER_NAME	Layer_220
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	221
{
LAYER_NAME	Layer_221
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	222
{
LAYER_NAME	Layer_222
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	223
{
LAYER_NAME	Layer_223
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	224
{
LAYER_NAME	Layer_224
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	225
{
LAYER_NAME	Layer_225
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	226
{
LAYER_NAME	Layer_226
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	227
{
LAYER_NAME	Layer_227
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	228
{
LAYER_NAME	Layer_228
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	229
{
LAYER_NAME	Layer_229
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	230
{
LAYER_NAME	Layer_230
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	231
{
LAYER_NAME	Layer_231
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	232
{
LAYER_NAME	Layer_232
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	233
{
LAYER_NAME	Layer_233
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	234
{
LAYER_NAME	Layer_234
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	235
{
LAYER_NAME	Layer_235
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	236
{
LAYER_NAME	Layer_236
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	237
{
LAYER_NAME	Layer_237
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	238
{
LAYER_NAME	Layer_238
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	239
{
LAYER_NAME	Layer_239
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	240
{
LAYER_NAME	Layer_240
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	241
{
LAYER_NAME	Layer_241
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	242
{
LAYER_NAME	Layer_242
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	243
{
LAYER_NAME	Layer_243
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	244
{
LAYER_NAME	Layer_244
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	245
{
LAYER_NAME	Layer_245
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	246
{
LAYER_NAME	Layer_246
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	247
{
LAYER_NAME	Layer_247
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	248
{
LAYER_NAME	Layer_248
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	249
{
LAYER_NAME	Layer_249
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
LAYER	250
{
LAYER_NAME	Layer_250
LAYER_TYPE	UNASSIGNED
PLANE	NONE
ROUTING_DIRECTION	NO_PREFERENCE
LAYER_THICKNESS	0
COPPER_THICKNESS	0
DIELECTRIC	0.000000
COST	0
}
}
*REMARK*    PARENT_KEYWORD PARENT_VALUE
*REMARK*  [ { 
*REMARK*       CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ CHILD_KEYWORD CHILD_VALUE
*REMARK*     [ { 
*REMARK*          GRAND_CHILD_KEYWORD GRAND_CHILD_VALUE [...] 
*REMARK*       } ]] 
*REMARK*    } ] 

RULES_SECTION	METRIC
{
NET_CLASS	DATA
DESIGN	RULES
{
RULE_SET	(1)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.15
VIA_TO_TRACK	0.15
VIA_TO_VIA	0.15
PAD_TO_TRACK	0.15
PAD_TO_VIA	0.15
PAD_TO_PAD	0.15
SMD_TO_TRACK	0.15
SMD_TO_VIA	0.15
SMD_TO_PAD	0.15
SMD_TO_SMD	0.15
COPPER_TO_TRACK	0.15
COPPER_TO_VIA	0.15
COPPER_TO_PAD	0.15
COPPER_TO_SMD	0.15
COPPER_TO_COPPER	0.15
TEXT_TO_TRACK	0.15
TEXT_TO_VIA	0.15
TEXT_TO_PAD	0.15
TEXT_TO_SMD	0.15
OUTLINE_TO_TRACK	0.15
OUTLINE_TO_VIA	0.15
OUTLINE_TO_PAD	0.15
OUTLINE_TO_SMD	0.15
OUTLINE_TO_COPPER	0.15
DRILL_TO_TRACK	0.15
DRILL_TO_VIA	0.15
DRILL_TO_PAD	0.15
DRILL_TO_SMD	0.15
DRILL_TO_COPPER	0.15
SAME_NET_SMD_TO_VIA	0
SAME_NET_SMD_TO_CRN	0
SAME_NET_VIA_TO_VIA	0
SAME_NET_PAD_TO_CRN	0
MIN_TRACK_WIDTH	0.15
REC_TRACK_WIDTH	0.15
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1524
BODY_TO_BODY	0.1524
SAME_NET_TRACK_TO_CRN	0
}
}
RULE_SET	(2)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
HIGH_SPEED_RULE	:
{
MIN_LENGTH	0
MAX_LENGTH	1269.99996
STUB_LENGTH	0
PARALLEL_LENGTH	25.4
PARALLEL_GAP	5.08
TANDEM_LENGTH	25.4
TANDEM_GAP	5.08
MIN_DELAY	0.000000
MAX_DELAY	10.000000
MIN_CAPACITANCE	0.000000
MAX_CAPACITANCE	10.000000
MIN_IMPEDANCE	50.000000
MAX_IMPEDANCE	150.000000
SHIELD_NET	*
SHIELD_GAP	5.08
MATCH_LENGTH_TOLERANCE	5.08
}
}
RULE_SET	(3)
{
FOR	:
{
DEFAULT	:
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
ROUTE_RULE	:
{
LENGTH_MINIMIZATION_TYPE	1
TRACE_SHARE	Y
VIA_SHARE	Y
AUTO_ROUTE	Y
RIPUP	Y
SHOVE	Y
ROUTE_PRIORITY	3
MAX_NUMBER_OF_VIAS	-1
VALID_LAYER	1
VALID_LAYER	2
VALID_VIA_TYPE	*USE_CURRENT*
}
}
RULE_SET	(4)
{
FOR	:
{
NET	5V
}
AGAINST	:
{
DEFAULT	:
}
LAYER	0
CLEARANCE_RULE	:
{
TRACK_TO_TRACK	0.15
VIA_TO_TRACK	0.15
VIA_TO_VIA	0.15
PAD_TO_TRACK	0.15
PAD_TO_VIA	0.15
PAD_TO_PAD	0.15
SMD_TO_TRACK	0.15
SMD_TO_VIA	0.15
SMD_TO_PAD	0.15
SMD_TO_SMD	0.15
COPPER_TO_TRACK	0.15
COPPER_TO_VIA	0.15
COPPER_TO_PAD	0.15
COPPER_TO_SMD	0.15
COPPER_TO_COPPER	0.15
TEXT_TO_TRACK	0.15
TEXT_TO_VIA	0.15
TEXT_TO_PAD	0.15
TEXT_TO_SMD	0.15
OUTLINE_TO_TRACK	0.15
OUTLINE_TO_VIA	0.15
OUTLINE_TO_PAD	0.15
OUTLINE_TO_SMD	0.15
OUTLINE_TO_COPPER	0.15
DRILL_TO_TRACK	0.15
DRILL_TO_VIA	0.15
DRILL_TO_PAD	0.15
DRILL_TO_SMD	0.15
DRILL_TO_COPPER	0.15
SAME_NET_SMD_TO_VIA	0
SAME_NET_SMD_TO_CRN	0
SAME_NET_VIA_TO_VIA	0
SAME_NET_PAD_TO_CRN	0
MIN_TRACK_WIDTH	0.15
REC_TRACK_WIDTH	0.5
MAX_TRACK_WIDTH	1
DRILL_TO_DRILL	0.1524
BODY_TO_BODY	0.1524
SAME_NET_TRACK_TO_CRN	0
}
}
DIF_PAIR	D1
{
NET	PA12/USBDP
NET	PA11/USBDM
MIN_LENGTH	0
MAX_LENGTH	11379.2
GAP	0.24
MAX_OBSTACLE_SIZE	0.635
MAX_OBSTACLE_NUMBER	3
WIDTH	0.15
}
DIF_PAIR	D2
{
NET	DM_NSLINK
NET	DP_NSLINK
MIN_LENGTH	0
MAX_LENGTH	11379.2
GAP	0.24
MAX_OBSTACLE_SIZE	0.635
MAX_OBSTACLE_NUMBER	3
WIDTH	0.15
}
DIF_PAIR	D3
{
NET	PA11
NET	PA12
MIN_LENGTH	0
MAX_LENGTH	11379.2
GAP	0.24
MAX_OBSTACLE_SIZE	0.635
MAX_OBSTACLE_NUMBER	3
WIDTH	0.15
}
}
}

*FIELDS*    USER FIELDS

"DRAWN" 
"CHECKED" 
"QUALITY CONTROL" 
"RELEASED" 
"COMPANY" 
"COMPANY ADDRESS" 
"TITLE" N32G45XCL-STB
"CODE" A
"SCALE" 
"DRAWING NO" 
"REV" 
"Drawn By" 
"Checked By" 
"QC By" 
"Released By" 
"Drawn Date" 
"Checked Date" 
"QC Date" 
"Release Date" 
"Company Name" NATIONS
"Drawing Number" 1
"Revision" 1.1

*SHT*   2 NS-LINK -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        8.021          Scale of window expansion
WINDOWCENTER 2676   4383    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

15700  13250  0   1 417  10 0 "Default Font"
DEBUG USB
7150   13150  0   1 417  10 0 "Default Font"
MCU
15510  9850   0   1 417  10 0 "Default Font"
HEADER
15510  6350   0   1 417  10 0 "Default Font"
LED
11050  14000  0   1 556  10 0 "Default Font"
NS-LINK

*LINES*      LINES ITEMS

D79026           LINES    21000  2100   34  40
OPEN   2   10  255
0      0     
-5010  0     
OPEN   2   10  255
-500   0     
-500   -950  
OPEN   2   10  255
-1800  -950  
-1800  -1200 
OPEN   2   10  255
-3100  0     
-3100  -950  
OPEN   2   10  255
-3800  0     
-3800  -950  
OPEN   2   10  255
0      -950  
-5000  -950  
OPEN   2   10  255
-5000  1290  
-5000  -1200 
OPEN   2   10  255
0      800   
-5000  800   
OPEN   2   10  255
-5000  -400  
-7500  -400  
CLOSED 7   10  255
0      -1200 
0      1290  
-5000  1290  
-5000  400   
-7500  400   
-7500  -1200 
0      -1200 
OPEN   2   10  255
-5010  0     
-7500  0     
OPEN   2   10  255
-5000  -800  
-7500  -800  
OPEN   2   10  255
-6000  400   
-6000  -1200 
OPEN   2   10  255
-20000 6400  
-20500 6400  
OPEN   2   10  255
-20000 10200 
-20500 10200 
OPEN   2   10  255
-16670 14500 
-16670 14000 
OPEN   2   10  255
-13340 14500 
-13340 14000 
OPEN   2   10  255
-10010 14500 
-10010 14000 
OPEN   2   10  255
-6680  14500 
-6680  14000 
OPEN   2   10  255
500    2600  
0      2600  
OPEN   2   10  255
500    6400  
0      6400  
OPEN   2   10  255
500    10200 
0      10200 
OPEN   2   10  255
-3350  14500 
-3350  14000 
OPEN   2   10  255
-2870  13800 
-2870  12800 
OPEN   2   10  255
-470   13800 
-470   12800 
OPEN   2   10  255
-1370  13800 
-1370  12800 
OPEN   2   10  255
-3470  13400 
0      13400 
OPEN   2   10  255
-3470  13800 
0      13800 
OPEN   2   10  255
-3470  13600 
0      13600 
OPEN   2   10  255
-3470  13200 
0      13200 
OPEN   2   10  255
-3470  13000 
0      13000 
CLOSED 5   10  255
0      14000 
-3470  14000 
-3470  12800 
0      12800 
0      14000 
CLOSED 5   10  255
0      -1200 
0      14000 
-20000 14000 
-20000 -1200 
0      -1200 
OPEN   2   10  255
-20000 2600  
-20500 2600  
-2300  400    0   12 250  10 1 "Default Font"
TITLE
-1470  -1050  0   8 153  10 1 "Default Font"
Sheet Number
-1220  -1050  0   8 153  10 1 "Default Font"
Number of Sheets
-300   -600   0   12 306  10 1 "Default Font"
Revision
-2500  1050   0   12 250  10 1 "Default Font"
Company Name
-400   -200   0   0 97   10 0 "Default Font"
REV:
-3600  -200   0   0 97   10 0 "Default Font"
SIZE:
-4550  -200   0   0 97   10 0 "Default Font"
CODE:
-7460  250    0   0 97   10 0 "Default Font"
DRAWN:
-5960  250    0   0 97   10 0 "Default Font"
DATED:
-5960  -150   0   0 97   10 0 "Default Font"
DATED:
-7460  -150   0   0 97   10 0 "Default Font"
CHECKED:
-7460  -550   0   0 97   10 0 "Default Font"
QUALITY CONTROL:
-5960  -550   0   0 97   10 0 "Default Font"
DATED:
-5960  -950   0   0 97   10 0 "Default Font"
DATED:
-7460  -950   0   0 97   10 0 "Default Font"
RELEASED:
-4960  1100   0   0 97   10 0 "Default Font"
COMPANY:
-4960  600    0   0 97   10 0 "Default Font"
TITLE:
-2150  -200   0   0 97   10 0 "Default Font"
DRAWING NO:
-1750  -1100  0   0 97   10 0 "Default Font"
SHEET:     OF
-4950  -1100  0   0 97   10 0 "Default Font"
SCALE:
-2150  13850  0   0 97   10 0 "Default Font"
REVISION RECORD
-1200  13650  0   0 97   10 0 "Default Font"
APPROVED:
-2350  13650  0   0 97   10 0 "Default Font"
ECO NO:
-3250  13650  0   0 97   10 0 "Default Font"
LTR
-420   13650  0   0 97   10 0 "Default Font"
DATE:
-1700  14100  0   0 250  25 0 "Default Font"
1
-5050  14100  0   0 250  25 0 "Default Font"
2
-8350  14100  0   0 250  25 0 "Default Font"
3
-11700 14100  0   0 250  25 0 "Default Font"
4
-15000 14100  0   0 250  25 0 "Default Font"
5
-18350 14100  0   0 250  25 0 "Default Font"
6
-20250 12100  0   0 250  25 0 "Default Font"
D
-20250 8300   0   0 250  25 0 "Default Font"
C
-20250 4500   0   0 250  25 0 "Default Font"
B
-20250 650    0   0 250  25 0 "Default Font"
A
100    8350   0   0 250  25 0 "Default Font"
C
100    12050  0   0 250  25 0 "Default Font"
D
100    4500   0   0 250  25 0 "Default Font"
B
100    850    0   0 250  25 0 "Default Font"
A
DRW53857         LINES    2500   13700  1   0
CLOSED 5   10  0  
0      0     
0      -9300 
8800   -9300 
8800   0     
0      0     
DRW54153         LINES    12200  13700  1   0
CLOSED 5   10  0  
0      0     
0      -3100 
5700   -3100 
5700   0     
0      0     
D54202           LINES    12200  10400  1   0
CLOSED 5   10  0  
0      0     
0      -3300 
5700   -3300 
5700   0     
0      0     
D54207           LINES    12200  6900   1   0
CLOSED 5   10  0  
0      0     
0      -2500 
5700   -2500 
5700   0     
0      0     
DRW12905         LINES    2300   14700  1   0
CLOSED 5   20  0  
0      0     
0      -10500
15800  -10500
15800  0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN50            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.21.33
"Default Font"
"Default Font"
-820 400 0 8 93 10 "Default Font"
REF-DES
-1050 400 0 1 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-100  0    

PIN35            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.35.28
"Default Font"
"Default Font"
100 50 90 10 93 10 "Default Font"
REF-DES
100 280 90 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-70   0    

PIN60            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.35.28
"Default Font"
"Default Font"
100 0 0 9 93 10 "Default Font"
REF-DES
330 0 0 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-120  0    

PIN25            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.07.58.51
"Default Font"
"Default Font"
-70 0 0 8 93 10 "Default Font"
REF-DES
-300 0 0 1 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-50   0    

PIN45            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.10.03.08
"Default Font"
"Default Font"
-70 0 0 9 93 10 "Default Font"
REF-DES
160 0 0 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-90   0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

PIN100           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2018.07.02.06.46.22
"Regular Arial"
"Default Font"
280 0 0 8 93 10 "Regular Arial"
REF-DES
50 0 0 1 93 10 "Regular Arial"
PART-TYPE
OPEN   2   1   255
0     0    
-200  0    

PIN150           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2018.07.23.13.41.14
"Regular Arial"
"Regular Arial"
50 5200 0 8 93 10 "Regular Arial"
REF-DES
-50 5200 0 1 93 10 "Regular Arial"
PART-TYPE
OPEN   2   1   255
0     0    
-300  0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

BUBBLE           33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

Y                33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-5V              33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

-12V             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5VA             33500 33274 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CON_MINIUSB      32000 32000 100 10 100 10 4 1 0 11 0 0
TIMESTAMP 2019.12.11.09.21.40
"Default Font"
"Default Font"
80 1260 0 4 100 10 "Default Font"
REF-DES
290 -40 0 6 100 10 "Default Font"
PART-TYPE
340 -150 0 6 100 10 "Default Font"
*
350 -270 0 6 100 10 "Default Font"
*
OPEN   5   10  255
0     0    
0     1200 
500   1200 
500   0    
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CON-SIP-4P       32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.11.27.05.40.08
"Default Font"
"Default Font"
50 50 0 4 97 10 "Default Font"
REF-DES
100 -500 0 6 97 10 "Default Font"
PART-TYPE
100 -600 0 6 97 10 "Default Font"
*
100 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -500 
200   -500 
200   0    
0     0    
T-100  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -200  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -300  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-100  -400  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

DIODE            32000 32000 90 10 80 10 4 4 0 2 18 0
TIMESTAMP 2019.12.01.15.48.44
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0

HEADER\8X2       32000 32000 100 10 100 10 4 18 0 16 0 0
TIMESTAMP 2019.03.12.09.21.06
"Default Font"
"Default Font"
300 950 0 4 100 10 "Default Font"
REF-DES
300 900 0 6 100 10 "Default Font"
PART-TYPE
350 -200 0 6 100 10 "Default Font"
SPIL PART #
350 -300 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
200   600  
250   600  
CIRCLE 2   10  255
200   500  
250   500  
CIRCLE 2   10  255
200   400  
250   400  
CIRCLE 2   10  255
200   300  
250   300  
CIRCLE 2   10  255
200   200  
250   200  
CIRCLE 2   10  255
200   100  
250   100  
CIRCLE 2   10  255
200   0    
250   0    
CIRCLE 2   10  255
300   600  
350   600  
CIRCLE 2   10  255
300   500  
350   500  
CIRCLE 2   10  255
300   400  
350   400  
CIRCLE 2   10  255
300   300  
350   300  
CIRCLE 2   10  255
300   200  
350   200  
CIRCLE 2   10  255
300   100  
350   100  
CIRCLE 2   10  255
300   0    
350   0    
CLOSED 5   10  255
150   650  
400   650  
400   -150 
150   -150 
150   650  
CIRCLE 2   10  255
200   -100 
250   -100 
CIRCLE 2   10  255
300   -100 
350   -100 
CIRCLE 2   10  255
300   -100 
350   -100 
T0     600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T0     -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T550   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

N32G4XC          32000 32000 97 10 97 10 4 1 0 48 0 0
TIMESTAMP 2019.11.28.08.56.49
"Default Font"
"Default Font"
2300 2340 0 0 97 10 "Default Font"
REF-DES
2300 -40 0 2 97 10 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 "Default Font"
*
2300 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2300  0    
2300  2300 
0     2300 
0     0    
T-200  1700  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1700  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.28
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CAP              32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2019.11.28.11.16.25
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

CON1X3           32000 32000 100 10 100 10 4 7 0 3 0 0
TIMESTAMP 2019.12.01.16.15.06
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 -250 0 6 100 10 "Default Font"
PART-TYPE
0 -240 0 6 100 10 "Default Font"
*
0 -340 0 6 100 10 "Default Font"
*
CIRCLE 2   10  255
0     50   
0     150  
CIRCLE 2   10  255
0     -50  
0     50   
CLOSED 5   10  255
-100  200  
-100  -200 
100   -200 
100   200  
-100  200  
CIRCLE 2   10  255
0     -50  
0     -150 
OPEN   2   10  255
-100  100  
-50   100  
OPEN   2   10  255
-100  -100 
-50   -100 
OPEN   2   10  255
-50   0    
-100  0    
T-200  100   0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T-200  -100  0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
OFF 2
REFIN S 
REFOUT L 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
PWR 7
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA

CON-SIP-4P CON  1   0   0     0
TIMESTAMP 2019.11.27.05.40.07
GATE 1 4 0
CON-SIP-4P
1 0 U
2 0 U
3 0 U
4 0 U

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

MINIUSB CON  1   0   0     0
TIMESTAMP 2019.12.11.09.21.39
GATE 1 11 0
CON_MINIUSB
1 0 U VBUS
2 0 U D-
3 0 U D+
4 0 U ID
5 0 U GND
6 0 U SHIELD1
7 0 U SHIELD2
8 0 U SHIELD3
9 0 U SHIELD4
10 0 U H1
11 0 U H2

DIODE_2 UND  1   0   0     0
TIMESTAMP 2019.12.01.15.48.43
GATE 1 2 0
DIODE
1 0 U
2 0 U

HEADER-8X2 CON  1   0   0     0
TIMESTAMP 2019.03.12.09.21.05
GATE 1 16 0
HEADER\8X2
1 0 U
3 0 U
5 0 U
7 0 U
9 0 U
11 0 U
13 0 U
15 0 U
2 0 U
4 0 U
6 0 U
8 0 U
10 0 U
12 0 U
14 0 U
16 0 U

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

N32G4XC UND  1   0   0     0
TIMESTAMP 2019.11.28.08.56.48
GATE 1 48 0
N32G4XC
1 0 U VBAT
2 0 U PC13-TAMPER-RTC
3 0 U PC14-OSC32_IN
4 0 U PC15-OSC32_OUT
5 0 U PD0-OSC_IN
6 0 U PD1-OSC_OUT
7 0 U NRST
8 0 U VSSA
9 0 U VDDA
10 0 U PA0-WKUP
11 0 U PA1
12 0 U PA2
13 0 U PA3
14 0 U PA4
15 0 U PA5
16 0 U PA6
17 0 U PA7
18 0 U PB0
19 0 U PB1
20 0 U PB2-BOOT
21 0 U PB10
22 0 U PB11
23 0 U VSS_1
24 0 U VDD_1
25 0 U PB12
26 0 U PB13
27 0 U PB14
28 0 U PB15
29 0 U PA8
30 0 U PA9
31 0 U PA10
32 0 U PA11
33 0 U PA12
34 0 U PA13-SWDIO
35 0 U VSS_2
36 0 U VDD_2
37 0 U PA14-SWCLK
38 0 U PA15
39 0 U PB3
40 0 U PB4
41 0 U PB5
42 0 U PB6
43 0 U PB7
44 0 U BOOT0
45 0 U PB8
46 0 U PB9
47 0 U VSS_3
48 0 U VDD_3

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

C0603 CAP  1   0   0     0
TIMESTAMP 2019.11.28.11.16.24
GATE 1 2 0
CAP
1 1 U
2 1 U

CON1X3 CON  1   0   0     3
TIMESTAMP 2019.12.01.16.15.04
GATE 1 3 0
CON1X3
1 0 U
2 0 U
3 0 U
1 2 3 

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U



*PART*       ITEMS



J4           MINIUSB          13950 11000   0 1 97 10 97 10 4 3 11 0 0 0
"Default Font"
"Default Font"
250 1300 0 4 97 10 0 "Default Font"
REF-DES
290 -40 0 6 97 10 0 "Default Font"
PART-TYPE
340 -150 0 6 97 10 0 "Default Font"
*
350 -270 0 6 97 10 0 "Default Font"
*
"DECAL" 
"Description" 6 pin header
"PCB DECAL" CON_MINIUSB
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1

J10          CON-SIP-4P       17200 8100    0 0 97 10 97 10 4 1 4 0 0 2
"Default Font"
"Default Font"
100 50 0 4 97 10 0 "Default Font"
REF-DES
100 -500 0 6 97 10 0 "Default Font"
PART-TYPE
100 -600 0 6 97 10 0 "Default Font"
*
100 -700 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SIP-4P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1
3 60 10 0 1

R20          R0402            15100 5750    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R15          R0402            15100 5150    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D6           LED0805          14100 5800    0 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
300 -200 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D7           LED0805          14100 5200    0 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
300 -200 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D5           DIODE_2          15550 12300   0 0 97 10 97 10 4 2 2 0 0 18
"Default Font"
"Default Font"
250 150 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
300 -150 0 6 97 10 1 "Default Font"
VALUE
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SOD123
"VALUE" SS14L
0 130 14 0 1
1 130 14 0 1

J5           HEADER-8X2       13850 8000    0 0 97 10 97 10 4 10 16 0 0 0
"Default Font"
"Default Font"
300 950 0 4 97 10 0 "Default Font"
REF-DES
300 900 0 6 97 10 0 "Default Font"
PART-TYPE
350 -200 0 6 97 10 3 "Default Font"
Spil Part #
350 -300 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"Description" 7 X 2 PIN POLARIZED HEADER, 0.1" CENTERS
"Cost" 
"Part Number" 
"Manufacturer #1" 
"Spil Part #" 34-117
"Mating Spil Part #" ???
"PCB DECAL" HEADER16
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1

R11          R0402            15350 11950   0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 100 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R12          R0402            15350 11850   0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -50 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 100 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C22          CAP1206          15200 12900   0 0 97 10 97 10 4 15 2 0 0 26
"Default Font"
"Default Font"
180 -210 0 0 97 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Default Font"
PART-TYPE
180 -250 0 2 97 10 3 "Default Font"
Value
180 -360 0 2 97 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

U4           N32G4XC          5700  7200    0 0 97 10 97 10 4 2 48 0 0 2
"Default Font"
"Default Font"
1050 1300 0 0 97 10 0 "Default Font"
REF-DES
950 1050 0 2 97 10 0 "Default Font"
PART-TYPE
850 1050 0 2 97 10 1 "Default Font"
Value
2300 -240 0 2 97 10 0 "Default Font"
*
"PCB DECAL" QFP48-3
"Value" N32G455CCL7
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

C30          0402C            3550  9200    0 0 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C32          0402C            3550  8400    0 0 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

R19          R0402            8400  7850    0 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -40 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 140 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 100R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R17          R0402            6950  6550   90 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
200 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 160 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R4           R0402            3950  7950    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 -10 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R18          R0402            6650  10200  90 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
150 -50 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -50 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C5           C0603            4650  9150    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C9           C0603            4800  8000    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C14          C0603            7600  6900    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C18          C0603            8500  9400    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C19          C0603            5600  9900    0 3 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -400 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -100 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C20          C0603            5900  9900    0 3 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
-200 -400 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
-250 -100 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

R24          R0402            5350  7950    0 1 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
100 0 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 4.7K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J12          CON1X3           6700  11400  90 1 97 10 97 10 4 2 3 0 0 2
"Default Font"
"Default Font"
0 300 90 4 97 10 0 "Default Font"
REF-DES
0 -250 0 6 97 10 0 "Default Font"
PART-TYPE
0 -240 0 6 97 10 0 "Default Font"
*
0 -340 0 6 97 10 0 "Default Font"
*
"Marking" 
"PCB DECAL" 2.54MM_CON3P
0 60 10 0 1
1 60 10 0 1
2 60 10 0 1

C1           C0603            4200  7800    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
150 -210 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
150 -240 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

Y1           CRYSTAL_2PIN     4000  9050   90 3 97 10 97 10 4 2 2 0 0 2
"Default Font"
"Default Font"
250 120 0 4 97 10 0 "Default Font"
REF-DES
260 -120 0 6 97 10 0 "Default Font"
PART-TYPE
240 -296 0 6 97 10 0 "Default Font"
Value
240 -396 0 6 97 10 0 "Default Font"
*
"Value" 8MHz (AV08000301) 12pF
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 15200  12900  0 3 0
@@@O1    DP_NSLINK $OSR_SYMS 16450  11900  0 1 0
@@@O2    DM_NSLINK $OSR_SYMS 16450  12000  0 1 0
@@@O3    GND $GND_SYMS 14350  11300  0 0 0
@@@O4    GND $GND_SYMS 15700  4950   0 0 0
@@@O5    LED_CON $OSR_SYMS 13700  5800   0 0 0
@@@O6    LED_RUN $OSR_SYMS 13700  5200   0 0 0
@@@O7    5V $PWR_SYMS 16450  12450  0 0 0
@@@O8    VDD_LINK $PWR_SYMS 16950  8100   0 0 0
@@@O9    PA13/TMS/SWDIO $OSR_SYMS 16900  7900   0 0 0
@@@O10   PA14/TCK/SWCLK $OSR_SYMS 16900  7800   0 0 0
@@@O11   GND $GND_SYMS 16950  7650   0 0 0
@@@O12   PB0/RST $OSR_SYMS 13600  8100   0 0 0
@@@O13   VDD_LINK $PWR_SYMS 13650  8700   0 0 0
@@@O14   MCU_PA14/SWDCK $OSR_SYMS 14850  8400   0 1 0
@@@O15   MCU_PA13/SWDIO $OSR_SYMS 14850  8500   0 1 0
@@@O16   NSLINK_TMS_SWDIO $OSR_SYMS 13600  8500   0 0 0
@@@O17   NSLINK_TCK_SWCLK $OSR_SYMS 13600  8400   0 0 0
@@@O18   NRST $OSR_SYMS 14850  8100   0 1 0
@@@O19   VDD_LINK $PWR_SYMS 14550  8700   0 0 0
@@@O20   5V $PWR_SYMS 13600  8000   90 0 0
@@@O21   5V $PWR_SYMS 14850  8000   90 1 0
@@@O22   GND $GND_SYMS 13650  7800   0 0 0
@@@O23   GND $GND_SYMS 14550  7800   0 0 0
@@@O24   MCU_PA9/TX1 $OSR_SYMS 14850  8300   0 3 0
@@@O25   MCU_PA10/RX1 $OSR_SYMS 14850  8200   0 3 0
@@@O26   NSLINK_USART1_TX $OSR_SYMS 13600  8200   0 0 0
@@@O27   NSLINK_USART1_RX $OSR_SYMS 13600  8300   0 0 0
@@@O28   VDD_LINK $PWR_SYMS 3450   8000   90 0 0
@@@O29   GND $GND_SYMS 4200   7250   0 0 0
@@@O30   DM_NSLINK $OSR_SYMS 9000   8500   0 1 0
@@@O31   DP_NSLINK $OSR_SYMS 9000   8600   0 1 0
@@@O32   PB0/RST $OSR_SYMS 6800   6450   90 0 0
@@@O33   PA14/TCK/SWCLK $OSR_SYMS 7400   10100  90 2 0
@@@O34   PA13/TMS/SWDIO $OSR_SYMS 9000   8700   0 1 0
@@@O35   LED_RUN $OSR_SYMS 9000   8200   0 1 0
@@@O36   LED_CON $OSR_SYMS 6900   10100  90 2 0
@@@O37   GND $GND_SYMS 7000   6300   0 0 0
@@@O38   VDD_LINK $PWR_SYMS 4900   9600   0 0 0
@@@O39   VDD_LINK $PWR_SYMS 6300   10800  0 0 0
@@@O40   VDD_LINK $PWR_SYMS 8300   9600   0 0 0
@@@O41   GND $GND_SYMS 8700   8800   90 0 0
@@@O42   GND $GND_SYMS 6400   9900   0 2 0
@@@O43   GND $GND_SYMS 7300   6800   0 0 0
@@@O44   VDD_LINK $PWR_SYMS 7850   6900   90 1 0
@@@O45   NSLINK_TCK_SWCLK $OSR_SYMS 9000   7900   0 1 0
@@@O46   NSLINK_TMS_SWDIO $OSR_SYMS 9000   8000   0 1 0
@@@O47   GND $GND_SYMS 3350   8400   90 1 0
@@@O48   GND $GND_SYMS 3350   9200   90 1 0
@@@O49   GND $GND_SYMS 5500   8200   90 1 0
@@@O50   VDD_LINK $PWR_SYMS 6800   11150  0 2 0
@@@O51   GND $GND_SYMS 6600   11100  0 0 0
@@@O52   NSLINK_USART1_RX $OSR_SYMS 9000   8400   0 1 0
@@@O53   NSLINK_USART1_TX $OSR_SYMS 9000   8300   0 1 0
@@@O54   GND $GND_SYMS 5800   9800   0 0 0
@@@O55   GND $GND_SYMS 4650   8700   0 0 0
@@@O56   GND $GND_SYMS 4800   7250   0 0 0
@@@O57   GND $GND_SYMS 7600   6300   0 0 0

*TIEDOTS*



@@@D0    14350  11600 
@@@D1    14350  11500 
@@@D2    14350  11400 
@@@D3    14350  11300 
@@@D4    15200  12300 
@@@D5    15700  5200  
@@@D6    4200   8000  
@@@D7    8900   8000  
@@@D8    4000   9200  
@@@D9    4000   8400  
@@@D10   4900   8100  
@@@D11   4900   8900  
@@@D12   5800   9800  
@@@D13   6300   10600 
@@@D14   5900   10600 
@@@D15   4900   9350  
@@@D16   4900   8100  
@@@D17   7600   6900  
@@@D18   8300   9500  
@@@D19   8500   8800  

*CONNECTION*


*SIGNAL* $$$14362 64 0
R4.1         @@@D6        2 0
4050   8000  
4200   8000  
@@@D6        U4.7         4 0
4200   8000  
4400   8000  
4400   8300  
5500   8300  
@@@D6        C1.1         2 0
4200   8000  
4200   7800  

*SIGNAL* $$$32474 64 0
R17.2        U4.20        2 0
7000   6850  
7000   7000  

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        C22.1        2 0
15200  12900 
15200  12900 
J4.5         @@@D0        3 0
14150  11700 
14350  11700 
14350  11600 
J4.6         @@@D0        2 0
14150  11600 
14350  11600 
@@@D0        @@@D1        2 0
14350  11600 
14350  11500 
J4.7         @@@D1        2 0
14150  11500 
14350  11500 
@@@D1        @@@D2        2 0
14350  11500 
14350  11400 
J4.8         @@@D2        2 0
14150  11400 
14350  11400 
@@@D2        @@@D3        2 0
14350  11400 
14350  11300 
J4.9         @@@D3        2 0
14150  11300 
14350  11300 
@@@D3        @@@O3        2 0
14350  11300 
14350  11300 
@@@D5        R20.1        3 0
15700  5200  
15700  5800  
15200  5800  
@@@D5        R15.1        2 0
15700  5200  
15200  5200  
@@@D5        @@@O4        2 0
15700  5200  
15700  4950  
J10.4        @@@O11       3 0
17100  7700  
16950  7700  
16950  7650  
J5.15        @@@O22       3 0
13850  7900  
13650  7900  
13650  7800  
J5.16        @@@O23       3 0
14400  7900  
14550  7900  
14550  7800  
C1.2         @@@O29       2 0
4200   7300  
4200   7250  
@@@O37       R17.1        2 0
7000   6300  
7000   6450  
U4.35        @@@D19       2 0
8200   8800  
8500   8800  
U4.47        @@@O42       2 0
6400   9700  
6400   9900  
@@@O47       C32.1        2 0
3350   8400  
3450   8400  
C30.1        @@@O48       2 0
3450   9200  
3350   9200  
U4.8         @@@O49       2 0
5500   8200  
5500   8200  
U4.23        @@@O43       2 0
7300   7000  
7300   6800  
J12.3        @@@O51       2 0
6600   11200 
6600   11100 
C20.1        @@@D12       3 0
5900   9900  
5900   9800  
5800   9800  
@@@D12       C19.1        3 0
5800   9800  
5600   9800  
5600   9900  
@@@D12       @@@O54       2 0
5800   9800  
5800   9800  
C5.2         @@@O55       2 0
4650   8650  
4650   8700  
C9.2         @@@O56       2 0
4800   7500  
4800   7250  
C14.2        @@@O57       2 0
7600   6400  
7600   6300  
C18.2        @@@D19       2 0
8500   8900  
8500   8800  
@@@D19       @@@O41       2 0
8500   8800  
8700   8800  

*SIGNAL* $$$4465 64 0
C22.2        @@@D4        2 0
15200  12400 
15200  12300 
@@@D4        J4.1         3 0
15200  12300 
15200  12100 
14150  12100 
@@@D4        D5.2         2 0
15200  12300 
15550  12300 

*SIGNAL* $$$32494 64 0
U4.44        R18.1        2 0
6700   9700  
6700   10100 

*SIGNAL* $$$29264 64 0
R18.2        J12.2        2 0
6700   10500 
6700   11200 

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J10.1        @@@O8        3 0
17100  8000  
16950  8000  
16950  8100  
J5.1         @@@O13       3 0
13850  8600  
13650  8600  
13650  8700  
J5.2         @@@O19       3 0
14400  8600  
14550  8600  
14550  8700  
@@@O28       R4.2         2 0
3450   8000  
3650   8000  
U4.9         @@@D10       2 0
5500   8100  
4900   8100  
@@@O38       @@@D15       2 0
4900   9600  
4900   9350  
@@@O39       @@@D13       2 0
6300   10800 
6300   10600 
@@@D18       @@@O40       2 0
8300   9500  
8300   9600  
C14.1        @@@D17       2 0
7600   6900  
7600   6900  
@@@D10       R24.2        3 0
4900   8100  
4900   8000  
5050   8000  
@@@D11       @@@D16       2 0
4900   8900  
4900   8100  
@@@D11       U4.1         2 0
4900   8900  
5500   8900  
J12.1        @@@O50       2 0
6800   11200 
6800   11150 
@@@D13       @@@D14       2 0
6300   10600 
5900   10600 
C20.2        @@@D14       2 0
5900   10400 
5900   10600 
@@@D13       U4.48        2 0
6300   10600 
6300   9700  
@@@D14       C19.2        3 0
5900   10600 
5600   10600 
5600   10400 
C5.1         @@@D15       3 0
4650   9150  
4650   9350  
4900   9350  
@@@D15       @@@D11       2 0
4900   9350  
4900   8900  
C9.1         @@@D16       3 0
4800   8000  
4800   8100  
4900   8100  
@@@D16       @@@D10       2 0
4900   8100  
4900   8100  
U4.24        @@@D17       3 0
7400   7000  
7400   6900  
7600   6900  
@@@D17       @@@O44       2 0
7600   6900  
7850   6900  
@@@D18       U4.36        3 0
8300   9500  
8300   8900  
8200   8900  
@@@D18       C18.1        3 0
8300   9500  
8500   9500  
8500   9400  

*SIGNAL* DM_NSLINK 0 0
R11.2        @@@O2        2 0
15650  12000 
16450  12000 
U4.32        @@@O30       2 0
8200   8500  
9000   8500  

*SIGNAL* DP_NSLINK 0 0
R12.2        @@@O1        2 0
15650  11900 
16450  11900 
U4.33        @@@O31       2 0
8200   8600  
9000   8600  

*SIGNAL* $$$24935 64 0
J4.2         R11.1        2 0
14150  12000 
15250  12000 

*SIGNAL* $$$24997 64 0
J4.3         R12.1        2 0
14150  11900 
15250  11900 

*SIGNAL* PB0/RST 0 0
@@@O12       J5.11        2 0
13600  8100  
13850  8100  
@@@O32       U4.18        2 0
6800   6450  
6800   7000  

*SIGNAL* $$$18547 64 0
U4.25        R19.1        2 0
8200   7800  
8300   7800  

*SIGNAL* $$$26932 64 0
Y1.2         @@@D9        2 0
4000   8498  
4000   8400  
U4.6         @@@D9        2 0
5500   8400  
4000   8400  
@@@D9        C32.2        2 0
4000   8400  
3650   8400  

*SIGNAL* PA14/TCK/SWCLK 0 0
J10.3        @@@O10       2 0
17100  7800  
16900  7800  
U4.37        @@@O33       2 0
7400   9700  
7400   10100 

*SIGNAL* PA13/TMS/SWDIO 0 0
J10.2        @@@O9        2 0
17100  7900  
16900  7900  
U4.34        @@@O34       2 0
8200   8700  
9000   8700  

*SIGNAL* 5V 0 0
D5.1         @@@O7        3 0
16050  12300 
16450  12300 
16450  12450 
J5.13        @@@O20       2 0
13850  8000  
13600  8000  
J5.14        @@@O21       2 0
14400  8000  
14850  8000  

*SIGNAL* $$$26931 64 0
Y1.1         @@@D8        2 0
4000   9098  
4000   9200  
U4.5         @@@D8        4 0
5500   8500  
4400   8500  
4400   9200  
4000   9200  
@@@D8        C30.2        2 0
4000   9200  
3650   9200  

*SIGNAL* LED_RUN 0 0
D7.2         @@@O6        2 0
14100  5200  
13700  5200  
@@@O35       U4.29        2 0
9000   8200  
8200   8200  

*SIGNAL* LED_CON 0 0
D6.2         @@@O5        2 0
14100  5800  
13700  5800  
U4.42        @@@O36       2 0
6900   9700  
6900   10100 

*SIGNAL* $$$32273 64 0
D6.1         R20.2        2 0
14600  5800  
14800  5800  

*SIGNAL* $$$3902 64 0
U4.10        R24.1        2 0
5500   8000  
5450   8000  

*SIGNAL* $$$32275 64 0
D7.1         R15.2        2 0
14600  5200  
14800  5200  

*SIGNAL* NSLINK_TCK_SWCLK 0 0
J5.5         @@@O17       2 0
13850  8400  
13600  8400  
@@@O45       U4.26        2 0
9000   7900  
8200   7900  

*SIGNAL* NSLINK_TMS_SWDIO 0 0
J5.3         @@@O16       2 0
13850  8500  
13600  8500  
@@@D7        U4.27        2 0
8900   8000  
8200   8000  
R19.2        @@@D7        3 0
8700   7800  
8900   7800  
8900   8000  
@@@D7        @@@O46       2 0
8900   8000  
9000   8000  

*SIGNAL* NSLINK_USART1_TX 0 0
J5.9         @@@O26       2 0
13850  8200  
13600  8200  
U4.30        @@@O53       2 0
8200   8300  
9000   8300  

*SIGNAL* NSLINK_USART1_RX 0 0
J5.7         @@@O27       2 0
13850  8300  
13600  8300  
U4.31        @@@O52       2 0
8200   8400  
9000   8400  

*SIGNAL* NRST 0 0
@@@O18       J5.12        2 0
14850  8100  
14400  8100  

*SIGNAL* MCU_PA9/TX1 0 0
J5.8         @@@O24       2 0
14400  8300  
14850  8300  

*SIGNAL* MCU_PA10/RX1 0 0
J5.10        @@@O25       2 0
14400  8200  
14850  8200  

*SIGNAL* MCU_PA13/SWDIO 0 0
@@@O15       J5.4         2 0
14850  8500  
14400  8500  

*SIGNAL* MCU_PA14/SWDCK 0 0
@@@O14       J5.6         2 0
14850  8400  
14400  8400  

*NETNAMES*



DP_NSLINK    @@@O1        320    -40    0 0 0      0      0 3 -1 12 97 "Default Font"
DM_NSLINK    @@@O2        322    -32    0 0 0      0      0 3 -1 12 97 "Default Font"
LED_CON      @@@O5        -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
LED_RUN      @@@O6        -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
5V           @@@O7        0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O8        0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
PA13/TMS/SWDIO @@@O9        -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA14/TCK/SWCLK @@@O10       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PB0/RST      @@@O12       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O13       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O14       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O15       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
NSLINK_TMS_SWDIO @@@O16       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NSLINK_TCK_SWCLK @@@O17       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NRST         @@@O18       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O19       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
5V           @@@O20       -290   -40    0 4 0      0      0 0 -1 10 97 "Default Font"
5V           @@@O21       310    -50    0 4 0      0      0 0 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O24       360    0      0 0 0      0      90 3 -1 10 97 "Default Font"
MCU_PA10/RX1 @@@O25       360    0      0 0 0      0      90 3 -1 10 97 "Default Font"
NSLINK_USART1_TX @@@O26       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NSLINK_USART1_RX @@@O27       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O28       -400   0      0 4 0      0      0 0 -1 10 97 "Default Font"
DM_NSLINK    @@@O30       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
DP_NSLINK    @@@O31       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB0/RST      @@@O32       0      -360   90 3 0      0      90 3 -1 10 97 "Default Font"
PA14/TCK/SWCLK @@@O33       40     360    90 0 0      0      90 3 -1 10 97 "Default Font"
PA13/TMS/SWDIO @@@O34       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
LED_RUN      @@@O35       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
LED_CON      @@@O36       40     380    90 0 0      0      90 3 -1 10 97 "Default Font"
VDD_LINK     @@@O38       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O39       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O40       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O44       400    50     0 7 0      0      0 0 -1 10 97 "Default Font"
NSLINK_TCK_SWCLK @@@O45       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
NSLINK_TMS_SWDIO @@@O46       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_LINK     @@@O50       250    -200   0 4 0      0      0 0 -1 10 97 "Default Font"
NSLINK_USART1_RX @@@O52       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
NSLINK_USART1_TX @@@O53       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"

*SHT*   1 MCU -1 $$$NONE
*CAE*        GENERAL PARAMETERS FOR THE SHEET"

SCALE        7.283          Scale of window expansion
WINDOWCENTER 4164   3968    Point defining the center of the window
BITCS0       0              system status bits
BITCS1       0              system status bits
BITCS2       0              system status bits

*TEXT*       FREE TEXT

17250  7350   0   1 417  10 0 "Default Font"
8M Crystal
17600  5050   0   1 417  10 0 "Default Font"
32.768K Crystal
18050  10700  0   0 417  10 0 "Default Font"
RESET
13300  10750  0   0 417  10 0 "Default Font"
MCU WAKEUP
10000  14800  0   1 417  10 0 "Default Font"
LDO 3.3V
4350   14800  0   1 417  10 0 "Default Font"
USB  5V IN
14750  14850  0   1 417  10 0 "Default Font"
KEY
18800  14300  0   1 417  10 0 "Default Font"
LED
11600  3600   0   1 278  10 0 "Default Font"
Mechanical Hole
8950   9950   0   1 417  10 0 "Default Font"
MCU

*LINES*      LINES ITEMS

D36720           LINES    21000  2100   34  40
OPEN   2   10  255
0      0     
-5010  0     
OPEN   2   10  255
-500   0     
-500   -950  
OPEN   2   10  255
-1800  -950  
-1800  -1200 
OPEN   2   10  255
-3100  0     
-3100  -950  
OPEN   2   10  255
-3800  0     
-3800  -950  
OPEN   2   10  255
0      -950  
-5000  -950  
OPEN   2   10  255
-5000  1290  
-5000  -1200 
OPEN   2   10  255
0      800   
-5000  800   
OPEN   2   10  255
-5000  -400  
-7500  -400  
CLOSED 7   10  255
0      -1200 
0      1290  
-5000  1290  
-5000  400   
-7500  400   
-7500  -1200 
0      -1200 
OPEN   2   10  255
-5010  0     
-7500  0     
OPEN   2   10  255
-5000  -800  
-7500  -800  
OPEN   2   10  255
-6000  400   
-6000  -1200 
OPEN   2   10  255
-20000 6400  
-20500 6400  
OPEN   2   10  255
-20000 10200 
-20500 10200 
OPEN   2   10  255
-16670 14500 
-16670 14000 
OPEN   2   10  255
-13340 14500 
-13340 14000 
OPEN   2   10  255
-10010 14500 
-10010 14000 
OPEN   2   10  255
-6680  14500 
-6680  14000 
OPEN   2   10  255
500    2600  
0      2600  
OPEN   2   10  255
500    6400  
0      6400  
OPEN   2   10  255
500    10200 
0      10200 
OPEN   2   10  255
-3350  14500 
-3350  14000 
OPEN   2   10  255
-2870  13800 
-2870  12800 
OPEN   2   10  255
-470   13800 
-470   12800 
OPEN   2   10  255
-1370  13800 
-1370  12800 
OPEN   2   10  255
-3470  13400 
0      13400 
OPEN   2   10  255
-3470  13800 
0      13800 
OPEN   2   10  255
-3470  13600 
0      13600 
OPEN   2   10  255
-3470  13200 
0      13200 
OPEN   2   10  255
-3470  13000 
0      13000 
CLOSED 5   10  255
0      14000 
-3470  14000 
-3470  12800 
0      12800 
0      14000 
CLOSED 5   10  255
0      -1200 
0      14000 
-20000 14000 
-20000 -1200 
0      -1200 
OPEN   2   10  255
-20000 2600  
-20500 2600  
-2300  400    0   12 250  10 1 "Default Font"
TITLE
-300   -600   0   12 306  10 1 "Default Font"
Revision
-1470  -1060  0   8 153  10 1 "Default Font"
Sheet Number
-1220  -1050  0   8 153  10 1 "Default Font"
Number of Sheets
-2500  1050   0   12 250  10 1 "Default Font"
Company Name
-400   -200   0   0 97   10 0 "Default Font"
REV:
-3600  -200   0   0 97   10 0 "Default Font"
SIZE:
-4550  -200   0   0 97   10 0 "Default Font"
CODE:
-7460  250    0   0 97   10 0 "Default Font"
DRAWN:
-5960  250    0   0 97   10 0 "Default Font"
DATED:
-5960  -150   0   0 97   10 0 "Default Font"
DATED:
-7460  -150   0   0 97   10 0 "Default Font"
CHECKED:
-7460  -550   0   0 97   10 0 "Default Font"
QUALITY CONTROL:
-5960  -550   0   0 97   10 0 "Default Font"
DATED:
-5960  -950   0   0 97   10 0 "Default Font"
DATED:
-7460  -950   0   0 97   10 0 "Default Font"
RELEASED:
-4960  1100   0   0 97   10 0 "Default Font"
COMPANY:
-4960  600    0   0 97   10 0 "Default Font"
TITLE:
-2150  -200   0   0 97   10 0 "Default Font"
DRAWING NO:
-1750  -1100  0   0 97   10 0 "Default Font"
SHEET:     OF
-4950  -1100  0   0 97   10 0 "Default Font"
SCALE:
-2150  13850  0   0 97   10 0 "Default Font"
REVISION RECORD
-1200  13650  0   0 97   10 0 "Default Font"
APPROVED:
-2350  13650  0   0 97   10 0 "Default Font"
ECO NO:
-3250  13650  0   0 97   10 0 "Default Font"
LTR
-420   13650  0   0 97   10 0 "Default Font"
DATE:
-1700  14100  0   0 250  25 0 "Default Font"
1
-5050  14100  0   0 250  25 0 "Default Font"
2
-8350  14100  0   0 250  25 0 "Default Font"
3
-11700 14100  0   0 250  25 0 "Default Font"
4
-15000 14100  0   0 250  25 0 "Default Font"
5
-18350 14100  0   0 250  25 0 "Default Font"
6
-20250 12100  0   0 250  25 0 "Default Font"
D
-20250 8300   0   0 250  25 0 "Default Font"
C
-20250 4500   0   0 250  25 0 "Default Font"
B
-20250 650    0   0 250  25 0 "Default Font"
A
100    8350   0   0 250  25 0 "Default Font"
C
100    12050  0   0 250  25 0 "Default Font"
D
100    4500   0   0 250  25 0 "Default Font"
B
100    850    0   0 250  25 0 "Default Font"
A
D93668           LINES    16600  11200  1   0
CLOSED 5   10  0  
0      0     
0      -2900 
3900   -2900 
3900   0     
0      0     
D93669           LINES    13000  11200  1   0
CLOSED 5   10  0  
0      0     
0      -2900 
3200   -2900 
3200   0     
0      0     
DRW58281         LINES    1800   15500  1   0
CLOSED 5   10  0  
0      0     
0      -3900 
10800  -3900 
10800  0     
0      0     
D61792           LINES    1800   11200  1   0
CLOSED 5   10  0  
0      0     
0      -9600 
10800  -9600 
10800  0     
0      0     
D61863           LINES    13000  15500  1   0
CLOSED 5   10  0  
0      0     
0      -3900 
3200   -3900 
3200   0     
0      0     
D61976           LINES    16600  14700  1   0
CLOSED 5   10  0  
0      0     
0      -3100 
3900   -3100 
3900   0     
0      0     
D69201           LINES    13000  7900   1   0
CLOSED 5   10  0  
0      0     
0      -4300 
7500   -4300 
7500   0     
0      0     

*CAEDECAL*  ITEMS

PIN              34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
140 20 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-520 0 0 1 100 10 "Default Font"
*
-80 0 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    

PINB             34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
230 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
140   0    
190   0    

PCLK             33500 33180 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
200   0    
OPEN   3   10  255
200   30   
260   0    
200   -30  

PCLKB            33500 33180 97 10 97 10 4 3 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
280 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   3   10  255
200   30   
260   0    
200   -30  
OPEN   2   10  255
0     0    
140   0    
CIRCLE 2   10  255
190   0    
140   0    

PINIEB           34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
220 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   4   10  255
0     0    
200   0    
140   30   
140   0    

PINORB           34000 34000 97 10 97 10 4 2 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
130 14 0 1 100 10 "Default Font"
REF-DES
300 0 0 8 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
180   0    
CIRCLE 2   10  255
230   0    
180   0    

PINSHORT         34000 34000 97 10 97 10 4 1 0 0 0 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
-530 10 0 1 100 10 "Default Font"
*
-70 10 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
100   0    

PINVRTS          34000 34000 97 10 97 10 4 1 0 0 3 1
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
20 -80 0 0 100 10 "Default Font"
REF-DES
-20 -40 0 9 100 10 "Default Font"
PART-TYPE
-500 10 0 1 100 10 "Default Font"
*
-30 14 0 1 100 10 "Default Font"
*
OPEN   2   10  255
0     -100 
0     0    

PIN50            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.21.33
"Default Font"
"Default Font"
-820 400 0 8 93 10 "Default Font"
REF-DES
-1050 400 0 1 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-100  0    

PIN35            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.35.28
"Default Font"
"Default Font"
100 50 90 10 93 10 "Default Font"
REF-DES
100 280 90 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-70   0    

PIN60            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.06.35.28
"Default Font"
"Default Font"
100 0 0 9 93 10 "Default Font"
REF-DES
330 0 0 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-120  0    

PIN25            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.07.58.51
"Default Font"
"Default Font"
-70 0 0 8 93 10 "Default Font"
REF-DES
-300 0 0 1 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-50   0    

PIN45            32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2017.06.28.10.03.08
"Default Font"
"Default Font"
-70 0 0 9 93 10 "Default Font"
REF-DES
160 0 0 0 93 10 "Default Font"
PART-TYPE
OPEN   2   1   255
0     0    
-90   0    

PIN\H            32000 32000 90 10 80 10 2 1 0 0 0 1
TIMESTAMP 2017.09.01.03.03.49
"Default Font"
"Default Font"
60 10 0 1 100 10 "Default Font"
REF-DES
140 10 0 8 100 10 "Default Font"
PART-TYPE
OPEN   2   10  255
0     0    
50    0    

PIN100           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2018.07.02.06.46.22
"Regular Arial"
"Default Font"
280 0 0 8 93 10 "Regular Arial"
REF-DES
50 0 0 1 93 10 "Regular Arial"
PART-TYPE
OPEN   2   1   255
0     0    
-200  0    

PIN150           32000 32000 100 10 100 10 2 1 0 0 0 1
TIMESTAMP 2018.07.23.13.41.14
"Regular Arial"
"Regular Arial"
50 5200 0 8 93 10 "Regular Arial"
REF-DES
-50 5200 0 1 93 10 "Regular Arial"
PART-TYPE
OPEN   2   1   255
0     0    
-300  0    

REFIN            33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
-360 0 0 1 100 10 "Default Font"
REF-DES
-360 -20 0 3 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   7   5   255
0     0    
-100  0    
-150  -50  
-300  -50  
-300  50   
-150  50   
-100  0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFOUT           33500 33180 97 10 97 10 4 1 0 1 24 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
350 10 0 0 100 10 "Default Font"
REF-DES
350 -10 0 2 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   8   5   255
0     0    
100   0    
100   50   
250   50   
300   0    
250   -50  
100   -50  
100   0    
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

REFIN&OUT        33400 33500 97 10 97 10 2 2 0 1 0 0
TIMESTAMP 2017.09.02.09.23.32
"Default Font"
"Default Font"
100 0 0 4 97 10 "Default Font"
REF-DES
100 -100 0 6 97 10 "Default Font"
PART-TYPE
CLOSED 7   10  255
100   0    
150   50   
300   50   
350   0    
300   -50  
150   -50  
100   0    
OPEN   2   10  255
0     0    
100   0    
T0     0     0 0 0 0 0 0 0 0 0 0 
P0 0 0 0 0 0 0 0 0

GND              33500 33180 97 10 97 10 4 4 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
100 -50 0 0 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-60   -160 
60    -160 
OPEN   2   5   255
-20   -220 
20    -220 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

AGND             33500 33180 97 10 97 10 4 1 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
260 0 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   6   5   255
0     0    
0     -50  
-100  -50  
0     -200 
100   -50  
0     -50  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

CHGND            33500 33180 97 10 97 10 4 5 0 1 26 0
TIMESTAMP 1999.08.25.21.39.16
"Default Font"
"Default Font"
264 -40 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -100 
OPEN   2   5   255
-100  -100 
100   -100 
OPEN   2   5   255
-100  -100 
-150  -200 
OPEN   2   5   255
0     -100 
-50   -200 
OPEN   2   5   255
100   -100 
50    -200 
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

+5V              32000 32000 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

BUBBLE           32000 32000 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     100  
CIRCLE 2   10  255
0     100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

Y                32000 32000 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
0 300 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   3   10  255
0     0    
0     100  
-100  200  
OPEN   2   10  255
0     100  
100   200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

+12V             32000 32000 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
4 484 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     300  
COPCLS 4   5   255
0     300  
-50   150  
50    150  
0     300  
-108   356    0   0 97  10
+12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

-5V              32000 32000 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
16 -520 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-80    -388   0   0 97  10
-5V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

-12V             32000 32000 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
8 -560 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     -300 
COPCLS 4   5   255
0     -300 
50    -150 
-50   -150 
0     -300 
-116   -412   0   0 97  10
-12V
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

+5VA             32000 32000 97 10 97 10 4 2 1 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
8 468 0 4 100 10 "Default Font"
REF-DES
0 200 0 6 100 10 "Default Font"
PART-TYPE
0 100 0 6 100 10 "Default Font"
*
0 0 0 6 100 10 "Default Font"
*
OPEN   2   10  255
0     0    
0     300  
COPCLS 4   10  255
0     300  
-50   150  
50    150  
0     300  
-108   336    0   0 97  10
+5VA
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 0

VCC              33500 33180 97 10 97 10 4 2 0 1 26 0
TIMESTAMP 2017.09.30.01.30.42
"Default Font"
"Default Font"
0 250 0 4 100 10 "Default Font"
REF-DES
0 200 0 0 100 10 "Default Font"
PART-TYPE
0 100 0 0 100 10 "Default Font"
*
0 0 0 0 100 10 "Default Font"
*
OPEN   2   5   255
0     0    
0     200  
COPCLS 4   5   255
0     200  
-50   100  
50    100  
0     200  
T0     0     0 0 0 0 0 0 0 0 0 8 
P0 0 0 0 0 0 0 0 128

0402C            32000 32000 100 10 100 10 3 4 0 2 26 0
TIMESTAMP 2020.04.07.11.04.42
"Default Font"
"Default Font"
0 90 0 4 70 7 "Default Font"
REF-DES
10 -80 0 6 70 7 "Default Font"
PART-TYPE
10 -160 0 6 70 7 "Default Font"
VALUE
OPEN   2   7   255
-26   60   
-26   -60  
OPEN   2   7   255
26    60   
26    -60  
OPEN   2   7   255
-54   0    
-26   0    
OPEN   2   7   255
54    0    
26    0    
T-100  0     0 0 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192
T100   0     0 1 60 10 0 1 140 10 0 8 PIN\H
P-100 0 0 1 -100 0 0 1 192

CRYSTAL_2PIN     32000 32000 97 10 97 10 4 5 0 2 2 0
TIMESTAMP 2020.05.09.07.25.23
"Default Font"
"Default Font"
250 120 0 4 97 10 "Default Font"
REF-DES
260 -120 0 6 97 10 "Default Font"
PART-TYPE
240 -296 0 6 97 10 "Default Font"
*
240 -396 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
200   100  
200   -100 
300   -100 
300   100  
200   100  
OPEN   2   10  255
168   72   
168   -72  
OPEN   2   10  255
336   72   
336   -72  
OPEN   2   10  255
144   0    
168   0    
OPEN   2   10  255
336   0    
360   0    
T-48   0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T552   0     0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CAP              32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2019.11.28.11.16.25
"Default Font"
"Default Font"
150 -210 0 0 100 10 "Default Font"
REF-DES
210 -40 0 2 100 10 "Default Font"
PART-TYPE
150 -240 0 2 100 10 "Default Font"
VALUE
150 -340 0 2 100 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -300 
0     -500 
T0     0     0 0 20 -90 0 0 -20 -40 0 9 PINVRTS
P-110 -140 0 1 0 0 0 0 128
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-110 -130 0 1 0 0 0 0 128

OSC-2P           32000 32000 97 10 97 10 4 5 0 2 16 0
TIMESTAMP 2018.09.07.06.27.59
"Default Font"
"Default Font"
350 -100 0 4 97 10 "Default Font"
REF-DES
450 -330 0 6 97 10 "Default Font"
PART-TYPE
450 -430 0 6 97 10 "Default Font"
*
450 -530 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     -130 
0     -270 
200   -270 
200   -130 
0     -130 
OPEN   2   10  255
0     -100 
200   -100 
OPEN   2   10  255
0     -300 
0     -300 
OPEN   2   10  255
0     -300 
0     -300 
OPEN   2   10  255
0     -300 
200   -300 
T100   0     90 2 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T100   -400  90 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

LED              32000 32000 90 10 80 10 4 8 0 2 18 0
TIMESTAMP 2019.02.01.02.46.48
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
OPEN   2   10  255
250   150  
350   250  
COPCLS 5   10  255
350   250  
290   230  
320   190  
330   180  
350   250  
OPEN   2   10  255
350   150  
450   250  
COPCLS 5   10  255
460   260  
400   240  
430   200  
440   190  
460   260  
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 0 0 0 0 128

SW_2P            32000 32000 97 10 97 10 4 6 0 2 16 0
TIMESTAMP 2019.01.05.10.52.59
"Default Font"
"Default Font"
0 100 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
0 -200 0 6 97 10 "Default Font"
*
0 -300 0 6 97 10 "Default Font"
*
OPEN   2   20  255
-150  40   
150   40   
OPEN   2   30  255
-80   60   
80    60   
CIRCLE 2   10  255
-60   0    
-100  0    
CIRCLE 2   10  255
100   0    
60    0    
OPEN   2   10  255
80    0    
200   0    
OPEN   2   10  255
-80   0    
-200  0    
T-200  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T200   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

R0402            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2017.02.17.18.25.55
"Default Font"
"Default Font"
70 -90 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     80   
0     20   
200   20   
200   80   
0     80   
T-100  50    0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   50    0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

CAPA             32000 32000 100 10 100 10 4 4 0 2 26 0
TIMESTAMP 2020.05.12.00.28.05
"Default Font"
"Default Font"
180 -210 0 0 83 10 "Default Font"
REF-DES
240 -30 0 2 100 10 "Default Font"
PART-TYPE
180 -250 0 2 83 10 "Default Font"
VALUE
180 -360 0 2 83 10 "Default Font"
*
OPEN   2   10  255
0     -200 
0     -50  
OPEN   2   1   255
-100  -200 
100   -200 
OPEN   2   1   255
-100  -300 
100   -300 
OPEN   2   10  255
0     -450 
0     -300 
T0     0     0 0 20 -80 0 0 -20 -40 0 9 PINVRTS
P-76 -112 0 1 -30 14 0 1 0
T0     -500  0 2 20 -80 0 0 -20 -40 0 9 PINVRTS
P-72 -136 0 1 -30 14 0 1 0

BAT_3V           32000 32000 97 10 97 10 4 4 0 2 2 0
TIMESTAMP 2019.10.10.11.12.20
"Default Font"
"Default Font"
0 0 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
0 -200 0 6 97 10 "Default Font"
*
0 -300 0 6 97 10 "Default Font"
*
OPEN   2   10  255
100   0    
100   -200 
OPEN   2   10  255
0     80   
0     -290 
OPEN   2   10  255
300   0    
300   -200 
OPEN   2   10  255
200   80   
200   -290 
T-200  -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T500   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CON_MINIUSB      32000 32000 100 10 100 10 4 1 0 11 0 0
TIMESTAMP 2019.12.11.09.21.40
"Default Font"
"Default Font"
80 1260 0 4 100 10 "Default Font"
REF-DES
290 -40 0 6 100 10 "Default Font"
PART-TYPE
340 -150 0 6 100 10 "Default Font"
*
350 -270 0 6 100 10 "Default Font"
*
OPEN   5   10  255
0     0    
0     1200 
500   1200 
500   0    
0     0    
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

CONDIP2_A        32000 32000 97 10 97 10 4 1 0 2 18 0
TIMESTAMP 2019.11.20.07.32.26
"Default Font"
"Default Font"
-80 0 90 4 97 10 "Default Font"
REF-DES
0 -300 0 6 97 10 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 "Default Font"
*
-350 -150 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
-50   100  
-50   -100 
50    -100 
50    100  
-50   100  
T0     200   90 2 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0
T0     -200  90 0 100 0 0 1 230 0 0 8 PINB
P-520 0 0 1 -80 0 0 1 0

SPX1117-3V3      32000 32000 97 10 97 10 4 1 0 4 0 0
TIMESTAMP 2019.12.11.09.57.22
"Default Font"
"Default Font"
200 100 0 4 97 10 "Default Font"
REF-DES
200 -500 0 6 97 10 "Default Font"
PART-TYPE
200 -600 0 6 97 10 "Default Font"
*
200 -700 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
0     -400 
400   -400 
400   0    
0     0    
T-200  -300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  -100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

DIODE            32000 32000 90 10 80 10 4 4 0 2 18 0
TIMESTAMP 2019.12.01.15.48.44
"Default Font"
"Default Font"
100 200 0 4 100 10 "Default Font"
REF-DES
250 -150 0 6 100 10 "Default Font"
PART-TYPE
250 -250 0 6 100 10 "Default Font"
*
250 -350 0 6 100 10 "Default Font"
*
OPEN   2   10  255
90    0    
390   0    
OPEN   2   10  255
340   90   
340   -90  
COPCLS 4   10  255
190   0    
190   -90  
340   0    
190   0    
COPCLS 4   10  255
190   0    
190   90   
340   0    
190   0    
T500   0     0 1 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0
T0     0     0 0 130 14 0 1 170 -30 0 8 PINSHORT
P-500 10 0 1 -70 10 0 1 0

0201R            32000 32000 97 10 97 10 4 1 0 2 26 0
TIMESTAMP 2018.02.11.07.24.24
"Default Font"
"Default Font"
370 -200 0 4 97 10 "Default Font"
REF-DES
0 -100 0 6 97 10 "Default Font"
PART-TYPE
80 -210 0 6 97 10 "Default Font"
*
80 -310 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     30   
0     -30  
200   -30  
200   30   
0     30   
T-100  0     0 0 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0
T300   0     0 1 60 10 0 1 140 10 0 8 PINSHORT
P-530 10 0 1 -70 10 0 1 0

THOU             32000 32000 97 10 97 10 4 1 0 1 18 0
TIMESTAMP 2019.01.10.03.45.45
"Default Font"
"Default Font"
0 200 0 4 97 10 "Default Font"
REF-DES
0 -200 0 6 97 10 "Default Font"
PART-TYPE
0 -300 0 6 97 10 "Default Font"
*
0 -400 0 6 97 10 "Default Font"
*
CIRCLE 2   10  255
-100  100  
100   -100 
T-200  0     0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

N32G4XC          32000 32000 97 10 97 10 4 1 0 48 2 0
TIMESTAMP 2020.05.13.07.13.06
"Default Font"
"Default Font"
2300 2340 0 0 97 10 "Default Font"
REF-DES
2300 -40 0 2 97 10 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 "Default Font"
*
2300 -240 0 2 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
2300  0    
2300  2300 
0     2300 
0     0    
T-200  1700  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1600  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1500  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  -200  90 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1500  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1600  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T2500  1700  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1700  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1600  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1500  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1400  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1300  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1200  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1100  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T1000  2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T900   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T800   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T700   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T600   2500  90 2 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0

HEAD2X14         32000 32000 97 10 97 10 4 1 0 28 0 0
TIMESTAMP 2019.12.01.07.42.10
"Default Font"
"Default Font"
200 1540 0 4 97 10 "Default Font"
REF-DES
200 -40 0 6 97 10 "Default Font"
PART-TYPE
200 -140 0 6 97 10 "Default Font"
*
200 -240 0 6 97 10 "Default Font"
*
CLOSED 5   10  255
0     0    
200   0    
200   1500 
0     1500 
0     0    
T-200  1400  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1400  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1300  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1300  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1200  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1200  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1100  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1100  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  1000  0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   1000  0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  900   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   900   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  800   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   800   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  700   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   700   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  600   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   600   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  500   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   500   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  400   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   400   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  300   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   300   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  200   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   200   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T-200  100   0 0 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0
T400   100   0 1 140 20 0 1 230 0 0 8 PIN
P-520 0 0 1 -80 0 0 1 0


*PARTTYPE*   ITEMS

$OSR_SYMS UND  0   0   2     0
TIMESTAMP 2017.09.02.09.23.38
OFF 3
REFIN S 
REFOUT L 
REFIN&OUT B 

$GND_SYMS UND  0   0   2     0
TIMESTAMP 1999.03.30.22.52.06
GND 3
GND G GND
AGND G AGND
CHGND G CHGND

$PWR_SYMS UND  0   0   2     0
TIMESTAMP 2017.09.30.01.30.42
PWR 8
+5V P +5V
BUBBLE P +5V
Y P +5V
+12V P +12V
-5V P -5V
-12V P -12V
+5VA P +5VA
VCC P +3.3V

CRYSTAL_2PIN OSC  1   0   0     0
TIMESTAMP 2020.05.09.07.25.23
GATE 1 2 0
CRYSTAL_2PIN
1 0 U
2 0 U

C0603 CAP  1   0   0     0
TIMESTAMP 2019.11.28.11.16.24
GATE 1 2 0
CAP
1 1 U
2 1 U

OSC-2P UND  1   0   0     0
TIMESTAMP 2018.09.07.06.27.58
GATE 1 2 0
OSC-2P
1 0 U
2 0 U

LED0805 DIO  1   0   0     2
TIMESTAMP 2019.02.01.02.46.45
GATE 1 2 0
LED
1 0 U
2 0 U
1 2 

SW_2P UND  1   0   0     2
TIMESTAMP 2019.01.05.10.52.56
GATE 1 2 0
SW_2P
1 0 U
2 0 U
1 2 

R0402 RES  1   0   0     0
TIMESTAMP 2017.02.17.18.25.55
GATE 1 2 0
R0402
1 0 U
2 0 U

CAP1206 CAP  1   0   0     0
TIMESTAMP 2020.05.12.00.28.04
GATE 1 2 0
CAPA
1 1 U
2 1 U

BAT_3V UND  1   0   0     0
TIMESTAMP 2019.10.10.11.12.18
GATE 1 2 0
BAT_3V
1 0 U +
2 0 U -

CONDIP2_A CON  1   0   0     2
TIMESTAMP 2019.11.20.07.32.25
GATE 1 2 0
CONDIP2_A
1 0 U
2 0 U
1 2 

DIODE_2 UND  1   0   0     0
TIMESTAMP 2019.12.01.15.48.43
GATE 1 2 0
DIODE
1 0 U
2 0 U

MINIUSB CON  1   0   0     0
TIMESTAMP 2019.12.11.09.21.39
GATE 1 11 0
CON_MINIUSB
1 0 U VBUS
2 0 U D-
3 0 U D+
4 0 U ID
5 0 U GND
6 0 U SHIELD1
7 0 U SHIELD2
8 0 U SHIELD3
9 0 U SHIELD4
10 0 U H1
11 0 U H2

AMS1117-3.3 UND  1   0   0     0
TIMESTAMP 2019.12.11.09.57.22
GATE 1 4 0
SPX1117-3V3
1 0 U GND
2 0 U OUT
3 0 U IN
4 0 U OUT

0402C CAP  1   0   0     0
TIMESTAMP 2020.04.07.11.04.41
GATE 1 2 0
0402C
1 0 U
2 0 U

0201R RES  1   0   0     0
TIMESTAMP 2018.02.11.07.24.23
GATE 1 2 0
0201R
1 0 U
2 0 U

THOU UND  1   0   0     0
TIMESTAMP 2019.01.10.03.45.44
GATE 1 1 0
THOU
1 0 U

N32G4XC UND  1   0   0     0
TIMESTAMP 2020.05.13.07.13.05
GATE 1 48 0
N32G4XC
1 0 U VBAT
2 0 U PC13-TAMPER-RTC
3 0 U PC14-OSC32_IN
4 0 U PC15-OSC32_OUT
5 0 U PD0-OSC_IN
6 0 U PD1-OSC_OUT
7 0 U NRST
8 0 U VSSA
9 0 U VDDA
10 0 U PA0-WKUP
11 0 U PA1
12 0 U PA2
13 0 U PA3
14 0 U PA4
15 0 U PA5
16 0 U PA6
17 0 U PA7
18 0 U PB0
19 0 U PB1
20 0 U PB2-BOOT
21 0 U PB10
22 0 U PB11
23 0 U VSS_1
24 0 U VDD_1
25 0 U PB12
26 0 U PB13
27 0 U PB14
28 0 U PB15
29 0 U PA8
30 0 U PA9
31 0 U PA10
32 0 U PA11
33 0 U PA12
34 0 U PA13-SWDIO
35 0 U VSS_2
36 0 U VDD_2
37 0 U PA14-SWCLK
38 0 U PA15
39 0 U PB3
40 0 U PB4
41 0 U PB5
42 0 U PB6
43 0 U PB7
44 0 U BOOT0
45 0 U PB8
46 0 U PB9
47 0 U VSS_3
48 0 U VDD_3

HEAD2X14 UND  1   0   0     0
TIMESTAMP 2019.12.01.07.42.09
GATE 1 28 0
HEAD2X14
1 0 L
2 0 L
3 0 L
4 0 L
5 0 L
6 0 L
7 0 L
8 0 L
9 0 L
10 0 L
11 0 L
12 0 L
13 0 L
14 0 L
15 0 L
16 0 L
17 0 L
18 0 L
19 0 L
20 0 L
21 0 L
22 0 L
23 0 L
24 0 L
25 0 L
26 0 L
27 0 L
28 0 L



*PART*       ITEMS



C6           0402C            16800 6350   90 1 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C8           0402C            16000 6350   90 1 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 12pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

Y5           OSC-2P           16600 4650   90 3 97 10 97 10 4 2 2 0 0 2
"Default Font"
"Default Font"
-50 -200 90 4 97 10 0 "Default Font"
REF-DES
270 -320 0 6 97 10 0 "Default Font"
PART-TYPE
250 -200 90 5 97 10 1 "Default Font"
VALUE
450 -530 0 6 97 10 0 "Default Font"
*
"PCB DECAL" XTL741
"VALUE" 32.768K
0 60 10 0 1
1 60 10 0 1

D1           LED0805          17800 13200  90 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

D2           LED0805          18500 13200  90 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

C3           0402C            16000 4250   90 1 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 10pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

C4           0402C            16800 4250   90 1 97 10 97 10 3 22 2 0 0 26
"Default Font"
"Default Font"
0 90 0 4 97 7 0 "Default Font"
REF-DES
10 -80 0 6 97 7 0 "Default Font"
PART-TYPE
10 -160 0 6 97 7 3 "Default Font"
Value
"MPN" 
"DESC" 
"MFR" 
"PACKAGE" 
"FOOTPRINT" 
"TOL" 
"ZTEPN" 
"MFG #1" 
"PART NB" 
"DECAL" 
"ASSEMBLY" SMT
"Voltage Rating" 
"Sim.Analog.Model" 
"Sim.Analog.Order" Model$
"Sim.Analog.Prefix" 
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT CAPACITOR 0.031 X 0.061 INCHES
"Part Number" 
"Tolerance" 
"Value" 10pF
"PCB DECAL" C0402
0 60 10 0 1
1 60 10 0 1

D3           LED0805          19200 13200  90 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
150 200 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

S7           SW_2P            18850 9600    0 0 97 10 97 10 4 1 2 0 0 16
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

S6           SW_2P            15150 9850   90 0 97 10 97 10 4 1 2 0 0 16
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R8           R0402            18450 10200  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R9           R0402            15200 9100   90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S1           SW_2P            14300 13200  90 0 97 10 97 10 4 1 2 0 0 16
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R6           R0402            14350 12550  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S2           SW_2P            14700 13200  90 0 97 10 97 10 4 1 2 0 0 16
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R7           R0402            14750 12550  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

S3           SW_2P            15100 13200  90 0 97 10 97 10 4 1 2 0 0 16
"Default Font"
"Default Font"
0 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SKPM
0 60 10 0 1
1 60 10 0 1

R10          R0402            15150 12550  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 10K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

C31          CAP1206          10000 13400   0 0 97 10 97 10 4 15 2 0 0 26
"Default Font"
"Default Font"
-150 -150 0 0 97 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Default Font"
PART-TYPE
-200 -350 0 2 97 10 3 "Default Font"
Value
180 -360 0 2 97 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

C7           CAP1206          8000  13450   0 0 97 10 97 10 4 15 2 0 0 26
"Default Font"
"Default Font"
-150 -150 0 0 97 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Default Font"
PART-TYPE
-200 -350 0 2 97 10 3 "Default Font"
Value
180 -360 0 2 97 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

B1           BAT_3V           5150  7400   90 3 97 10 97 10 4 1 2 0 0 2
"Default Font"
"Default Font"
150 250 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
0 -200 0 6 97 10 0 "Default Font"
*
0 -300 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CR1220
0 140 20 0 1
1 140 20 0 1

J3           MINIUSB          3000  12500   0 1 97 10 97 10 4 3 11 0 0 0
"Default Font"
"Default Font"
300 1250 0 4 97 10 0 "Default Font"
REF-DES
290 -40 0 6 97 10 0 "Default Font"
PART-TYPE
340 -150 0 6 97 10 0 "Default Font"
*
350 -270 0 6 97 10 0 "Default Font"
*
"DECAL" 
"Description" 6 pin header
"PCB DECAL" CON_MINIUSB
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1

J15          CONDIP2_A        11500 13600  90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R13          R0402            3950  13450   0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 100 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 100 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R14          R0402            3950  13350   0 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -50 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
250 50 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 33R
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

D4           LED0805          10850 13350  90 2 97 10 97 10 4 1 2 0 0 18
"Default Font"
"Default Font"
100 -100 90 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -250 0 6 97 10 0 "Default Font"
*
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" 0805-LED
0 130 14 0 1
1 130 14 0 1

U1           AMS1117-3.3      8950  13700   0 0 97 10 97 10 4 1 4 0 0 0
"Default Font"
"Default Font"
200 100 0 4 97 10 0 "Default Font"
REF-DES
200 -500 0 6 97 10 0 "Default Font"
PART-TYPE
200 -600 0 6 97 10 0 "Default Font"
*
200 -700 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SOT223
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1

D10          DIODE_2          6250  13600   0 0 97 10 97 10 4 2 2 0 0 18
"Default Font"
"Default Font"
250 150 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -150 0 6 97 10 1 "Default Font"
VALUE
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SOD123
"VALUE" SS14L
0 130 14 0 1
1 130 14 0 1

J6           CONDIP2_A        7450  13600  90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

R1           R0402            17850 12500  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R2           R0402            18550 12500  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R3           R0402            19250 12500  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R5           R0402            10900 12600  90 2 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
150 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 1K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R16          R0402            5850  13150  90 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
150 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-50 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 220K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

R21          R0402            5850  12250  90 0 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
150 150 90 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-50 150 90 5 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Manufacturer #1" IPC SM-782 STD.
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Part Number" 
"Tolerance" 
"Value" 330K
"PCB DECAL" R0402
0 60 10 0 1
1 60 10 0 1

J8           CONDIP2_A        11500 13250  90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

D8           DIODE_2          5250  7800    0 0 97 10 97 10 4 2 2 0 0 18
"Default Font"
"Default Font"
250 150 0 4 97 10 0 "Default Font"
REF-DES
250 -150 0 6 97 10 0 "Default Font"
PART-TYPE
250 -150 0 6 97 10 1 "Default Font"
VALUE
250 -350 0 6 97 10 0 "Default Font"
*
"PCB DECAL" SOD123
"VALUE" SS14L
0 130 14 0 1
1 130 14 0 1

J7           CONDIP2_A        6300  12750  90 1 97 10 97 10 4 3 2 0 0 18
"Default Font"
"Default Font"
-80 0 90 4 97 10 0 "Default Font"
REF-DES
0 -300 0 6 97 10 0 "Default Font"
PART-TYPE
-350 -50 0 6 97 10 0 "Default Font"
*
-350 -150 0 6 97 10 0 "Default Font"
*
"PCB DECAL" CON_254_2P
"Value" 
"Description" Rechargeable Battery
0 100 0 0 1
1 100 0 0 1

Y2           CRYSTAL_2PIN     16650 6650    0 3 97 10 97 10 4 2 2 0 0 2
"Default Font"
"Default Font"
250 120 0 4 97 10 0 "Default Font"
REF-DES
260 -120 0 6 97 10 0 "Default Font"
PART-TYPE
240 -296 0 6 97 10 0 "Default Font"
Value
240 -396 0 6 97 10 0 "Default Font"
*
"Value" 8MHz (AV08000301) 12pF
"PCB DECAL" SMD3225
0 140 20 0 1
1 140 20 0 1

R25          0201R            15450 4550    0 3 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-60 -30 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

R26          0201R            17500 4550    0 3 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-60 -30 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

C37          C0603            18400 9400    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
150 -210 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
150 -240 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C2           C0603            8400  13450   0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
100 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C11          C0603            10350 13400   0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
150 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
150 -200 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C10          CAP1206          3500  14200   0 0 97 10 97 10 4 15 2 0 0 26
"Default Font"
"Default Font"
180 -210 0 0 97 10 0 "Default Font"
REF-DES
240 -30 0 2 97 10 0 "Default Font"
PART-TYPE
180 -250 0 2 97 10 3 "Default Font"
Value
180 -360 0 2 97 10 0 "Default Font"
*
"Sim.Analog.Prefix" 
"Sim.Analog.Order" Model$
"Sim.Analog.Model" 
"Voltage Rating" 6.3V
"Tolerance" 
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Description" SURFACE MOUNT CAPACITOR 0.080 X 0.180 INCHES
"ASSEMBLY" SMT
"DECAL" O805,0805MIL
"PART NB" 
"MFG #1" 
"Value" 10uF
"PART DESC" SURFACE MOUNT CAPACITOR 0.048 X 0.079 INCHES
"PCB DECAL" C0805
0 20 -80 0 0
1 20 -80 0 0

C12          C0603            5900  7300    0 3 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
-250 -400 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
-300 -100 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

TH1          THOU             10862 3300    0 0 97 10 97 10 4 1 1 0 0 18
"Default Font"
"Default Font"
238 -50 0 4 97 10 0 "Default Font"
REF-DES
0 -200 0 6 97 10 0 "Default Font"
PART-TYPE
0 -300 0 6 97 10 0 "Default Font"
*
0 -400 0 6 97 10 0 "Default Font"
*
"PCB DECAL" THOU_40_30
0 140 20 0 1

TH2          THOU             10862 3000    0 0 97 10 97 10 4 1 1 0 0 18
"Default Font"
"Default Font"
238 0 0 4 97 10 0 "Default Font"
REF-DES
0 -200 0 6 97 10 0 "Default Font"
PART-TYPE
0 -300 0 6 97 10 0 "Default Font"
*
0 -400 0 6 97 10 0 "Default Font"
*
"PCB DECAL" THOU_40_30
0 140 20 0 1

TH3          THOU             10862 2700    0 0 97 10 97 10 4 1 1 0 0 18
"Default Font"
"Default Font"
238 -50 0 4 97 10 0 "Default Font"
REF-DES
0 -200 0 6 97 10 0 "Default Font"
PART-TYPE
0 -300 0 6 97 10 0 "Default Font"
*
0 -400 0 6 97 10 0 "Default Font"
*
"PCB DECAL" THOU_40_30
0 140 20 0 1

TH4          THOU             10862 2400    0 0 97 10 97 10 4 1 1 0 0 18
"Default Font"
"Default Font"
288 -50 0 4 97 10 0 "Default Font"
REF-DES
0 -200 0 6 97 10 0 "Default Font"
PART-TYPE
0 -300 0 6 97 10 0 "Default Font"
*
0 -400 0 6 97 10 0 "Default Font"
*
"PCB DECAL" THOU_40_30
0 140 20 0 1

C52          C0603            6200  6900    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
0 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
0 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C53          C0603            9500  5800    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
100 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
100 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C54          C0603            11500 7700    0 0 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
100 -150 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
100 -350 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C50          C0603            7500  8700    0 3 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
50 -450 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
50 -50 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 4.7uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

C51          C0603            7800  8700    0 3 97 10 97 10 4 4 2 0 0 26
"Default Font"
"Default Font"
-200 -450 0 0 97 10 0 "Default Font"
REF-DES
210 -40 0 2 97 10 0 "Default Font"
PART-TYPE
-250 -50 0 2 97 10 3 "Default Font"
Value
150 -340 0 2 97 10 0 "Default Font"
*
"Voltage Rating" 
"Part Number" 
"Value" 0.1uF
"PCB DECAL" C0603
0 20 -90 0 0
1 20 -80 0 0

U3           N32G4XC          7500  6100    0 0 97 10 97 10 4 2 48 0 0 2
"Default Font"
"Default Font"
2300 2340 0 0 97 10 0 "Default Font"
REF-DES
2300 -40 0 2 97 10 0 "Default Font"
PART-TYPE
2300 -140 0 2 97 10 0 "Default Font"
PCB DECAL
2200 -150 0 2 97 10 1 "Default Font"
VALUE
"PCB DECAL" QFP48-3
"VALUE" N32G455CCL7
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1
28 140 20 0 1
29 140 20 0 1
30 140 20 0 1
31 140 20 0 1
32 140 20 0 1
33 140 20 0 1
34 140 20 0 1
35 140 20 0 1
36 140 20 0 1
37 140 20 0 1
38 140 20 0 1
39 140 20 0 1
40 140 20 0 1
41 140 20 0 1
42 140 20 0 1
43 140 20 0 1
44 140 20 0 1
45 140 20 0 1
46 140 20 0 1
47 140 20 0 1

J2           HEAD2X14         3300  5300    0 0 97 10 97 10 4 1 28 0 0 0
"Default Font"
"Default Font"
100 1550 0 4 97 10 0 "Default Font"
REF-DES
100 -50 0 6 97 10 0 "Default Font"
PART-TYPE
200 -140 0 6 97 10 0 "Default Font"
*
200 -240 0 6 97 10 0 "Default Font"
*
"PCB DECAL" HEAD2X14
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1

R22          0201R            15600 6650    0 3 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-60 -30 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

R23          0201R            17450 6650    0 3 97 10 97 10 4 9 2 0 0 26
"Default Font"
"Default Font"
100 -120 0 4 97 10 0 "Default Font"
REF-DES
0 -100 0 6 97 10 0 "Default Font"
PART-TYPE
-60 -30 0 6 97 10 1 "Default Font"
Value
80 -310 0 6 97 10 0 "Default Font"
*
"Description" SURFACE MOUNT RESISTOR 0.031 X 0.061 INCHES, 1/10W
"Manufacturer #1" IPC SM-782 STD.
"Part Number" 
"Sim.Analog.Model" 
"Sim.Analog.Order" 
"Sim.Analog.Prefix" R
"Tolerance" 
"Value" 0R
"PCB DECAL" 0201R
0 60 10 0 1
1 60 10 0 1

J1           HEAD2X14         3300  7600    0 0 97 10 97 10 4 1 28 0 0 0
"Default Font"
"Default Font"
100 1550 0 4 97 10 0 "Default Font"
REF-DES
100 -50 0 6 97 10 0 "Default Font"
PART-TYPE
200 -140 0 6 97 10 0 "Default Font"
*
200 -240 0 6 97 10 0 "Default Font"
*
"PCB DECAL" HEAD2X14
0 140 20 0 1
1 140 20 0 1
2 140 20 0 1
3 140 20 0 1
4 140 20 0 1
5 140 20 0 1
6 140 20 0 1
7 140 20 0 1
8 140 20 0 1
9 140 20 0 1
10 140 20 0 1
11 140 20 0 1
12 140 20 0 1
13 140 20 0 1
14 140 20 0 1
15 140 20 0 1
16 140 20 0 1
17 140 20 0 1
18 140 20 0 1
19 140 20 0 1
20 140 20 0 1
21 140 20 0 1
22 140 20 0 1
23 140 20 0 1
24 140 20 0 1
25 140 20 0 1
26 140 20 0 1
27 140 20 0 1


*BUSSES*


*OFFPAGE REFS*



@@@O0    GND $GND_SYMS 16400  6050   0 0 0
@@@O1    PC14 $OSR_SYMS 15100  4550   0 2 0
@@@O2    PC15 $OSR_SYMS 17800  4550   0 3 0
@@@O3    GND $GND_SYMS 16400  3850   0 0 0
@@@O4    PA8 $OSR_SYMS 17800  13400  90 2 0
@@@O5    PB4 $OSR_SYMS 18500  13400  90 2 0
@@@O6    PB5 $OSR_SYMS 19200  13400  90 2 0
@@@O7    GND $GND_SYMS 17800  12000  0 0 0
@@@O8    GND $GND_SYMS 18500  12000  0 0 0
@@@O9    GND $GND_SYMS 19200  12000  0 0 0
@@@O10   GND $GND_SYMS 19300  9300   0 0 0
@@@O11   GND $GND_SYMS 18400  8850   0 0 0
@@@O12   VDD_MCU $PWR_SYMS 18400  10450  0 0 0
@@@O13   NRST $OSR_SYMS 17800  9600   0 1 1
@@@O14   VDD_MCU $PWR_SYMS 15150  10300  0 0 0
@@@O15   GND $GND_SYMS 15150  8650   0 0 0
@@@O16   PA0_WKUP $OSR_SYMS 14750  9500   0 0 0
@@@O17   GND $GND_SYMS 14300  12000  0 0 0
@@@O18   GND $GND_SYMS 14700  12000  0 0 0
@@@O19   GND $GND_SYMS 15100  12000  0 0 0
@@@O20   PA4 $OSR_SYMS 14300  13700  0 0 0
@@@O21   PA5 $OSR_SYMS 14300  14000  0 0 0
@@@O22   PA6 $OSR_SYMS 14300  14300  0 0 0
@@@O23   GND $GND_SYMS 8200   12650  0 0 0
@@@O24   GND $GND_SYMS 10850  12100  0 0 0
@@@O25   GND $GND_SYMS 10100  12600  0 0 0
@@@O26   GND $GND_SYMS 5050   6700   0 1 0
@@@O27   GND $GND_SYMS 3500   14300  0 2 0
@@@O28   PA12/USBDP $OSR_SYMS 4500   13400  0 1 0
@@@O29   PA11/USBDM $OSR_SYMS 4500   13500  0 1 0
@@@O30   PA0_WKUP $OSR_SYMS 6700   12750  0 1 0
@@@O31   GND $GND_SYMS 5800   11950  0 0 0
@@@O32   GND $GND_SYMS 3400   12800  0 0 0
@@@O33   GND $GND_SYMS 8750   13200  0 0 0
@@@O34   VDD_MCU $PWR_SYMS 11800  13600  90 1 0
@@@O35   5V $PWR_SYMS 7000   13900  0 0 0
@@@O36   VDD_LINK $PWR_SYMS 11800  13250  90 1 0
@@@O37   PA11 $OSR_SYMS 4500   13200  0 1 0
@@@O38   PA12 $OSR_SYMS 4500   13100  0 1 0
@@@O39   OSC_OUT $OSR_SYMS 15200  7000   0 0 0
@@@O40   OSC_IN $OSR_SYMS 17600  7000   0 1 0
@@@O41   OSC32_IN $OSR_SYMS 15100  4850   0 0 0
@@@O42   OSC32_OUT $OSR_SYMS 17800  4850   0 1 0
@@@O43   GND $GND_SYMS 10450  2200   0 0 0
@@@O44   PC13 $OSR_SYMS 2800   8700   0 0 0
@@@O45   PA0_WKUP $OSR_SYMS 4000   8500   0 1 0
@@@O46   PA1 $OSR_SYMS 2800   8400   0 0 0
@@@O47   PC14 $OSR_SYMS 4000   8700   0 1 0
@@@O48   PC15 $OSR_SYMS 2800   8600   0 0 0
@@@O49   PA2 $OSR_SYMS 4000   8400   0 1 0
@@@O50   PA3 $OSR_SYMS 2800   8300   0 0 0
@@@O51   PA4 $OSR_SYMS 4000   8300   0 1 0
@@@O52   PA5 $OSR_SYMS 2800   8200   0 0 0
@@@O53   PA6 $OSR_SYMS 4000   8200   0 1 0
@@@O54   PA7 $OSR_SYMS 2800   8100   0 0 0
@@@O55   PB0 $OSR_SYMS 4000   8100   0 1 0
@@@O56   PB1 $OSR_SYMS 2800   8000   0 0 0
@@@O57   PB10 $OSR_SYMS 2800   7900   0 0 0
@@@O58   PB11 $OSR_SYMS 4000   7900   0 1 0
@@@O59   PB15 $OSR_SYMS 4000   6300   0 3 0
@@@O60   PB14 $OSR_SYMS 2800   6400   0 2 0
@@@O61   PB13 $OSR_SYMS 4000   6400   0 3 0
@@@O62   PB12 $OSR_SYMS 2800   6500   0 2 0
@@@O63   MCU_PA10/RX1 $OSR_SYMS 2800   6200   0 2 0
@@@O64   MCU_PA9/TX1 $OSR_SYMS 4000   6200   0 3 0
@@@O65   PA8 $OSR_SYMS 2800   6300   0 2 0
@@@O66   MCU_PA13/SWDIO $OSR_SYMS 4000   6100   0 1 0
@@@O67   PA15 $OSR_SYMS 4000   6000   0 3 0
@@@O68   MCU_PA14/SWDCK $OSR_SYMS 2800   6100   0 2 0
@@@O69   PB3 $OSR_SYMS 2800   6000   0 2 0
@@@O70   PB8 $OSR_SYMS 4000   5700   0 3 0
@@@O71   PB7 $OSR_SYMS 2800   5800   0 2 0
@@@O72   PB6 $OSR_SYMS 4000   5800   0 3 0
@@@O73   PB5 $OSR_SYMS 2800   5900   0 2 0
@@@O74   PB9 $OSR_SYMS 2800   5700   0 2 0
@@@O75   PB4 $OSR_SYMS 4000   5900   0 3 0
@@@O76   VDD_MCU $PWR_SYMS 3900   5500   90 1 0
@@@O77   VDD_MCU $PWR_SYMS 2900   5500   90 0 0
@@@O78   PB2/BOOT1 $OSR_SYMS 4000   8000   0 1 0
@@@O79   VDD_MCU $PWR_SYMS 3900   9000   90 1 0
@@@O80   VDD_MCU $PWR_SYMS 3900   8900   90 1 0
@@@O81   VDD_MCU $PWR_SYMS 2900   9000   90 0 0
@@@O82   VDD_MCU $PWR_SYMS 2900   8900   90 0 0
@@@O83   GND $GND_SYMS 2900   7800   90 1 0
@@@O84   GND $GND_SYMS 2900   7700   90 1 0
@@@O85   GND $GND_SYMS 3900   7800   90 0 0
@@@O86   GND $GND_SYMS 3900   7700   90 0 0
@@@O87   PC13 $OSR_SYMS 7000   7700   0 0 0
@@@O88   OSC_IN $OSR_SYMS 7000   7400   0 0 0
@@@O89   NRST $OSR_SYMS 7000   7200   0 0 0
@@@O90   OSC_OUT $OSR_SYMS 7000   7300   0 0 0
@@@O91   PA0_WKUP $OSR_SYMS 7000   6900   0 0 0
@@@O92   PA1 $OSR_SYMS 7000   6800   0 0 0
@@@O93   OSC32_IN $OSR_SYMS 7000   7600   0 0 0
@@@O94   OSC32_OUT $OSR_SYMS 7000   7500   0 0 0
@@@O95   PA2 $OSR_SYMS 7000   6700   0 0 0
@@@O96   PA3 $OSR_SYMS 8100   5600   90 0 0
@@@O97   PA4 $OSR_SYMS 8200   5600   90 0 0
@@@O98   PA5 $OSR_SYMS 8300   5600   90 0 0
@@@O99   PA6 $OSR_SYMS 8400   5600   90 0 0
@@@O100  PA7 $OSR_SYMS 8500   5600   90 0 0
@@@O101  PB0 $OSR_SYMS 8600   5600   90 0 0
@@@O102  PB1 $OSR_SYMS 8700   5600   90 0 0
@@@O103  PB2/BOOT1 $OSR_SYMS 8800   5600   90 0 0
@@@O104  PB10 $OSR_SYMS 8900   5600   90 0 0
@@@O105  PB11 $OSR_SYMS 9000   5600   90 0 0
@@@O106  PB15 $OSR_SYMS 10300  7000   0 1 0
@@@O107  PB14 $OSR_SYMS 10300  6900   0 1 0
@@@O108  PB13 $OSR_SYMS 10300  6800   0 1 0
@@@O109  PB12 $OSR_SYMS 10300  6700   0 1 0
@@@O110  PA12/USBDP $OSR_SYMS 10300  7500   0 1 0
@@@O111  MCU_PA10/RX1 $OSR_SYMS 10300  7300   0 1 0
@@@O112  MCU_PA9/TX1 $OSR_SYMS 10300  7200   0 1 0
@@@O113  PA8 $OSR_SYMS 10300  7100   0 1 0
@@@O114  PA11/USBDM $OSR_SYMS 10300  7400   0 1 0
@@@O115  MCU_PA13/SWDIO $OSR_SYMS 10300  7600   0 1 0
@@@O116  PA15 $OSR_SYMS 9100   8900   90 2 0
@@@O117  MCU_PA14/SWDCK $OSR_SYMS 9200   8900   90 2 0
@@@O118  PB3 $OSR_SYMS 9000   8900   90 2 0
@@@O119  PB9 $OSR_SYMS 8300   8900   90 2 0
@@@O120  BOOT0 $OSR_SYMS 8500   8900   90 2 0
@@@O121  PB7 $OSR_SYMS 8600   8900   90 2 0
@@@O122  PB6 $OSR_SYMS 8700   8900   90 2 0
@@@O123  PB5 $OSR_SYMS 8800   8900   90 2 0
@@@O124  PB8 $OSR_SYMS 8400   8900   90 2 0
@@@O125  PB4 $OSR_SYMS 8900   8900   90 2 0
@@@O126  GND $GND_SYMS 7200   7100   90 1 0
@@@O127  GND $GND_SYMS 9100   5800   0 0 0
@@@O128  GND $GND_SYMS 10100  7700   90 0 0
@@@O129  GND $GND_SYMS 8200   8700   0 2 0
@@@O130  PD0 $OSR_SYMS 4000   8600   0 1 0
@@@O131  PA12 $OSR_SYMS 4000   5600   0 3 0
@@@O132  PA11 $OSR_SYMS 2800   5600   0 2 0
@@@O133  GND $GND_SYMS 3850   6600   90 0 0
@@@O134  GND $GND_SYMS 2950   6600   90 1 0
@@@O135  GND $GND_SYMS 3850   6700   90 0 0
@@@O136  GND $GND_SYMS 2950   6700   90 1 0
@@@O137  VDD_MCU $PWR_SYMS 3900   5400   90 1 0
@@@O138  VDD_MCU $PWR_SYMS 2900   5400   90 0 0
@@@O139  PD1 $OSR_SYMS 2800   8500   0 0 0
@@@O140  GND $GND_SYMS 3850   6500   90 0 0
@@@O141  PD1 $OSR_SYMS 15200  6650   0 0 0
@@@O142  PD0 $OSR_SYMS 17600  6650   0 1 0
@@@O143  GND $GND_SYMS 3000   8800   90 1 0
@@@O144  BOOT0 $OSR_SYMS 4000   8800   0 1 0
@@@O145  GND $GND_SYMS 5900   7250   0 0 0
@@@O146  VDD_MCU $PWR_SYMS 6200   7000   90 0 0
@@@O147  VDD_MCU $PWR_SYMS 9200   5400   0 2 0
@@@O148  VDD_MCU $PWR_SYMS 11600  7800   90 1 0
@@@O149  VDD_MCU $PWR_SYMS 8100   9350   0 0 0
@@@O150  GND $GND_SYMS 7500   8650   0 0 0
@@@O151  GND $GND_SYMS 6200   6400   0 0 0
@@@O152  GND $GND_SYMS 9500   5250   0 0 0
@@@O153  GND $GND_SYMS 11500  7150   0 0 0

*TIEDOTS*



@@@D0    16000  6650  
@@@D1    16000  4550  
@@@D2    16800  4550  
@@@D3    16400  3950  
@@@D4    18400  9600  
@@@D5    18400  9600  
@@@D6    15150  9500  
@@@D7    8000   13600 
@@@D8    5800   12750 
@@@D9    3400   13100 
@@@D10   3400   13000 
@@@D11   3400   12900 
@@@D12   3400   12800 
@@@D13   9650   13600 
@@@D14   10000  13600 
@@@D15   7000   13600 
@@@D16   10850  13600 
@@@D17   11150  13600 
@@@D18   3500   13600 
@@@D19   5800   13600 
@@@D20   3700   13500 
@@@D21   3600   13400 
@@@D22   16400  6150  
@@@D23   16800  6650  
@@@D24   16000  4550  
@@@D25   16800  4550  
@@@D26   8200   12800 
@@@D27   8400   13600 
@@@D28   10100  12800 
@@@D29   10350  13600 
@@@D30   10450  2700  
@@@D31   10450  3000  
@@@D32   10450  2400  
@@@D33   16000  6650  
@@@D34   16800  6650  
@@@D35   5900   7800  
@@@D36   8100   9300  
@@@D37   7800   9300  
@@@D38   7500   8650  
@@@D39   6200   7000  
@@@D40   9200   5900  
@@@D41   11500  7800  

*CONNECTION*


*SIGNAL* PB5 0 0
D3.2         @@@O6        2 0
19200  13200 
19200  13400 
J2.17        @@@O73       2 0
3100   5900  
2800   5900  
U3.41        @@@O123      2 0
8800   8600  
8800   8900  

*SIGNAL* PA12 0 0
J3.3         @@@D21       2 0
3200   13400 
3600   13400 
@@@D21       R14.1        2 0
3600   13400 
3850   13400 
@@@D21       @@@O38       3 0
3600   13400 
3600   13100 
4500   13100 
J2.24        @@@O131      2 0
3700   5600  
4000   5600  

*SIGNAL* $$$13605 64 0
R6.1         S1.1         2 0
14300  12650 
14300  13000 

*SIGNAL* $$$16580 64 0
U1.3         @@@D27       2 0
8750   13600 
8400   13600 
@@@D7        C7.1         2 0
8000   13600 
8000   13450 
@@@D7        J6.1         2 0
8000   13600 
7650   13600 
C2.1         @@@D27       2 0
8400   13450 
8400   13600 
@@@D27       @@@D7        2 0
8400   13600 
8000   13600 

*SIGNAL* $$$13607 64 0
S2.1         R7.1         2 0
14700  13000 
14700  12650 

*SIGNAL* GND 0 58
"AGND" 
"GND" 
"PART NUMBER" 
"SLEEP_XTAL_IN" 
"GND_a" 
"VBATR" 
"DESCRIPTION" 
"DXLED#" DXLED#
"dnd" 
"Rules.Routing.RestrictedVias.00000" PTH18 STANDARDVIA
"VALUE" GNDTFT
"DGND" 
"CD_CMD" 
"UGND" 
"V-CLK" 
"GND_BT" 
"System_Gnd" 
"Source Path" C:\WIN95\ORCAD\CAPTURE\LIBRARY\CAPSYM.OLB
"Name" AGND_IN
"CARDVCC" 
"CD5V" 50
"CD" GND
"v" A-GND
"VAR" 10V
"V+" 10V
"SYM.OLB" 
"M.OLB" 
"VAUL" AUDIO-GND
"FSDS" AM4
"AUDIO_CLK" 
"RFGND" 
"D-GND" 
"GND-FM" 
"CHGND" 
"RA" 
"DG" 
"BGND" 
"P_GND" 
"IF_GND" GND
"NET NAME" D
"RF GND" RF GND
"TGND" 
"DFT.Nail Count Per Net" 
"GND-S" 
"P30" ACC
"PGND" PGND
"IPGND" 
"vcc" 
"DCDIS" 
"3502_1.8V" 
"EXT GND" 
"GNDD" 
"GND(2)" GND(2)
"VBAT" 
"GND_SIGNAL" 
"OLB" 
"Data to ipod" 111
"GNDPA" GNDPA
@@@O0        @@@D22       2 0
16400  6050  
16400  6150  
C6.1         @@@D22       3 0
16800  6250  
16800  6150  
16400  6150  
@@@D3        C3.1         3 0
16400  3950  
16000  3950  
16000  4150  
@@@D3        @@@O3        2 0
16400  3950  
16400  3850  
R1.2         @@@O7        2 0
17800  12200 
17800  12000 
R2.2         @@@O8        2 0
18500  12200 
18500  12000 
R3.2         @@@O9        2 0
19200  12200 
19200  12000 
C4.1         @@@D3        3 0
16800  4150  
16800  3950  
16400  3950  
@@@O10       S7.2         3 0
19300  9300  
19300  9600  
19050  9600  
C37.2        @@@O11       2 0
18400  8900  
18400  8850  
R9.2         @@@O15       2 0
15150  8800  
15150  8650  
R6.2         @@@O17       2 0
14300  12250 
14300  12000 
R7.2         @@@O18       2 0
14700  12250 
14700  12000 
R10.2        @@@O19       2 0
15100  12250 
15100  12000 
@@@O23       @@@D26       2 0
8200   12650 
8200   12800 
@@@O24       R5.2         2 0
10850  12100 
10850  12300 
C31.2        @@@D28       3 0
10000  12900 
10000  12800 
10100  12800 
@@@O26       B1.2         2 0
5050   6700  
5050   6900  
@@@O27       C10.1        2 0
3500   14300 
3500   14200 
R21.1        @@@O31       2 0
5800   12150 
5800   11950 
J3.5         @@@D9        3 0
3200   13200 
3400   13200 
3400   13100 
J3.6         @@@D9        2 0
3200   13100 
3400   13100 
@@@D9        @@@D10       2 0
3400   13100 
3400   13000 
J3.7         @@@D10       2 0
3200   13000 
3400   13000 
@@@D10       @@@D11       2 0
3400   13000 
3400   12900 
J3.8         @@@D11       2 0
3200   12900 
3400   12900 
@@@D11       @@@D12       2 0
3400   12900 
3400   12800 
J3.9         @@@D12       2 0
3200   12800 
3400   12800 
@@@D12       @@@O32       2 0
3400   12800 
3400   12800 
U1.1         @@@O33       2 0
8750   13400 
8750   13200 
@@@D22       C8.1         3 0
16400  6150  
16000  6150  
16000  6250  
@@@D26       C7.2         3 0
8200   12800 
8000   12800 
8000   12950 
@@@D26       C2.2         3 0
8200   12800 
8400   12800 
8400   12950 
@@@D28       @@@O25       2 0
10100  12800 
10100  12600 
@@@D28       C11.2        3 0
10100  12800 
10350  12800 
10350  12900 
TH1.1        @@@D31       3 0
10662  3300  
10450  3300  
10450  3000  
TH4.1        @@@D32       2 0
10662  2400  
10450  2400  
TH3.1        @@@D30       2 0
10662  2700  
10450  2700  
TH2.1        @@@D31       2 0
10662  3000  
10450  3000  
@@@D31       @@@D30       2 0
10450  3000  
10450  2700  
@@@D32       @@@D30       2 0
10450  2400  
10450  2700  
@@@D32       @@@O43       2 0
10450  2400  
10450  2200  
J1.25        @@@O83       2 0
3100   7800  
2900   7800  
J1.27        @@@O84       2 0
3100   7700  
2900   7700  
J1.26        @@@O85       2 0
3700   7800  
3900   7800  
J1.28        @@@O86       2 0
3700   7700  
3900   7700  
U3.8         @@@O126      2 0
7300   7100  
7200   7100  
U3.23        @@@O127      2 0
9100   5900  
9100   5800  
U3.35        @@@O128      2 0
10000  7700  
10100  7700  
U3.47        @@@O129      2 0
8200   8600  
8200   8700  
J2.4         @@@O133      2 0
3700   6600  
3850   6600  
J2.3         @@@O134      2 0
3100   6600  
2950   6600  
J2.2         @@@O135      2 0
3700   6700  
3850   6700  
J2.1         @@@O136      2 0
3100   6700  
2950   6700  
J2.6         @@@O140      2 0
3700   6500  
3850   6500  
J1.5         @@@O143      2 0
3100   8800  
3000   8800  
C12.1        @@@O145      2 0
5900   7300  
5900   7250  
C50.1        @@@D38       2 0
7500   8700  
7500   8650  
@@@D38       C51.1        3 0
7500   8650  
7800   8650  
7800   8700  
@@@D38       @@@O150      2 0
7500   8650  
7500   8650  
C52.2        @@@O151      2 0
6200   6400  
6200   6400  
C53.2        @@@O152      2 0
9500   5300  
9500   5250  
C54.2        @@@O153      2 0
11500  7200  
11500  7150  

*SIGNAL* $$$13609 64 0
S3.1         R10.1        2 0
15100  13000 
15100  12650 

*SIGNAL* VDD_LINK 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
J8.1         @@@O36       2 0
11700  13250 
11800  13250 

*SIGNAL* $$$4739 64 0
D10.2        @@@D19       2 0
6250   13600 
5800   13600 
C10.2        @@@D18       2 0
3500   13700 
3500   13600 
@@@D18       J3.1         2 0
3500   13600 
3200   13600 
R16.2        @@@D19       2 0
5800   13450 
5800   13600 
@@@D19       @@@D18       2 0
5800   13600 
3500   13600 

*SIGNAL* $$$10873 64 0
R3.1         D3.1         2 0
19200  12600 
19200  12700 

*SIGNAL* PA11 0 0
J3.2         @@@D20       2 0
3200   13500 
3700   13500 
@@@D20       R13.1        2 0
3700   13500 
3850   13500 
@@@D20       @@@O37       3 0
3700   13500 
3700   13200 
4500   13200 
J2.23        @@@O132      2 0
3100   5600  
2800   5600  

*SIGNAL* $$$23084 64 0
R5.1         D4.1         2 0
10850  12700 
10850  12850 

*SIGNAL* PB4 0 0
D2.2         @@@O5        2 0
18500  13200 
18500  13400 
J2.18        @@@O75       2 0
3700   5900  
4000   5900  
U3.40        @@@O125      2 0
8900   8600  
8900   8900  

*SIGNAL* OSC32_IN 0 0
Y5.2         @@@D24       2 0
16200  4550  
16000  4550  
C3.2         @@@D1        2 0
16000  4350  
16000  4550  
@@@D1        R25.1        2 0
16000  4550  
15550  4550  
@@@D24       @@@D1        2 0
16000  4550  
16000  4550  
@@@D24       @@@O41       3 0
16000  4550  
16000  4850  
15100  4850  
U3.3         @@@O93       2 0
7300   7600  
7000   7600  

*SIGNAL* $$$12302 64 0
@@@D8        J7.2         2 0
5800   12750 
6100   12750 
R16.1        @@@D8        2 0
5800   13050 
5800   12750 
R21.2        @@@D8        2 0
5800   12550 
5800   12750 

*SIGNAL* VDD_MCU 0 10
"Rules.Routing.RestrictedVias.00000" VIA12 VIA18 VIA27 VIA78
"VBAT" VBAT
"value" 3V
"VDD" 3.0V
"DESCRIPTION" VCC
"PART NUMBER" 
"CARDVCC" 
"vcc" d
"DCDIS" 
"GFGF" 
S6.2         @@@O14       2 0
15150  10050 
15150  10300 
R8.1         @@@O12       2 0
18400  10300 
18400  10450 
@@@O34       J15.1        2 0
11800  13600 
11700  13600 
J2.26        @@@O76       2 0
3700   5500  
3900   5500  
J2.25        @@@O77       2 0
3100   5500  
2900   5500  
J1.2         @@@O79       2 0
3700   9000  
3900   9000  
J1.4         @@@O80       2 0
3700   8900  
3900   8900  
J1.1         @@@O81       2 0
3100   9000  
2900   9000  
J1.3         @@@O82       2 0
3100   8900  
2900   8900  
J2.28        @@@O137      2 0
3700   5400  
3900   5400  
J2.27        @@@O138      2 0
3100   5400  
2900   5400  
U3.9         @@@D39       2 0
7300   7000  
6200   7000  
U3.24        @@@D40       2 0
9200   5900  
9200   5900  
U3.36        @@@D41       2 0
10000  7800  
11500  7800  
U3.48        @@@D36       2 0
8100   8600  
8100   9300  
C50.2        @@@D37       3 0
7500   9200  
7500   9300  
7800   9300  
@@@D36       @@@O149      2 0
8100   9300  
8100   9350  
C51.2        @@@D37       2 0
7800   9200  
7800   9300  
@@@D37       @@@D36       2 0
7800   9300  
8100   9300  
C52.1        @@@D39       2 0
6200   6900  
6200   7000  
@@@D39       @@@O146      2 0
6200   7000  
6200   7000  
@@@D40       @@@O147      2 0
9200   5900  
9200   5400  
@@@D40       C53.1        3 0
9200   5900  
9500   5900  
9500   5800  
C54.1        @@@D41       2 0
11500  7700  
11500  7800  
@@@D41       @@@O148      2 0
11500  7800  
11600  7800  

*SIGNAL* 5V 0 0
@@@D15       J6.2         2 0
7000   13600 
7250   13600 
D10.1        @@@D15       2 0
6750   13600 
7000   13600 
@@@D15       @@@O35       2 0
7000   13600 
7000   13900 

*SIGNAL* OSC32_OUT 0 0
Y5.1         @@@D2        2 0
16600  4550  
16800  4550  
@@@D2        R26.2        2 0
16800  4550  
17200  4550  
C4.2         @@@D25       2 0
16800  4350  
16800  4550  
@@@D25       @@@D2        2 0
16800  4550  
16800  4550  
@@@D25       @@@O42       3 0
16800  4550  
16800  4850  
17800  4850  
U3.4         @@@O94       2 0
7300   7500  
7000   7500  

*SIGNAL* $$$17610 64 0
D8.2         B1.1         3 0
5250   7800  
5050   7800  
5050   7600  

*SIGNAL* $$$18572 64 0
@@@D14       @@@D29       2 0
10000  13600 
10350  13600 
U1.4         @@@D13       2 0
9550   13600 
9650   13600 
@@@D13       U1.2         3 0
9650   13600 
9650   13400 
9550   13400 
@@@D13       @@@D14       2 0
9650   13600 
10000  13600 
C31.1        @@@D14       2 0
10000  13400 
10000  13600 
D4.2         @@@D16       2 0
10850  13350 
10850  13600 
@@@D16       @@@D17       2 0
10850  13600 
11150  13600 
J8.2         @@@D17       3 0
11300  13250 
11150  13250 
11150  13600 
@@@D17       J15.2        2 0
11150  13600 
11300  13600 
C11.1        @@@D29       2 0
10350  13400 
10350  13600 
@@@D29       @@@D16       2 0
10350  13600 
10850  13600 

*SIGNAL* $$$7386 64 0
D8.1         @@@D35       2 0
5750   7800  
5900   7800  
C12.2        @@@D35       2 0
5900   7800  
5900   7800  
@@@D35       U3.1         2 0
5900   7800  
7300   7800  

*SIGNAL* OSC_IN 0 0
Y2.1         @@@D23       2 0
16698  6650  
16800  6650  
C6.2         @@@D23       2 0
16800  6450  
16800  6650  
@@@D23       @@@D34       2 0
16800  6650  
16800  6650  
U3.5         @@@O88       2 0
7300   7400  
7000   7400  
@@@D34       @@@O40       3 0
16800  6650  
16800  7000  
17600  7000  
@@@D34       R23.2        2 0
16800  6650  
17150  6650  

*SIGNAL* OSC_OUT 0 0
@@@D0        Y2.2         2 0
16000  6650  
16098  6650  
@@@O39       @@@D0        3 0
15200  7000  
16000  7000  
16000  6650  
C8.2         @@@D33       2 0
16000  6450  
16000  6650  
U3.6         @@@O90       2 0
7300   7300  
7000   7300  
R22.1        @@@D33       2 0
15700  6650  
16000  6650  
@@@D33       @@@D0        2 0
16000  6650  
16000  6650  

*SIGNAL* PD0 0 0
J1.10        @@@O130      2 0
3700   8600  
4000   8600  
R23.1        @@@O142      2 0
17550  6650  
17600  6650  

*SIGNAL* PD1 0 0
J1.11        @@@O139      2 0
3100   8500  
2800   8500  
R22.2        @@@O141      2 0
15300  6650  
15200  6650  

*SIGNAL* $$$2339 64 0
R1.1         D1.1         2 0
17800  12600 
17800  12700 

*SIGNAL* PC14 0 0
@@@O1        R25.2        2 0
15100  4550  
15150  4550  
J1.8         @@@O47       2 0
3700   8700  
4000   8700  

*SIGNAL* NRST 0 0
S7.1         @@@D4        2 0
18650  9600  
18400  9600  
@@@D5        C37.1        2 0
18400  9600  
18400  9400  
@@@D4        @@@D5        2 0
18400  9600  
18400  9600  
@@@O13       @@@D5        2 0
17800  9600  
18400  9600  
R8.2         @@@D4        2 0
18400  9900  
18400  9600  
U3.7         @@@O89       2 0
7300   7200  
7000   7200  

*SIGNAL* PA12/USBDP 0 0
R14.2        @@@O28       2 0
4250   13400 
4500   13400 
U3.33        @@@O110      2 0
10000  7500  
10300  7500  

*SIGNAL* $$$2340 64 0
R2.1         D2.1         2 0
18500  12600 
18500  12700 

*SIGNAL* PA1 0 0
J1.13        @@@O46       2 0
3100   8400  
2800   8400  
U3.11        @@@O92       2 0
7300   6800  
7000   6800  

*SIGNAL* PA2 0 0
J1.14        @@@O49       2 0
3700   8400  
4000   8400  
U3.12        @@@O95       2 0
7300   6700  
7000   6700  

*SIGNAL* PA3 0 0
J1.15        @@@O50       2 0
3100   8300  
2800   8300  
U3.13        @@@O96       2 0
8100   5900  
8100   5600  

*SIGNAL* PA4 0 0
S1.2         @@@O20       2 0
14300  13400 
14300  13700 
J1.16        @@@O51       2 0
3700   8300  
4000   8300  
U3.14        @@@O97       2 0
8200   5900  
8200   5600  

*SIGNAL* PA5 0 0
S2.2         @@@O21       3 0
14700  13400 
14700  14000 
14300  14000 
J1.17        @@@O52       2 0
3100   8200  
2800   8200  
U3.15        @@@O98       2 0
8300   5900  
8300   5600  

*SIGNAL* PA6 0 0
S3.2         @@@O22       3 0
15100  13400 
15100  14300 
14300  14300 
J1.18        @@@O53       2 0
3700   8200  
4000   8200  
U3.16        @@@O99       2 0
8400   5900  
8400   5600  

*SIGNAL* PA7 0 0
J1.19        @@@O54       2 0
3100   8100  
2800   8100  
U3.17        @@@O100      2 0
8500   5900  
8500   5600  

*SIGNAL* PA8 0 0
D1.2         @@@O4        2 0
17800  13200 
17800  13400 
J2.9         @@@O65       2 0
3100   6300  
2800   6300  
U3.29        @@@O113      2 0
10000  7100  
10300  7100  

*SIGNAL* MCU_PA9/TX1 0 0
J2.12        @@@O64       2 0
3700   6200  
4000   6200  
U3.30        @@@O112      2 0
10000  7200  
10300  7200  

*SIGNAL* MCU_PA10/RX1 0 0
J2.11        @@@O63       2 0
3100   6200  
2800   6200  
U3.31        @@@O111      2 0
10000  7300  
10300  7300  

*SIGNAL* PC15 0 0
@@@O2        R26.1        2 0
17800  4550  
17600  4550  
J1.9         @@@O48       2 0
3100   8600  
2800   8600  

*SIGNAL* PA0_WKUP 0 0
S6.1         @@@D6        2 0
15150  9650  
15150  9500  
@@@O16       @@@D6        2 0
14750  9500  
15150  9500  
R9.1         @@@D6        2 0
15150  9200  
15150  9500  
J7.1         @@@O30       2 0
6500   12750 
6700   12750 
J1.12        @@@O45       2 0
3700   8500  
4000   8500  
U3.10        @@@O91       2 0
7300   6900  
7000   6900  

*SIGNAL* PA11/USBDM 0 0
R13.2        @@@O29       2 0
4250   13500 
4500   13500 
U3.32        @@@O114      2 0
10000  7400  
10300  7400  

*SIGNAL* BOOT0 0 0
U3.44        @@@O120      2 0
8500   8600  
8500   8900  
J1.6         @@@O144      2 0
3700   8800  
4000   8800  

*SIGNAL* MCU_PA13/SWDIO 0 0
J2.14        @@@O66       2 0
3700   6100  
4000   6100  
U3.34        @@@O115      2 0
10000  7600  
10300  7600  

*SIGNAL* MCU_PA14/SWDCK 0 0
J2.13        @@@O68       2 0
3100   6100  
2800   6100  
U3.37        @@@O117      2 0
9200   8600  
9200   8900  

*SIGNAL* PA15 0 0
J2.16        @@@O67       2 0
3700   6000  
4000   6000  
U3.38        @@@O116      2 0
9100   8600  
9100   8900  

*SIGNAL* PB0 0 0
J1.20        @@@O55       2 0
3700   8100  
4000   8100  
U3.18        @@@O101      2 0
8600   5900  
8600   5600  

*SIGNAL* PB1 0 0
J1.21        @@@O56       2 0
3100   8000  
2800   8000  
U3.19        @@@O102      2 0
8700   5900  
8700   5600  

*SIGNAL* PB2/BOOT1 0 0
J1.22        @@@O78       2 0
3700   8000  
4000   8000  
U3.20        @@@O103      2 0
8800   5900  
8800   5600  

*SIGNAL* PB3 0 0
J2.15        @@@O69       2 0
3100   6000  
2800   6000  
U3.39        @@@O118      2 0
9000   8600  
9000   8900  

*SIGNAL* PB6 0 0
J2.20        @@@O72       2 0
3700   5800  
4000   5800  
U3.42        @@@O122      2 0
8700   8600  
8700   8900  

*SIGNAL* PB7 0 0
J2.19        @@@O71       2 0
3100   5800  
2800   5800  
U3.43        @@@O121      2 0
8600   8600  
8600   8900  

*SIGNAL* PB8 0 0
J2.22        @@@O70       2 0
3700   5700  
4000   5700  
U3.45        @@@O124      2 0
8400   8600  
8400   8900  

*SIGNAL* PB9 0 0
J2.21        @@@O74       2 0
3100   5700  
2800   5700  
U3.46        @@@O119      2 0
8300   8600  
8300   8900  

*SIGNAL* PB10 0 0
J1.23        @@@O57       2 0
3100   7900  
2800   7900  
U3.21        @@@O104      2 0
8900   5900  
8900   5600  

*SIGNAL* PB11 0 0
J1.24        @@@O58       2 0
3700   7900  
4000   7900  
U3.22        @@@O105      2 0
9000   5900  
9000   5600  

*SIGNAL* PB12 0 0
J2.5         @@@O62       2 0
3100   6500  
2800   6500  
U3.25        @@@O109      2 0
10000  6700  
10300  6700  

*SIGNAL* PB13 0 0
J2.8         @@@O61       2 0
3700   6400  
4000   6400  
U3.26        @@@O108      2 0
10000  6800  
10300  6800  

*SIGNAL* PB14 0 0
J2.7         @@@O60       2 0
3100   6400  
2800   6400  
U3.27        @@@O107      2 0
10000  6900  
10300  6900  

*SIGNAL* PB15 0 0
J2.10        @@@O59       2 0
3700   6300  
4000   6300  
U3.28        @@@O106      2 0
10000  7000  
10300  7000  

*SIGNAL* PC13 0 0
J1.7         @@@O44       2 0
3100   8700  
2800   8700  
U3.2         @@@O87       2 0
7300   7700  
7000   7700  

*NETNAMES*



PC14         @@@O1        -350   50     0 3 0      0      0 3 -1 10 97 "Default Font"
PC15         @@@O2        360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PA8          @@@O4        0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB4          @@@O5        0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB5          @@@O6        50     500    90 2 0      0      90 3 -1 10 97 "Default Font"
VDD_MCU      @@@O12       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
NRST         @@@O13       -550   -50    0 0 0      0      0 2 -1 10 97 "Default Font"
VDD_MCU      @@@O14       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
PA0_WKUP     @@@O16       -350   -50    0 1 0      0      0 3 -1 10 97 "Default Font"
PA4          @@@O20       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O21       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O22       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA12/USBDP   @@@O28       320    -40    0 0 0      0      0 3 -1 12 97 "Default Font"
PA11/USBDM   @@@O29       322    -32    0 0 0      0      0 3 -1 12 97 "Default Font"
PA0_WKUP     @@@O30       350    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O34       400    50     0 6 0      0      0 0 -1 10 97 "Default Font"
5V           @@@O35       0      250    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_LINK     @@@O36       400    50     0 6 0      0      0 0 -1 10 97 "Default Font"
PA11         @@@O37       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA12         @@@O38       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
OSC_OUT      @@@O39       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC_IN       @@@O40       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
OSC32_IN     @@@O41       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC32_OUT    @@@O42       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PC13         @@@O44       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA0_WKUP     @@@O45       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA1          @@@O46       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PC14         @@@O47       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PC15         @@@O48       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA2          @@@O49       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA3          @@@O50       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA4          @@@O51       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O52       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O53       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA7          @@@O54       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PB0          @@@O55       360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB1          @@@O56       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PB10         @@@O57       -350   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PB11         @@@O58       350    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB15         @@@O59       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PB14         @@@O60       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB13         @@@O61       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PB12         @@@O62       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
MCU_PA10/RX1 @@@O63       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O64       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PA8          @@@O65       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O66       350    -50    0 0 0      0      0 3 -1 10 97 "Default Font"
PA15         @@@O67       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O68       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB3          @@@O69       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB8          @@@O70       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PB7          @@@O71       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB6          @@@O72       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PB5          @@@O73       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB9          @@@O74       -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
PB4          @@@O75       360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O77       -450   0      0 6 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O76       450    -50    0 5 0      0      0 0 -1 10 97 "Default Font"
PB2/BOOT1    @@@O78       350    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O79       400    50     0 7 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O80       400    50     0 7 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O81       -400   50     0 6 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O82       -400   50     0 6 0      0      0 0 -1 10 97 "Default Font"
PC13         @@@O87       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC_IN       @@@O88       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
NRST         @@@O89       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC_OUT      @@@O90       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA0_WKUP     @@@O91       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA1          @@@O92       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC32_IN     @@@O93       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
OSC32_OUT    @@@O94       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA2          @@@O95       -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PA3          @@@O96       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA4          @@@O97       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA5          @@@O98       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA6          @@@O99       0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PA7          @@@O100      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB0          @@@O101      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB1          @@@O102      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB2/BOOT1    @@@O103      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB10         @@@O104      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB11         @@@O105      0      -360   90 2 0      0      0 3 -1 10 97 "Default Font"
PB15         @@@O106      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB14         @@@O107      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB13         @@@O108      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PB12         @@@O109      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA12/USBDP   @@@O110      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA10/RX1 @@@O111      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA9/TX1  @@@O112      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA8          @@@O113      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA11/USBDM   @@@O114      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA13/SWDIO @@@O115      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA15         @@@O116      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
MCU_PA14/SWDCK @@@O117      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB3          @@@O118      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB9          @@@O119      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
BOOT0        @@@O120      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB7          @@@O121      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB6          @@@O122      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB5          @@@O123      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB8          @@@O124      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PB4          @@@O125      0      360    90 0 0      0      0 3 -1 10 97 "Default Font"
PD0          @@@O130      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
PA12         @@@O131      360    0      0 2 0      0      0 3 -1 10 97 "Default Font"
PA11         @@@O132      -360   0      0 3 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O138      -450   0      0 6 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O137      450    -50    0 5 0      0      0 0 -1 10 97 "Default Font"
PD1          @@@O139      -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PD1          @@@O141      -360   0      0 1 0      0      0 3 -1 10 97 "Default Font"
PD0          @@@O142      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
BOOT0        @@@O144      360    0      0 0 0      0      0 3 -1 10 97 "Default Font"
VDD_MCU      @@@O146      -450   -50    0 4 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O147      50     -400   90 4 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O148      0      250    0 7 0      0      0 0 -1 10 97 "Default Font"
VDD_MCU      @@@O149      0      250    0 4 0      0      0 0 -1 10 97 "Default Font"

*END*     OF ASCII OUTPUT FILE