1、功能说明
    1、TIM3 TIM4在TIM1周期下计数
2、使用环境
    软件开发环境：  KEIL MDK-ARM V5.26.2.0
    硬件环境：      基于N32G4XVL-STB V1.1开发
3、使用说明
    系统配置；
        1、时钟源：
                    HSE=8M,PLL=144M,AHB=144M,APB1=36M,APB2=72M,TIM1 CLK=144M,TIM3 CLK=72M,TIM4 CLK=72M
        2、端口配置：
                    PA6选择为TIM3的CH1输出
                    PB6选择为TIM4的CH1输出
                    PA8选择为TIM1的CH1输出
        3、TIM：
                    TIM1 CH1 周期触发TIM3 TIM4的门控
    使用方法：
        1、编译后打开调试模式，用示波器或者逻辑分析仪观察TIM1 CH1、TIM3 CH1、TIM4 CH1的波形
        2、程序运行后，TIM3 15倍周期TIM1，TIM4 10倍周期TIM1
4、注意事项
    无

1. Function description
     1. TIM3 TIM4 counts under the TIM1 cycle
2. Use environment
     Software development environment: KEIL MDK-ARM V5.26.2.0
     Hardware environment: Developed based on N32G4XVL-STB V1.1
3. Instructions for use
     System Configuration;
         1. Clock source:
                     HSE=8M, PLL=144M, AHB=144M, APB1=36M, APB2=72M, TIM1 CLK=144M, TIM3 CLK=72M, TIM4 CLK=72M
         2. Port configuration:
                     PA6 is selected as the CH1 output of TIM3
                     PB6 is selected as the CH1 output of TIM4
                     PA8 is selected as the CH1 output of TIM1
         3. TIM:
                     TIM1 CH1 period triggers the gating of TIM3 TIM4
     Instructions:
         1. After compiling, turn on the debug mode, use an oscilloscope or logic analyzer to observe the waveforms of TIM1 CH1, TIM3 CH1, and TIM4 CH1
         2. After the program runs, TIM3 15 times cycle TIM1, TIM4 10 times cycle TIM1
4. Matters needing attention
     without