# Static Call Graph for image .\Objects\JumpToBoot.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Mon Jun 20 17:36:56 2022

### Maximum Stack Usage = 100 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ Debug_USART_Config ⇒ USART_Init ⇒ RCC_GetClocksFreqValue

### Mutually Recursive functions

- PendSV_Handler ⇒ PendSV_Handler
- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - ADC3_4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - BusFault_Handler from n32g45x_it.o(i.BusFault_Handler) referenced from startup_n32g45x.o(RESET)
  - CAN1_RX1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - CAN1_SCE_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - CAN2_RX0_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - CAN2_RX1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - CAN2_SCE_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - CAN2_TX_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - COMP7_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - COMP_1_2_3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - COMP_4_5_6_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA1_Channel8_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel5_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel6_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel7_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DMA2_Channel8_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DVP_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - DebugMon_Handler from n32g45x_it.o(i.DebugMon_Handler) referenced from startup_n32g45x.o(RESET)
  - ETH_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - ETH_WKUP_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI0_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI15_10_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - EXTI9_5_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - FLASH_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - HardFault_Handler from n32g45x_it.o(i.HardFault_Handler) referenced from startup_n32g45x.o(RESET)
  - I2C1_ER_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C1_EV_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C2_ER_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C2_EV_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C3_ER_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C3_EV_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C4_ER_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - I2C4_EV_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - MMU_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - MemManage_Handler from n32g45x_it.o(i.MemManage_Handler) referenced from startup_n32g45x.o(RESET)
  - NMI_Handler from n32g45x_it.o(i.NMI_Handler) referenced from startup_n32g45x.o(RESET)
  - PVD_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - PendSV_Handler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - QSPI_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - RCC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - RSRAM_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - RTCAlarm_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - RTC_WKUP_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - Reset_Handler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SAC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SDIO_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SPI1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SPI2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SPI3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - SVC_Handler from n32g45x_it.o(i.SVC_Handler) referenced from startup_n32g45x.o(RESET)
  - SysTick_Handler from n32g45x_it.o(i.SysTick_Handler) referenced from startup_n32g45x.o(RESET)
  - SystemInit from system_n32g45x.o(i.SystemInit) referenced from startup_n32g45x.o(.text)
  - TAMPER_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM1_BRK_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM1_CC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM1_UP_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM5_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM6_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM7_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM8_BRK_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM8_CC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TIM8_UP_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - TSC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - UART4_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - UART5_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - UART6_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - UART7_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USART1_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USART2_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USART3_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USBWakeUp_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - UsageFault_Handler from n32g45x_it.o(i.UsageFault_Handler) referenced from startup_n32g45x.o(RESET)
  - WWDG_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - XFMC_IRQHandler from startup_n32g45x.o(.text) referenced from startup_n32g45x.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_n32g45x.o(.text)
  - fputc from bsp_usart.o(i.fputc) referenced from printfb.o(i.__0printf$bare)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_n32g45x.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Calls]

  - >> PendSV_Handler
  [Called By]
  - >> PendSV_Handler
  [Address Reference Count : 1]
  - startup_n32g45x.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_n32g45x.o(RESET)

  ADC3_4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  COMP7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  COMP_1_2_3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  COMP_4_5_6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA1_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DMA2_Channel8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DVP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C4_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  I2C4_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  MMU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  QSPI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  RSRAM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  TSC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  UART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  XFMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_n32g45x.o(.text))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g45x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g45x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  Debug_USART_Config (Thumb, 126 bytes, Stack size 24 bytes, bsp_usart.o(i.Debug_USART_Config))
  [Stack]

  - Max Depth = 100
  - Call Chain = Debug_USART_Config ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> GPIO_InitPeripheral
  - >> USART_Init
  - >> USART_Enable
  - >> RCC_EnableAPB2PeriphClk
  [Called By]
  - >> main

  FLASH_PrefetchBufSet (Thumb, 44 bytes, Stack size 8 bytes, n32g45x_flash.o(i.FLASH_PrefetchBufSet))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_PrefetchBufSet
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  FLASH_SetLatency (Thumb, 50 bytes, Stack size 16 bytes, n32g45x_flash.o(i.FLASH_SetLatency))
  [Stack]

  - Max Depth = 16
  - Call Chain = FLASH_SetLatency
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  FLASH_iCacheCmd (Thumb, 44 bytes, Stack size 8 bytes, n32g45x_flash.o(i.FLASH_iCacheCmd))
  [Stack]

  - Max Depth = 8
  - Call Chain = FLASH_iCacheCmd
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  GPIO_DeInit (Thumb, 226 bytes, Stack size 8 bytes, n32g45x_gpio.o(i.GPIO_DeInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_DeInit ⇒ RCC_EnableAPB2PeriphReset
  [Calls]
  - >> RCC_EnableAPB2PeriphReset
  - >> assert_failed
  [Called By]
  - >> Jump_To_BOOT

  GPIO_InitPeripheral (Thumb, 390 bytes, Stack size 40 bytes, n32g45x_gpio.o(i.GPIO_InitPeripheral))
  [Stack]

  - Max Depth = 40
  - Call Chain = GPIO_InitPeripheral
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Debug_USART_Config
  - >> IAP_Button_Config

  GPIO_ReadInputDataBit (Thumb, 174 bytes, Stack size 16 bytes, n32g45x_gpio.o(i.GPIO_ReadInputDataBit))
  [Stack]

  - Max Depth = 16
  - Call Chain = GPIO_ReadInputDataBit
  [Calls]
  - >> assert_failed
  [Called By]
  - >> IAP_Button_Read

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g45x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  IAP_Button_Config (Thumb, 38 bytes, Stack size 8 bytes, main.o(i.IAP_Button_Config))
  [Stack]

  - Max Depth = 48
  - Call Chain = IAP_Button_Config ⇒ GPIO_InitPeripheral
  [Calls]
  - >> GPIO_InitPeripheral
  - >> RCC_EnableAPB2PeriphClk
  [Called By]
  - >> main

  IAP_Button_Read (Thumb, 12 bytes, Stack size 8 bytes, main.o(i.IAP_Button_Read))
  [Stack]

  - Max Depth = 24
  - Call Chain = IAP_Button_Read ⇒ GPIO_ReadInputDataBit
  [Calls]
  - >> GPIO_ReadInputDataBit
  [Called By]
  - >> main

  IWDG_ReloadKey (Thumb, 10 bytes, Stack size 0 bytes, n32g45x_iwdg.o(i.IWDG_ReloadKey))
  [Called By]

  - >> Jump_To_BOOT

  IWDG_SetPrescalerDiv (Thumb, 48 bytes, Stack size 8 bytes, n32g45x_iwdg.o(i.IWDG_SetPrescalerDiv))
  [Stack]

  - Max Depth = 8
  - Call Chain = IWDG_SetPrescalerDiv
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Jump_To_BOOT

  IWDG_WriteConfig (Thumb, 32 bytes, Stack size 8 bytes, n32g45x_iwdg.o(i.IWDG_WriteConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = IWDG_WriteConfig
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Jump_To_BOOT

  Jump_To_BOOT (Thumb, 220 bytes, Stack size 32 bytes, main.o(i.Jump_To_BOOT))
  [Stack]

  - Max Depth = 64
  - Call Chain = Jump_To_BOOT ⇒ SetSysClock_HSI_PLL ⇒ RCC_GetFlagStatus
  [Calls]
  - >> IWDG_WriteConfig
  - >> IWDG_SetPrescalerDiv
  - >> IWDG_ReloadKey
  - >> GPIO_DeInit
  - >> SetSysClock_HSI_PLL
  - >> USART_DeInit
  - >> RCC_EnableAPB1PeriphReset
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g45x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g45x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  RCC_ConfigHclk (Thumb, 68 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_ConfigHclk))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_ConfigHclk
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_ConfigPclk1 (Thumb, 60 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_ConfigPclk1))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_ConfigPclk1
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_ConfigPclk2 (Thumb, 62 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_ConfigPclk2))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_ConfigPclk2
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_ConfigPll (Thumb, 254 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_ConfigPll))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_ConfigPll
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_ConfigSysclk (Thumb, 44 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_ConfigSysclk))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_ConfigSysclk
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_DeInit (Thumb, 74 bytes, Stack size 0 bytes, n32g45x_rcc.o(i.RCC_DeInit))
  [Called By]

  - >> SetSysClock_HSI_PLL

  RCC_EnableAPB1PeriphClk (Thumb, 74 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_EnableAPB1PeriphClk))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_EnableAPB1PeriphClk
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_EnableAPB1PeriphReset (Thumb, 74 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_EnableAPB1PeriphReset))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_EnableAPB1PeriphReset
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Jump_To_BOOT
  - >> USART_DeInit

  RCC_EnableAPB2PeriphClk (Thumb, 74 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_EnableAPB2PeriphClk))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_EnableAPB2PeriphClk
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Debug_USART_Config
  - >> IAP_Button_Config

  RCC_EnableAPB2PeriphReset (Thumb, 74 bytes, Stack size 16 bytes, n32g45x_rcc.o(i.RCC_EnableAPB2PeriphReset))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_EnableAPB2PeriphReset
  [Calls]
  - >> assert_failed
  [Called By]
  - >> GPIO_DeInit
  - >> USART_DeInit

  RCC_EnableHsi (Thumb, 30 bytes, Stack size 8 bytes, n32g45x_rcc.o(i.RCC_EnableHsi))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_EnableHsi
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_EnablePll (Thumb, 30 bytes, Stack size 8 bytes, n32g45x_rcc.o(i.RCC_EnablePll))
  [Stack]

  - Max Depth = 8
  - Call Chain = RCC_EnablePll
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_GetClocksFreqValue (Thumb, 240 bytes, Stack size 20 bytes, n32g45x_rcc.o(i.RCC_GetClocksFreqValue))
  [Stack]

  - Max Depth = 20
  - Call Chain = RCC_GetClocksFreqValue
  [Called By]
  - >> USART_Init

  RCC_GetFlagStatus (Thumb, 140 bytes, Stack size 24 bytes, n32g45x_rcc.o(i.RCC_GetFlagStatus))
  [Stack]

  - Max Depth = 24
  - Call Chain = RCC_GetFlagStatus
  [Calls]
  - >> assert_failed
  [Called By]
  - >> SetSysClock_HSI_PLL

  RCC_GetSysclkSrc (Thumb, 10 bytes, Stack size 0 bytes, n32g45x_rcc.o(i.RCC_GetSysclkSrc))
  [Called By]

  - >> SetSysClock_HSI_PLL

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g45x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SetSysClock_HSI_PLL (Thumb, 126 bytes, Stack size 8 bytes, main.o(i.SetSysClock_HSI_PLL))
  [Stack]

  - Max Depth = 32
  - Call Chain = SetSysClock_HSI_PLL ⇒ RCC_GetFlagStatus
  [Calls]
  - >> FLASH_iCacheCmd
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufSet
  - >> RCC_GetSysclkSrc
  - >> RCC_GetFlagStatus
  - >> RCC_EnablePll
  - >> RCC_EnableHsi
  - >> RCC_EnableAPB1PeriphClk
  - >> RCC_DeInit
  - >> RCC_ConfigSysclk
  - >> RCC_ConfigPll
  - >> RCC_ConfigPclk2
  - >> RCC_ConfigPclk1
  - >> RCC_ConfigHclk
  [Called By]
  - >> Jump_To_BOOT

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, n32g45x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  SystemInit (Thumb, 146 bytes, Stack size 8 bytes, system_n32g45x.o(i.SystemInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_n32g45x.o(.text)

  USART_ClrFlag (Thumb, 134 bytes, Stack size 16 bytes, n32g45x_usart.o(i.USART_ClrFlag))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_ClrFlag
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Usart_SendByte

  USART_DeInit (Thumb, 240 bytes, Stack size 8 bytes, n32g45x_usart.o(i.USART_DeInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART_DeInit ⇒ RCC_EnableAPB2PeriphReset
  [Calls]
  - >> RCC_EnableAPB2PeriphReset
  - >> assert_failed
  - >> RCC_EnableAPB1PeriphReset
  [Called By]
  - >> Jump_To_BOOT

  USART_Enable (Thumb, 106 bytes, Stack size 16 bytes, n32g45x_usart.o(i.USART_Enable))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_Enable
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Debug_USART_Config

  USART_GetFlagStatus (Thumb, 176 bytes, Stack size 16 bytes, n32g45x_usart.o(i.USART_GetFlagStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetFlagStatus
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Usart_SendByte

  USART_Init (Thumb, 436 bytes, Stack size 56 bytes, n32g45x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> assert_failed
  - >> RCC_GetClocksFreqValue
  [Called By]
  - >> Debug_USART_Config

  USART_SendData (Thumb, 90 bytes, Stack size 16 bytes, n32g45x_usart.o(i.USART_SendData))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_SendData
  [Calls]
  - >> assert_failed
  [Called By]
  - >> Usart_SendByte

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, n32g45x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_n32g45x.o(RESET)

  Usart_SendByte (Thumb, 38 bytes, Stack size 16 bytes, bsp_usart.o(i.Usart_SendByte))
  [Stack]

  - Max Depth = 32
  - Call Chain = Usart_SendByte ⇒ USART_SendData
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  - >> USART_ClrFlag
  [Called By]
  - >> fputc

  __0printf$bare (Thumb, 8 bytes, Stack size 0 bytes, printfb.o(i.__0printf$bare), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$bare (Thumb, 0 bytes, Stack size 0 bytes, printfb.o(i.__0printf$bare), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 0 bytes, printfb.o(i.__0printf$bare))
  [Called By]

  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  assert_failed (Thumb, 4 bytes, Stack size 0 bytes, main.o(i.assert_failed))
  [Called By]

  - >> IWDG_WriteConfig
  - >> IWDG_SetPrescalerDiv
  - >> RCC_EnableAPB2PeriphReset
  - >> GPIO_ReadInputDataBit
  - >> GPIO_InitPeripheral
  - >> GPIO_DeInit
  - >> FLASH_iCacheCmd
  - >> FLASH_SetLatency
  - >> FLASH_PrefetchBufSet
  - >> USART_SendData
  - >> USART_Init
  - >> USART_GetFlagStatus
  - >> USART_Enable
  - >> USART_DeInit
  - >> USART_ClrFlag
  - >> RCC_GetFlagStatus
  - >> RCC_EnablePll
  - >> RCC_EnableHsi
  - >> RCC_EnableAPB2PeriphClk
  - >> RCC_EnableAPB1PeriphReset
  - >> RCC_EnableAPB1PeriphClk
  - >> RCC_ConfigSysclk
  - >> RCC_ConfigPll
  - >> RCC_ConfigPclk2
  - >> RCC_ConfigPclk1
  - >> RCC_ConfigHclk

  fputc (Thumb, 58 bytes, Stack size 16 bytes, bsp_usart.o(i.fputc))
  [Stack]

  - Max Depth = 48
  - Call Chain = fputc ⇒ Usart_SendByte ⇒ USART_SendData
  [Calls]
  - >> Usart_SendByte
  [Address Reference Count : 1]
  - printfb.o(i.__0printf$bare)

  main (Thumb, 44 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 100
  - Call Chain = main ⇒ Debug_USART_Config ⇒ USART_Init ⇒ RCC_GetClocksFreqValue
  [Calls]
  - >> __2printf
  - >> Debug_USART_Config
  - >> Jump_To_BOOT
  - >> IAP_Button_Read
  - >> IAP_Button_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClock (Thumb, 236 bytes, Stack size 16 bytes, system_n32g45x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  _printf_core (Thumb, 34 bytes, Stack size 24 bytes, printfb.o(i._printf_core), UNUSED)
  [Called By]

  - >> __0printf$bare

  ### Undefined Global Symbols