Nsing.N32H49x_Library.1.0.0版本：
1. USART LIN DEMO配置RX增加上拉设置
2. 修改SPI_NSS_LOW宏定义
3. 优化RCC时钟配置例程
4. USBFS增加无晶体模式下远程唤醒功能
5. 新增V2版本xspi驱动函数及例程
6. 添加IAR工程和部分例程
7. 优化RTC_EnterInitMode()函数
8. 修改RTC_GetTime和RTC_GetSubSecond函数：通过读DATE寄存器解除日期寄存器锁定
9. 补全USBHS主机复合设备Demo
10. 优化FLASH_EraseOnePage函数：添加地址判断
11. 优化SPI_FLASH例程：增加TE/BUSY/RXNE标志判断
12. 修改例程中的EXTI_GetITStatus为EXTI_GetStatusFlag
13. TIM_InitTimBaseStruct驱动函数，结构体初始化补充完整

Nations.N32H49x_Library.0.1.0版本：
1.初版发布
----------------------------------------------------------------------------------------------------------------------------------------------------
Nsing.N32H49x_Library.1.0.0 version:
1. Configured USART LIN DEMO to add pull-up setting for RX
2. Modified SPI_NSS_LOW macro definition
3. Optimised RCC clock configuration routine
4. Added remote wake-up functionality in crystal-less mode for USBFS
5. Added V2 version xspi driver functions and examples
6. Added IAR project and partial examples
7. Optimised RTC_EnterInitMode() function
8. Modified RTC_GetTime and RTC_GetSubSecond functions: Unlocks date register by reading DATE register
9. Completion of USBHS host composite device demonstration
10. Optimisation of FLASH_EraseOnePage function: addition of address validation
11. Optimisation of SPI_FLASH routine: inclusion of TE/BUSY/RXNE flag checks
12. Modification of EXTI_GetITStatus to EXTI_GetStatusFlag within example code
13. TIM_InitTimBaseStruct driver function, structure initialization completion.

Nations.N32H49x_Library.0.1.0 version:
1.Initial Release



