1、功能说明

	1、此例程展示在 RT_Thread 系统创建 SPI 设备，并读写操作 W25Q128
    
2、使用环境

	/* 硬件环境：工程对应的开发硬件平台 */
	开发板：N32L43XM-STB N32L40XM-STB V1.1 N32G457QEL_EVB V1.1

3、使用说明
	
	/* 描述相关模块配置方法；例如:时钟，I/O等 */
	SystemClock：108MHz
	GPIO:  SPI1: NSS--PA4、SCK--PA5、MISO--PA6、MOSI--PA7
    串口： TX--PA9


	/* 描述Demo的测试步骤和现象 */
	1.编译后下载程序复位运行
	2.本例程创建两个线程，test0 线程和 test1 线程，test0 线程用于控制 D1 500ms闪烁，
      在 test1 线程中读写操作W25Q128，测试结果通过串口打印
    

4、注意事项
	将 N32L43XM-STB V1.1 开发板上的 SPI1 接口接在 N32G457QEL_EVB V1.1 开发板的 W25Q128 上，两个开发板需要共地



1. Function description
    This routine shows how to create an SPI device on the RT_Thread system and read, write W25Q128

2. Use environment
    Hardware environment: development hardware platform corresponding to the project 
    Development board:      N32L43XM-STB N32L40XM-STB V1.1

3. Instructions for use
    Describe the configuration method of related modules; for example: clock, I/O, etc. 
        1. SystemClock: 108MHz
        2. GPIO: SPI1: NSS--PA4、SCK--PA5、MISO--PA6、MOSI--PA7
        Log: TX--PA9 Baud rate: 115200

    Describe the test steps and phenomena of Demo 
        1. After compiling, download the program to reset and run;
        2. This routine creates two threads in main(), test0 thread and test1 thread, test0 thread is used to control D1 500ms flashing, test1 thread read, writeoperation W25Q128, test results printed through the serial port.

4. Attention
    Connect the SPI1 interface of the N32L43XM-STB V1.1 development board to the W25Q128 of the N32G457QEL_EVB V1.1 development board, the two development boards need to share the ground